///////////////////////////////////////////////////////////////////////////////
!----------------------------------------------------------------------!

Win-Test
--------

4.59.0-dev

  *** Report bugs to f6fvy at free.fr ***

- Bugfix : When turning the antenna with an Azimuth in the callsign
  field (Ctrl+F12), the network frame was sent twice in a row.

- PACC contest : M/2 processing (trailing indicator in the Cabrillo
  ouput file and Alt-Y action) added to PA stations. Tnx PC2A.

- EU DX contest : EU.DAT improved to automatically fill in the region
  when possible, based on DXCC entity, prefix, or call area.

- UBA Contests : Cabrillo file format updated to v3. Tnx DL7YS.

- Bugfix : Under some circumstances, NAQP LCR "Not In Log" errors were
  not displayed in the report. Tnx N6TV.

  *** Report bugs to olecam at f5mzn.org ***

4.58.0 (Jan 15, 2026)

- Bugfix : Tools / Check log / Download the LCR file... could crash
  Win-Test with certain specific URL.

- ICOM IC-7300MKII added. Tnx JR8VSE.

- Bugfix : DARC RTTY Short : Several bugs fixed. Tnx DL7YS. 

- EUDX contest multipliers list (EU.DAT) updated.

- Bugfix : When importing CQWW RTTY Cabrillo log, the second exchange
  of the entrant ("DX" or K/VE state/province) wasn't correctly set.

- Commonwealth Contest : Scoring updated. Update the RGGB_CMW exchanges
  DB (Tools / Data files / Exchanges database...) to prefill the HQ
  stations. Tnx G7TWC.
 
- OTRSP : New setting added to skip TX focus checking. This parameter
  is intended for use with interfaces that have a lazy OTRSP
  implementation. Tnx F6IFY.

- RSGB IOTA : Self-spotting is now permitted. Tnx F1AKK.

- Bugfix : When the contest configuration dialog was cancelled after
  correcting a log containing corrupted QSOs, Win-Test crashed.

4.57.0 (June 30, 2025)

- When spotting a station during a VHF+ contest, the grids are now
  sent. You can also adjust the propagation mode with the Up/Down
  arrow keys. Tnx F4CWN.

- Suspicious grid squares are now listed as exchange errors in log
  check tools.

- Summary : For VHF+ contests, the ODX on each band is now indicated
  when copying as text.

- Bugfix : UBA Spring and ON monobanders contests : The log was stuck
  on 20m. Tnx F5IN.

- ON 80m contest updated. It's now a dual band 80/40m contest.

- The grid squares checking datafile can now be updated in the
  Grid squares map properties dialog or with the Options / Datafiles
  menu.

  The latest files now include the largest inland lakes, which are
  considered exclusions from the entity in which they are located.

  As usual, if you find any errors in grids, please report them.

4.56.0 (May 17, 2025)

- Bugfix : In some dialog boxes, the Ctrl-Backspace keys added
  "square characters" instead of deleting the previous word.

- MRAI (Memorial DL6RAI) removed from the contest list. Tnx DL5RMH.

- Grid squares : For all contests using a grid square as an exchange,
  its validity is checked on the fly according to the callsign's DXCC
  entity. Two different colors are used to distinguish between syntax
  errors and incorrect positioning. If, despite the care and time
  taken in compiling the data file, you find any errors, please
  report them.

  Note: For the moment, inland lakes or certain estuaries are not taken
  into account and are considered part of the entity. However, land
  enclaves (e.g. 7P in ZS) normally are.
  
- IC-7760 added. Tnx F4HIN.

- Bugfix : SA-10 : The mult statistics in the Rate window were not
  displayed at all.

- Bugfix : SA-10 : The spots warning were indicating "New DXCC"
  instead of "New prefix".

- When "talk" commands are used to send or receive messages, a "-@"
  suffix is displayed in the Gab window.

- Extend the log errors file to _err.txt files when archiving.

- Help added to the MP3 configuration dialog to enable the MP3
  Fraunhofer codec.

- 122 GHz band (122G) added to the EU VHF+ contests. Tnx DL8AUU. 

- All Asian DX LCR parser added. Tnx N6TV and JARL.

- Bugfix : The tooltips are now displayed when the ONTOP option is
  enabled. Tnx K5GN, N6TV.

4.55.0 (Jan 16, 2025)

- PACC : Self spot allowed. Tnx PA2A.

- FOC Marathon : Rules updated. Tnx DL6KVA.

- Bugfix : When the callsign field was empty, and the previous QSO
  was from the same entity as yours, using Alt-F12 or Ctrl-F12 was
  turning the antenna to 0 deg / 180 deg while it was not supposed to.
  Tnx N6TV.

- Mixed mode contests : Elecraft K3 and K4 are now set to the correct
  mode if the "Pass to Sub-Vfo frequency" was used in the radio or
  the Alt-A windows. Tnx N6TV.  

- New items added to the RadioWnd contextual menus to turn the antenna
  when right-clicking on a spot. Tnx SM6VTZ.

- When corrupted QSO are found when loading the log, and you accept
  Win-Test to fix it, a textual error file is generated with data
  regarding the corrupted records so you can try to find information
  on these QSO. Tnx F1ULQ/9L5A.

- Spots coming from a skimmer with the same callsign as the log
  are now considered the same way as the op-entered. If you have one 
  (or more) local skimmer(s) with a different callsign, they can be
  added using the Options / DX-cluster / Additional local skimmers...
  dialog box.

  To make these spots stand out in the bandmap list, an option has
  been added to move them at the top of the list, while maintaining
  the selected sort order.

  To make things clearer and more consistent, the op-entered spots
  and the spots coming from a local skimmer are now all named
  "local spots".

- 9A DX contest : Self spotting allowed in SSB added. Tnx DC8YZ.

- Freq / Callsign order reversed for self-spots to be consistent with
  Alt-F3. Tnx DC8YZ.

- Russian 160m : Points credit updated. Tnx R2AA.

- ARRL 160, ARRL SS, ARRL FD : Alt-Z window slightly redesigned to add
  prefixes to the overseas territories.

- ARRL SS LCR parser improved. Tnx N6TV.

- Bugfix : When a partial frequency was entered that corresponded to
  a band, but was not used in the contest, the frequency was ignored.
  Ex : "432" on 10m during a CQWW DX. Tnx F4CWN.

- Solar data window : When the window is opened, a SH/WWV or SH/WCY
  request is automatically sent to ensure the latest data are
  available.

4.54.0 (Oct 14, 2024)

- DARC WAG : Rules updated (mults are now counted per mode when 
  entering in Mixed category). Tnx DL7YS.

- On VHF+ (2m and higher), it is no longer necessary to fill in the
  callsign to turn the antenna (Ctrl-F12) if the QTH locator field
  is filled and valid. Tnx F5NZY.

- RSGB IOTA : LCR parser implemented.

- Bugfix : When no log was loaded, the table of custom CW abbreviations
  was not correctly initialized.

- CVA DX HF implemented.

- WAE QTC : The option of sending leading zeros is taken into account
  for QTC serial numbers. Tnx N6TV.

- IARU HF : 0/1 indicator added in the Cabrillo output for RUN1/RUN2 
  when entering in Multi-2 category. Tnx VK2IA.

- 3D22 added to the callsigns exceptions list.

- LABRE DX implemented. 

4.53.0 (July 3, 2024)

- RSGB contests once again allow points and multis to be credited to
  Russian and Belorussian stations.

- %d (day - 2 digits), %A (weekday - long) and %a (weekday - abbrev)
  parameters added to the default filenames and subdirectories names
  formats to specify the day of the contest.
  Useful when the same contest occurs several times per month.

  See Options / Log / New contest files properties...

  Tnx DL7YS.

- Bugfix : 3.4 GHz band removed from the French VHF+ contest.
  Tnx F4CWN.

4.52.0 (May 19, 2024)

- Lua API version string is 1.11.0

- Bugfix : Under some circumstances, WCY data were assigned to
  WWV.

- Autoscale the A chart of the solar data to accommodate any value.

- Update the CQMM DX code to accept AN (Antarctica) as a continent.
  Tnx PY4WAS.

- The DXCC entity for rover stations (ex W1ABC/R) are now correctly
  resolved. Tnx F5HRY.

- IARU FD Region 1 : Cabrillo file format updated to v3. Tnx DL8MAS.

- King Of Spain : M/M category on DX-side : Serial numbers are global
  across bands. Tnx CT1DRB.

- NAC Microwave : Band multipliers updated. Tnx SM6VTZ.

- DARC Easter and DARC XMas : Rules updated (QSO and mults are now
  counted per mode).

- Self-Spotting capability added. Works only for contests that
  permit it, namely to date the ARRL contests, the Russian
  DX (SSB only), the CQMM, and the DXPed logs.

  Use Commands / Self-Spotting... (or the text command SELFSPOTTING)
  to enable or not this feature, set the time between each self-spot
  and the optional comment. These settings are saved per log.

  You can also enable or disable the sending of the self-spots on
  the fly with the text commands SELFSPOTON (or SSON) and
  SELFSPOTOFF (or SSOFF).

  A self-spot is sent whenener a CQ key (as defined in the Tools /
  Automatic CQ repeat dialog) is pressed, by respecting the rules
  and limitations above, even if this key is redirected to a Lua
  script. F1 is always considered as a CQ key by default.

- Lua : wtPacket:SendSelfSpot() sends a self-spot to the packet
  network.

  WARNING : This API follows the same rules and limitations as the
  built-in feature described above.

- Lua : wtContest:IsSelfSpotPermitted() function added. Return a
  boolean value (true or false) is the contest rules permit
  self-spots in the current mode of the active radio.

- Lua : wtPacket:Send(strText) function added. Send the strText
  string to the packet cluster.

- When using the CQ repeat mode, and if a Lua script is tied to the
  CQ key, the script is executed for every CQ.

- YOTA : Rules updated. Tnx HA3LN.

- NAQP : LCR parser added. Tnx N6TV.

4.51.0 (January 19, 2024)

- Bugfix: WT might crash in some situation when a configured COM port
  was no longer available. Tks DC8YZ, M0CFW, EW2AA, and DL5NEN.

- ARRL Round Up RTTY : Cabrillo file format updated to v3.

- OK/OM DX contest : The rules of the CW and SSB legs are (finally !)
  unified. Never despair. Tnx OK1IC.

- Bugfix : RSGB AFS : 1 point per QSO (not 10). Tnx PA2A.

- NRAU Baltic : XX Troms added to the LA mults. Tnx SM5AJV.

- RAC Canada day and Canada winter : The permanent headquarters
  station VE3RHQ now gives 20 points. Tnx VE5CPU and VE5SF.

- Stew Perry : LCR parser added. Tnx N6TR.

- Bugfix : LCR report : Using Ctrl-O, under some circumstances, may
  lead to a crash.

- Bugfix : Stew Perry : The freq column in the Alt-A wnd was too wide.

- DARC 10m : Rules updated (QSO and mults are now valid per mode).
  Tnx DM6EE and DL7YS.

- DARC 10m : Cabrillo file format updated to v3.

- FT-100 : Fixed freq decoding of the CAT stream. Tnx DL8RDL.

- Croatian DX Contest : New rules implemented.

4.50.0 (October 22, 2023)

- DARC XMas, DARC Easter and DARC RTTY Short contests Cabrillo output
  file format upgraded to v3.

- ARRL DX : LCR parser updated. Tnx N6TV.

- Bugfix : OTRSP : Excessive AUX commands were sent when any VFO
  frequency was modified. Tnx N6TV.

- YO DX contest : Bands restricted from 80 to 10m and Cabrillo output
  file format upgraded to v3. Tnx PA2A.

- Bugfix : WAE EU-side : Under some circumstances, received QTC
  date/time could be wrong. Tnx DL7AWO and DL7YS.

- External UDP messages : Better way to send these UDP frames, and
  make them compatible with the current version of FreqEZ.

- Bugfix : Contest recorder : When stopping the record or when the
  files were rotated, Win-Test could hang/crash randomly. Tnx DL1MGB.

- Bugfix : WAE Non-EU side : If an EU QSO was logged with exchange 000,
  and if it wasn't a mult, it wasn't displayed in the transmit QTC
  dialog and couldn't been sent.

- Bugfix : The DTR line wasn't correctly set when the DTR always ON was
  used. Tnx DL5MLO.

- Add a checkmark to the Intelligent QSL menu item if this feature is
  enabled

- SAC : The Q with Russian and Belarus stations count 0 point and don't
  count as multipliers. See https://www.sactest.net/blog/rules/ for
  details.

- Added support of the Serial-over-TCP/IP protocol (RFC2217). It is a
  Telnet protocol extension for controlling Serial Ports remotely.
  Hardware devices like the USR-TCP232-302 ethernet module are
  supported (please note that USR-TCP232-302 has a limited support
  of RFC2217, especially the serial speed which must be set on the
  device itself). Software Virtual COM emulators supporting RFC2217 can
  also be used remotely, see
  https://gist.github.com/ssz360/696a5397003562156f62a556d29d961f for
  some examples how to use com0com-rfc2217.
  Unfortunately, RFC2217 extension is not suitable for time-critical
  interfaces like WinKey.

4.49.0 (June 26, 2023)

- ARRL FD, ARRL SS and ARRL 160 : RAC sections updated. ARRLSEC.DAT
  updated as well. Tnx N6TV and KD4D.

- Bugfix : REF DDFM 50 MHz : All French dpts whose number is less than
  10 weren't correctly considered as dpt in the log.

- Bugfix : Interfaces dialog : The COM ports scrolling wasn't working
  when clicking in the Page Up/Down zones of the scroll bar. Tnx F5MZN.

4.48.0 (June 6, 2023)

- REF DDFM 50 MHz : Rules updated. Tnx F5LEN, F4CWN.

- Additional messages (Alt-C) : Checkbox added to close or not the
  dialog automatically.

- ARRL 10m : LCR parser updated.

4.47.0 (May 2, 2023)

- Lua API version string is 1.10.0

- Bugfix : DARC Easter : The worked mults wnd (Alt-M) didn't display
  the correct data. Tnx DL7YS.

- Bugfix : F10 window : Under some circumstances and for specific
  contests, it could crash the program. Tnx PA2A.

- Yuri Gagarin International DX Contest disabled because of the new
  rules where the same exchange can be counted differently (per band,
  or per band and mode) depending on its nature. The code can't cope
  with that.

- New text command : LOADMSGS to open the current op. directory and
  allow loading CW or RTTY messages.

- Lua : wtQso:SetSentSerial(nSerial) : If applicable, it sets the
  sent serial number of the current QSO.

- Self-spot allowed for the ARRL DX, ARRL Sweepstakes and Russian DX.
  Complain to the ARRL and SRR if you want to stop this madness.
  Tnx N6TV.

- Lua : wtGab:Send now accepts a third optional boolean parameter to
  *not* log the sent gab. New API syntax :

  wtGab:Send(strText[, strToStation [, bDontLog]])

  Tnx KD4D.

  Ex : wtGab:Send("Hello world!", "STN45", true)

  will send "Hello world!" as a gab to STN45, but won't log/display it
  in the sender Gab window.

- Lua : onBandChange event : If the radio is out of bands, the value
  of wtArg when onBandChange is called is set to "0/RadioId".
  Tnx TK5EP.

- Lua : New wtApp:Timeout(nDuration) added. Similar to wtApp:Sleep
  except Win-Test is not blocked while it is executed.

  nDuration expressed in ms.

- Lua : New wtApp:TimeoutBox(nDuration, [strText, [bAbortEnabled]])
  API added.

  Displays a modal dialog box with a timeout progress bar, an optional
  centered text and an (optionally enabled) abort button.

  The duration is expressed in milliseconds (min 100).

  Win-Test is not totally blocked while it is executed.

- File / Explore now only copies the path if the Shift key is held.

- Fix bug : The NA Sprint LCR parser failed under some circumstances.
  Tnx N6TV.

- All CQ Contests : Restrictions regarding Russia and Belarus are
  now lifted. Tnx PA2A.

- CQWW RTTY : LCR parser added. Tnx F5UII.

- Option added in the World Map display to the differentiate skimmers
  spots from the human spots.

- Bugfix : When hovering an hyperlink, the hand cursor was not always
  displayed.

- Bugfix : HA DX contest : It was not possible to edit the serial
  sent (for non-HA stns). Tnx DJ8EW, DL6RAI.

4.46.0 (Jan 17, 2023)

- Lua API version string is 1.9.0

- Lua : wtApp:TextCommand now accepts "*" as strStn to send to all
  stations of the network.

- Lua : New local variable wtFrom. Set to nil by default. Contains
  the name of the station that sent the text command thru network
  to run a local script. Can be useful when two (or more) stations
  exchange data with scripts.

- Lua : New onBandChange event when there is a band change. wtArg
  includes the band name and the radio as strings
  (ex : "10/0" for 10m on radio1).

  Reminder : The band name can have letters in it (2KM, 10G etc.)

  onBandChange.wts example :

  _, _, band, radio = string.find(wtArg, "(%d+[GKM]*)/(%d+)")
  wtApp:AlertBox("RadioID: " .. radio .. " Band: " .. band)

  Tnx TK5EP.

- Bugfix : ARRL RTTY Roundup : The Check Mult window (F10) was
  not filled properly. Tnx PA2A.

- WAG : LCR parser added.

- Cabrillo import : When the Cabrillo contest identifier is
  unknown, Win-Test now offers the possibility to choose the
  contest the log is referring to.

- Radio wnd / List view : When possible, set an inactive VFO
  indicator. Tnx DJ0ZY.

- Carrier / Tune timer : The remaining time is now displayed
  in the Stop button caption.

- Explore Current op. directory added to the File menu.

  Two (similar) Lua API added to get this path :
  - wtApp:GetCurrentOpPath()
  - wtOp:GetPath()

- Lua : New wtKeyer:Load(strFileName) API to load messages
  from a .smsgs file. If no path is specified, the current op.
  directory is used. Tnx F6IFY.

- The default directory to save or load CW/RTTY messages is now
  set to the current op. directory.

- The QTC transmit and receive dialogs are checked to be always
  visible even if their positions were saved with a different
  monitors configuration. Tnx F5UII.

- The WAE messages can now be saved and loaded.

- Partner Wnd : After a Q is entered and the window is cleaned,
  the remaining content stays in place to not mess up the $GRABn
  variables. Tnx FY5KE.

- Scripts manager : Refresh button added. Useful if you alter
  directly the scripts directory.

- Ctrl-X now prompts for a text command to be executed on the
  current QSO if it applies.

- The log caret / cursor can now be displayed as a solid block
  (Options / Log). Text commands : BLOCKCARET / NOBLOCKCARET or
  BLOCKCURSOR / NOBLOCKCURSOR. Tnx DL6RAI.

- When archiving, the full path of the generated zip file is copied
  to the clipboard.

- When using RUN vs S&P, Alt-F4 (return to the last RUN CQ freq)
  switches automatically to RUN. Tnx F5UII.

- WAE : Following the rules, if the received serial is set to 000,
  points are credited only if it is a new mult. Tnx F5UII.

- Text commands : "NOTES" added as a text command to open the notes
  file attached to the current log.

- Partner window : Partial callsigns or callsigns with wildcard
  character(s) '?' are now removed if they match the callsign
  entered in the log. Tnx FY5KE.

- Bugfix : When entering your own callsign in the log (to cancel a
  QSO), your own location was displayed on the spots map (if enabled).

- Checkmark added to the freq offsets menu item if they're enabled.

- The summary data broadcast is now allowed for single-ops,
  independently of the Master setting in the contest configuration
  dialog. Tnx K2RET.

- Bugfix : FT-891 : Code totally rewritten and it now works as
  expected. Tnx RX3APM for report, and DK5MR for testing.

4.45.0 (Oct 18, 2022)

- Flex 6000 series added. Fixes the RTTY filter selection bug with
  the Kenwood interface. Only one slice is displayed, unless the
  split is selected. Tnx DL6DH, DL8OH, DL6RAI.

- Outbound RadioInfo external UDP messages capability added in the
  interfaces settings dialog (network advanced settings), to make
  easier to use additional programs or devices. Already tested with
  the rf-kit.de RF2K-S SSPA. Tnx F5HRY.

- Freq offsets : New text commands to access the setup : OFFSETSETUP
  (or OFFSETSSETUP). New text commands to enable/disable the
  freq offsets : OFFSET/NOOFFSET, OFFSETS/NOOFFSETS,
  OFFSETON/OFFSETOFF, OFFSETSON/OFFSETSOFF. Tnx F5UII.

- OCDX : /M, /MM and /P do not count as prefix multipliers.

- New setting dialog (Commands / Carrier timer...) to enable or not
  the carrier/tune (Ctrl-T) timer and set its duration. Tnx F5HRY.

- Bugfix : IARU FD R1 : /MM stations do not count as mult. Tnx DL6RAI.

- Bugfix : WAEDC : When the Alt-M window was copied, the numerical
  call areas of the countries that apply weren't used. Tnx DL6RAI.

- The /LH callsign extension (LightHouse) doesn't interfere anymore
  in the DXCC entity resolution. Tnx F5UII.

- DXPed HF : Distance added to the geographical data of the F10 wnd.
  Tnx F5UII.

- Yaesu Band data code for 60m added on the LPT output. As the default
  code (identical to 40m) can interfere with other bands, the user can
  choose to use the 50 MHz (6m) band code or an usused code. Tnx FY5FY.

- Bugfix : OK1WC Challenge : When the callsign length was over 8 chars,
  the mult extraction (last char of the suffix) wasn't working
  correctly. Tnx DJ0ZY/DD5M.

- Text and CSV export : The format YYMMDD is added to the fields list.
  Tnx F6AJA.

- IOTA contest : Cabrillo updated to v3.

- Bugfix : IOTA contest : In Multi-1 category, the QSO numbering was
  wrong. Tnx DL6RAI and others.

- IOTA contest : Rules 2022 : The Q with Russian and Belarus stations
  count 0 point and don't count as multipliers. See
  https://www.rsgbcc.org/hf/rules/2022/riota.shtml (RSGB IOTA Contest
  website) for details.

4.44.0 (July 20, 2022)

- When applying exchange(s) to entered QSOs (Ctrl-F10), the numbers
  of found QSO and updated QSO are notified.

- Bugfix : REG1TEST files : The QSO points and the claimed score were
  always set to 0 by default. Tnx F1EZG @ TM5R.

4.43.0 (July 1st, 2022)

- All Asian DX : Cabrillo updated to v3.

- Generic VHF+ contests have been extended to accommodate contests
  where a fixed exchange is sent instead of a serial number. Just enter
  this exchange in the "Exchange" field of the contest configuration
  dialog. If this entry field remains empty, the usual serial numbers
  are used. Tnx DL6RAI, DJ0ZY.

- All VHF+ generic contests are no more limited to 6-char grids
  (locators) and now accept 4-char grids (locators) exchanges as well.

- New option in the Cabrillo options dialog and the REG1TEST options
  dialog to set the claimed score to 0 point. Useful if you are using
  a contest template that is not fully adapted to the scoring method,
  and you don't want to mess up the claimed scores (if any).

- Bugfix : The CW default messages for the REF DDFM 50 MHz were wrong.

- The names of two microwaves bands over 76 GHz were wrong. They are
  now correctly labelled 122G and 134G, instead of 119G and 142G.
  Tnx F4CWN.

- New band data code available on the LPT output, designed for VHF+
  bands, from 50 MHz to 122 GHz. Tnx F4CWN.

- Bugfix : The title of the LPT port properties dialog was incorrect.

- Bugfix : When using markers in the bandmap and if the marker text
  was totally visible, the first line of the tooltip was empty.
  Tnx F6BGC.

- Band plans : New option to reject (automatic) spots outside the
  defined segments for a given mode, acting as filters. Tnx DL3DXX.

  Reminder : By default, the band plans are used to determine the
  mode of the (non-automatic) spots. They don't act as freq filters.

- Merge Logs : When sorting logs and if the timestamps of two (or more)
  QSO are identical (can happen if logs were imported from Cabrillo
  files), Win-Test now relies on the serial sent (if any) to
  order these QSO. Tnx N6TV.

- Yaesu FTDX-10 added. Tnx DL4LAM.

4.42.0 (May 20, 2022)

- When creating your Cabrillo log, you can now also submit it in
  one click to the Super Check Partial Database. Tks K6TU.

  This feature requires wtScpSubmit.dll which is included in the latest
  Win-Test installers. If needed, this dll is also available at
  http://download.win-test.com/utils/wtScpSubmit.dll
  It must be placed in the Win-Test installation directory.

  Under some circumstances (especially with oldest OS), you may need
  MSVCP140.dll and/or others to be installed on your system.
  The easiest way is to install the latest Microsoft Visual C++
  Redistributable packages for Visual Studio X86 available here:
  https://aka.ms/vs/17/release/vc_redist.x86.exe

  Finally, on Win7, to ensure TLS 1.1 and 1.2 are enabled, apply
  this easy fix https://is.gd/QlQgbg

- CQ-M : 10-minute rule for MOST (M/S) entries removed (rules 2022).

- Add LCR parsers to the CQ-M, RAEM, and Yuri Gagarin DX contests.

- Add the Out Of Band sections to the CQ WW and CQ WPX LCR parsers.
  Tnx F6KOP.

- OK/OM : Rules 2022 : The Q with Russian and Belarus stations count
  0 point and don't count as multipliers. See http://www.okomdx.crk.cz/
  (OK-OM DX contest website) for details.

- Interfaces Setup dialog : The keying compensation can now be
  negative (in the case where the TRX extends the keying). Tnx N6TV.

- Bugfix : The display options of the zones window(s) (Alt+Z) were
  not always correctly retained between sessions. Tnx F5LIW.

- CQWPX : Rules 2022 : The Q with Russian and Belarus stations count
  0 point and don't count as multipliers. See https://is.gd/HIMOLP
  (CQWPX blog) for details.

- Lua : It's now possible to attach Lua scripts to text commands that
  are identical to mode names ("SSB", "CW", "RTTY", etc.). In these
  cases, the script will be called *after* the command is processed
  normally by Win-Test. Tnx TK5EP.

- The DX spots window (Alt+A) display options are now interactive.

- Bugfix : Notes report dlg : After editing a note, the log caret
  wasn't restored.

- World Map : Options : The colors of the paths can now be the same
  as the markers.

4.41.0 (Feb 15, 2022)

- Lua API version string is 1.8.0

- Op-entered spots are now protected from spots of the same DX on
  a freq inside the mode bandwidth window. Tnx DL6RAI.

- NA Sprint : LCR parser updated. Tnx N6TV.

- New countdown timer added (Tools menu or TIMER text command),
  especially for the single-ops. It indicates exactly when they can
  operate again after a pause. It's based on the time of the last
  QSO entered in the log, truncated to the minute.

  You can also use the text command TIMER/nnHmmM or TIMER/nnHmm
  (meaning nn hours and mm minutes), or TIMER/xxH (nn hours) or
  TIMER/nnM (nn minutes) to set and start the timer automatically.

  Tnx F5NZY.

- Shortcuts added to some of the reports buttons.

- QSO times are now by default considered as truncated to the minute
  for Time ON / Time OFF calculations and the QSY rules. Tnx F5NKX.

- Contest Recorder : AltGr+O, and text commands RECORD/NORECORD (and
  STARTRECORD/STOPRECORD) added to Start/Stop recording.

- REG1TEST / EDI : Under some circumstances, the ouput file wasn't
  created. Tnx OZ1ZAA.

- UBA DX : Updated to comply with the rules 2022. Tnx F5LIW.

- World Map : "Copy content as image" menu item added.

- RTTY windows : Esc button added. Tnx PA2A.

- Notes report dialog. It's now possible to edit a note by selecting
  it and use Alt-N to modify the comment. Tnx F4CWN.

- REF HF : For M/S entrants, the compliance of the 10-min rule can be
  checked by using the appropriate item in the Tools / Check log menu.

- REF HF : Timer added in the Alt-J wnd for the M/S entrants.

- Lua : New wtRadio* API :
  wtRadio*:GetBand(), wtRadio*:GetMode() and wtRadio*:GetCqData()
  added.

  GetBand() and GetMode() return the current band and mode of the
  radio. GetCqData() return a Lua table with various data on the last
  sent CQ (that are stored for Alt-F4) : "freq", "qsx", "band", "mode"
  and "wpm" (for CW).

- Bugfix : $MSG10 was actually sending the additional MSG1 instead of
  MSG10. A 20-year old typo in the code ! Tnx SP5KP.

- World Map : New options to display short and longs paths for
  "my spotters" and the NCDXF beacons.

- New "NCDXF" text command to set the active radio on the NCDXF beacons
  frequency (if it applies).

- New option in the world map display option to show the NCDXF beacon
  that currently transmits if the radio is on the NCDXF frequency
  (+/- 100 Hz).

- The world map display options are now interactive.
  Different styles and a night opacity slider are also added.

- The "copy as image" feature now also copies the image in PNG format,
  to extend the paste scope (mail, twitter etc.).

- The RBN nodes and frequent spotters databases can be directly updated
  with the contextual menu of the map wnd (Display options).

4.40.0 (Jan 18, 2022)

- New option in the world map window to mark locations from where you
  are spotted.

  Note: The diameter of the marker is supposed to represent the signal
  strength. However, disparities between reception conditions,
  equipment used, and/or the accuracy of the s-meters can lead to
  outliers. It is therefore must be considered only as a relative
  indication.

- Bugfix : The RUN, MULT, RUN1, RUN2 text commands and their shortcuts
  Alt-Y and Ctrl-F3 (toggle) were not disabled in the Single-Op
  categories. Tnx F5NZY.

- Interface dialog : The usable COM ports are now extended up to COM32.
  The parameters list now also displays the Handshake (HS), Always ON
  (ON) and Always OFF (OFF) settings, and are ordered by Pin (DTR then
  RTS). Tnx DL5XJ, DL6RAI.

- New NCDXF/IBP Beacons window : Displays the transmission schedule
  of the NCDXF / IBP (International Beacons Project) beacons. A double
  click on a line gets the radio on the beacon freq. An "i" (stands for
  "info") in the status column indicates a comment you can read by
  hovering the mouse over it. Tnx VE3SUN.

- LCR : Croatian CW contest LCR parser added.

- LCR : Parser for CQ WW LCR updated. Works for preview and final
  reports.

- New feature : You can now grab a spot from the visible spots in the
  Radio windows or in the DX-cluster window by entering the callsign
  (or some letters of it) and Ctrl-Space.

- Bugfix : Automatic op-entered spots during QSOs (especially in S&P)
  were not replaced by DX-cluster / external spots.

- Bufix : When sending a gab composed of CAPITAL letters, do not
  shake our own gab window.

- REF HF and REF 160m : LCR process updated. Tnx F4CWN.

- French (and some Belgian) users : Button added in the keys
  redefinitions dialog to load AZERTY redefinitions that allow the
  AZERTY keyboards users to access the numbers located on the top row
  without using the Shift or Shift Lock keys. They allow direct access
  to the ?, . and / keys of the bottom row as well. This button is
  displayed only when the language is set to French.

4.39.0 (Dec 6, 2021)

- DX cluster (Alt-A) and Radio windows : The CT1BOH spot quality tags
  can now be displayed if they're sent by the skimmer. You can also
  filter the displayed spots by tag when applicable.

  Unless it's disabled by the user, in the list tab of the Radio
  window, the displayed spots are grouped by quality before being
  sorted. Tnx ES5TV.

- Script Manager : Hyperlink to the Lua API reference web page added.

- Op-entered spots are kept until worked or deleted on purpose, even
  if other stations are externally spotted on their frequencies.
  Tnx DL6RAI.

- Radio wnd : List tab : When spots are sorted by points or mult type,
  the second sorting criteria is now the beam heading rather than
  the spot frequency. Tnx DL6RAI.

- Gab : To draw attention, any gab text containing only CAPITAL
  letters now shakes the recipients gab window.

- SCP files : Defensive coding to attempt to prevent at best against
  crashes under some circumstances with badly-formatted or corrupted
  SCP or MASTER files. Tnx SP5KP.

- Bugfix : For several contests, the columns headers were overlapping.
  Tnx F5HRY.

- Bugfix : WinKey : When using +/- in messages, the speed was randomly
  not reset to its initial value and the next message was sent with
  an incorrect greater speed. Tnx NN7CW and DL6RAI for their detailed
  reports and numerous tests to fix this long-standing bug.

- RDA Contest : LCR view added.

- OK/OM CW : 10 mins timer enabled for M/S category. RUN stations only.

- Bugfix : OK/OM CW DX-side : The district information display in the
  Mult window (F10) was broken.

- Larger log font sizes available for short-sighted ;-)
  Tnx TA2SE, W1NN.

- DX Spots window (Alt-A) : New option to pin the op-entered spots to
  the bottom of the window so you can always see them. Tnx DL6RAI.

- WAG : The output Cabrillo file is now following the v3 specs.
  Tnx DL1RTL.

- EU-DX : Multipliers list updated. Tnx IK6QON.

- Bugfix : When Win-Test was started from the command line with an
  alternate application data directory (-a switch), the directory
  name wasn't unquoted. Tnx F1HAR.

4.38.1 (Nov 1st, 2021)

- Bugfix : After importing a Cabrillo file, the resulting wt4 file
  couldn't be opened by Win-Test 4.38.0. Tnx F5LIW.

4.38.0 (Oct 25, 2021)

- Lua API version string is 1.7.0

- Defensive coding to check the log file when opening to prevent file
  corruptions. Tnx DL1DAW.

- Workaround for the USBSER.SYS bug that doesn't update the RTS line
  until DTR is accessed. Tnx R2AXZ (author of the Blue Pill Serial
  Monster).

- RDA Contest : Cabrillo updated to v3.

- WAE Transmit and Receive windows : New messages available.

- WAE : New CW variable $RAWTIME to send the QTC time with cut numbers
  disabled.

- WAE : Transmit QTC window : A QTC line can now be directly sent by
  using the coresponding  numeric key (0 sends the line labelled 10).

- Lua : New wtContest API :
  wtContest:GetCategoryId(), wtContest:GetModeCategoryId(),
  wtContest:GetPowerClassId() and wtContest:GetOverlayId() added.

- Lua : For standardization purposes, the microHam and OTRSP events
  scripts are now renamed :

  microhamFsOn -> onMicrohamFsOn
  microhamFsOff -> onMicrohamFsOff
  otrspCrOn -> onOtrspCrOn
  otrspCrOff -> onOtrspCrOff
  otrspCrEvent -> onOtrspCrEvent

  For now, to maintain compatibility, the script legacy names are
  still executed.

- Lua : New scripts called on log opening (onFileOpen) and on log
  closing (onFileClose).

- EU HF : The Cabrillo header is updated (EUHFC instead of EU-HF).
  Tnx DL6RAI.

- CQWW DX : The Youth overlay is added to the Overlay drop-down list.

- CQWW DX : The Explorer category is added to the Category drop-down
  list (Single-Op Explorer and Multi-Op Explorer).

- Bugfix : LCR parser fixed for the CQ WPX reports.

- In the contest settings dlg, you can now set the default power class
  to use when creating new logs. Tnx DL6RAI.

- Bugfix : CW : The spaced digits option was not read when starting
  Win-Test. Despite the ckecked option in the menu item, it was not
  enabled.

- New archiving feature : File / Archive... (or ARCHIVE text command).
  It creates a timestamped zipped file in the log directory of the
  files related to the current log that are selected.

  Warning : Archiving audio recordings file that are usually pretty
  large can take a while... Be patient.

- For standardization purposes, all timestamped files are now
  timestamped to the nearest second.

- Time Shifting : The selection of the QSO and the stations are now
  independent. And a backup of the log is automatically performed
  before proceeding. Tnx EA7X/EF4HQ.

- Bugfix : CQWW VHF : When using the default CW messages, the sent grid
  was 6-char instead of 4-char. Tnx F5HRY.

- Bugfix : IARU HF : There are cases where different DXCC entities have
  the same Society (ex OH and OH0) and were counted as different mults.

- Bugfix : The "Dupes included or not in QSO counts and avg
  calculations" string in the summary text was always in local language
  even if summary in English was selected.

- Marconi Memorial HF : Points per QSO updated.

4.37.0 (June 29, 2021)

- WAE : Rules 2021 : BY is added to the call area multipliers (so
  Chinese stations with different digits in their prefix count as
  different mults). Tnx DL7YS.

- Bugfix : VHF+ contests : Sorting the Spots list by QSO points
 (related to distance if it can be computed) wasn't working.

- ARRL FD : The "Covid" rule (Home stations can work home stations)
  is extended to 2021. Tnx VE2FWW.

- KCJ and KCJ Top Band contests rules updated. Tnx JI1RXQ.

- VHF+ contests : Discrepancies between gridsquares in the log for
  different bands weren't displayed in the Bad Exchanges check report.
  Tnx F4CWN.

- ARRL 10m : LCR viewer updated to fit to the new LCR format.

- The question mark character is now enabled in all QSO input fields,
  and the cursor is positioned on it when cycling the fields. Tnx N6TV.

- CW : New option for spaced digits in serials : When enabled, a
  half-space (^) is inserted between each digits of the serial, making
  it more readable at high speed.

- Bugfix : When copying the Summary wnd as text, the "Generated by
  Win-Test" line was missing. Tnx DL6RAI.

- F10 Wnd : In DXPed HF or VHF, the date of the QSO is now displayed.

- Summary wnd : When using a language different from English, some
  column titles were incorrectly truncated.

4.36.0 (May 19, 2021)

- CQ-M : Scoring is now updated and follows the rules 2021.

- IARU HF : In M/S (Mixed only) category, the 10-min status timer now
  takes into account mode changes. Tnx HA6OI.

- HA DX : The Cabrillo output file now includes the RUN/MULT indicator
  for the M/S entrants. Tnx HA6OI.

- YOTA (Youngsters On The Air) contest implemented.

- ARI DX / ARI 40-80 : Provinces list and exchange equivalence file
  (ARIPROV.DAT) updated. Tnx HB9AMO, DL6RAI.

- Bugfix : In Phone, when entering a (very) long exchange, the cursor
  might insert a ghost space character at the end of the field.

- City, State/Prov, Postal Code and Country separate fields added to
  the contest settings dialog to improve the compatibility with
  the Cabrillo v3 header fields. These fields are assembled together to
  maintain the back compatibility with the Cabrillo v2 format if needed.
  If is highly recommended to edit your saved profiles (if any) by
  loading, editing and saving them one by one in the dialog.

- CQMM DX implemented.

- All file dialogs are now resizable.

- YUDX : LCR view added.

- LCR viewer : Column order unified.

- Bugfix : VHF+ contests : Under some circumstances, when the
  automatic exchange (grid) guessing was set, the Check Partial wnd
  wasn't updated anymore after the field was automatically filled.

- OK/OM Contest SSB : This contest was not listed when the contests
  of the month checkbox (in April) was selected. Tnx F1HAR.

- OK/OM contest : You can now directly download your LCR in Win-Test
  from the "rejected" link in the final results and preliminary
  results page.

4.35.0 (April 8, 2021)

- King Of Spain : The 10 min rule for the multi-op entrants is now
  removed.

- Bugfix : OK/OM Contest SSB : When entering as non OK/OM, the
  points credit was wrong when working an OK/OM stn. Tnx F1HAR.

- Radio Wnd : Ctrl+R shortcut added to allow cycle the view tabs
  without using your mouse.

- Option added in the dialog to replace op in batch, to match any
  operator already entered.

- LZ DX contest : LCR view added.

- SPDX : The limitation on the number of band/mode changes during a
  clock hour in all categories is now removed.

- Fix bug : When parsing the DX cluster stream, lines were discarded
  if the callsign of the spotter was longer than 9 characters
  (ex : 3V/KF5EYY-#, IK4VET-1-# or JR1BFZ/2-#) and the freq higher
  than 9999.9 MHz. Tnx DL6RAI.

- RTTY windows : It's now possible to log the data stream to files
  created with the .ry1 and .ry2 extensions. Tnx DL6RAI.

- Bugfix : RSGB Commonwealth Contest : The off-time value wasn't
  specified for this contest (60 mins) and the default value (15 mins)
  was used instead. Tnx M0UNN.

- The default off-time when not specified in the rules is now set
  to 30 minutes instead of 15.

- WAEDC : LCR review added. Tnx DL7YS, DL6RAI.

- DX Cluster Announces (Alt+A) : Exchanges can now be displayed (if it
  applies). Tnx F4CWN.

- Bugfix : Tools / Automatic CQ Repeat : The delay between CQ was
  not saved between sessions. Tnx F4CWN.

- Bugfix : Tools / Search for possible bad exchanges : If there was
  no log discrepancies and a check against the database was
  requested, it was not displayed. Tnx F4CWN.

- DX Cluster announces (Alt+A) : New dialog to facilitate the choice
  of bands to be displayed, replacing the sub-menus. Tnx F5HRY.

- Alt+F4 / Alt+F5 : When running in CW, the current CW speed is saved
  when CQ'ing (or using Alt+F5), and is restored when QSYing back to
  the saved run frequency.

- UI : All textual child windows that can be resized with the mouse
  (Check Partials (F12), N + 1 (F8), Skeds (Alt+B), Gab (Alt+I),
  Stats (Ctrl+F9), Radios, RTTY, DX Cluster monitor (Alt+O) and
  announces (Alt+A))  are now resized according to the size
  of the font used. To remove this constraint and resize freely,
  keep the Shift key down while resizing.

- Cabrillo output : The @ character is now allowed in the operators
  list. Tnx N6TV.

- ARRL DX : Band changes restrictions set to 10 for the M/S category,
  according to the new rules. Tnx N1PSE.

- Check Partial (F12) : In some cases, when multiple wildcard
  characters ('?') were used, no search was performed. It's no longer
  the case as soon as there are at least 2 characters that are not
  wildcards in the pattern to search. Tnx F4CWN.

- PACC : Cabrillo v3 output implemented.

- Summary wnd : For the Instagrammers and such, your callsign is now
  added to the window title. Tnx F6BGC.

- Multi-Distributed category introduced.

- Bugfix : Lua : wtQso:IsModeCw() was always returning false.

- More restrictive checks applied to the exchanges database to dump
  malformed callsigns or exchanges.

- New Exchanges Database information dialog : Options / Data files /
  Exchanges database... Text commands : EXCHDB, EXCHDATABASE,
  EXCHFILE or EXCHFILES. Tnx N6TV, DL5YM.

- LCR : Add instructions if Win-Test can't directly download and/or
  process LCR for some contests.

- RDXC : MOST indicators (0 and 1 for RUN and MULT) added to the
  Cabrillo output file. The 6-char grid square is now also required
  for all entrants. Tnx UA9QCQ.

- The callsign exceptions (callsigns that don't follow the usual
  rules, like RAEM, 5VDE, 7QAA, etc.) are no more hardcoded and are
  now grouped in the exceptions.dat file (in the /extras directory)
  for easy updating.

- CQWW 160m : Cabrillo v3 output implemented. Tnx N6TV.

- ADIF output : QSO with my own callsign are always discarded.
  Tnx N6TV.

4.34.1 (Feb. 5, 2021)

- EU-DX Contest : The 10m band was missing in the summary. Tnx F1DUZ.

- EU-DX Contest : CW and SSB columns added for the Mixed category.

- Italian translation DLL updated.

4.34.0 (Jan. 25, 2021)

- Lua API version string is 1.6.0

- Bugfix : CQWW 160m : The exchange database file ARRL-USVE.DTB wasn't
  loaded. Tnx DL4MM.

- Bugfix : UK/EI : If the district field was manually filled before
  the serial number, that field was emptied when the cursor got back
  to the callsign. Tnx PA2A.

- QQSLON / QQSLOFF or QQSL / NOQQSL text commands to enable (or
  disable) the Quick QSL feature. QUICKQSL still opens the Quick
  QSL settings dialog. Tnx F6IFY.

- EU-DX Contest added. Requires EU.DAT countries file. Tnx IK6QON.

- Lua : wtRadio*:SetFreq(fFreq) and wtRadio*:SetFreq(fFreq, nVfo) now
  ignore the freq if it's outside of any band, and return with no
  error message. Tnx F6IFY.

- Lua : wtQso:IsModeDigital() and wtQso:IsModeCw() added.

- Lua : nQsoNum (optional) added as argument to
  wtQso:GetData([nQsoNum]) function.

- LCR : IARU HF LCR processing rules updated.

- 5VDE added as an exception callsign.

- LCR : If Win-Test supports LCR review and the contest has been
  entered in a multi-op category, an Operator column is added
  in the review dialog. Tnx F5HRY.

- OK/OM contest : LCR processing added. Requires to save the "rejected
  QSO" page as an html file and to load it in Win-Test. Tnx F8BXI.

- CQWW DX : LCR processing rules updated to fit the new CQWW LCR
  format.

- ARRL Contests : The ARRL has finally unified the US States and
  VE provinces and territories lists, and the Prince Edward Island
  abbreviation is now PE for the ARRL DX, ARRL 10 and ARRL roundup
  RTTY contests.

- NAQP : The Prince Edward Island abbreviation is now PE. Tnx N6TV
  and AC0W.

- NA Sprints : The Prince Edward Island abbreviation is now PE.

- NRAU contest : New abbreviations for some Fylke / Lan / Province /
  Region updated. Tnx ES7GM.

- RAEM Contest : The polar circle location (giving extra bonus points)
  was slightly wrong.

- Script manager : The minus key located in the numpad is now
  considered different from the key located in the character keys.
  To be consistent, the same rule applies when redefining keys.
  Tnx F5HRY.

- Bugfix : The IC-9100 couldn't work... Because of a stupid typo !
  Tnx DL2AKT and N6TV.

- Bugfix : WAE RTTY : When the log was reopened, the next sent QTC
  group number was wrong. Tnx DL6RAI, DJ9MH and DJ4MZ.

- JIDX : 160m added to the SSB leg. Tnx N6TV and N6KI.

- Icom IC-705 added. Tnx OH1MA.

- "Ethernet network" reworded as "Local Network" to prevent confusion.
  Tnx FY5FY.

4.33.0 (Oct 14, 2020)

- Bugfix : AGCW-DTC : 2 points Club stations list updated. Tnx DL6RAI.

- Bugfix : WAG : The Exchanges file (WAG_DL.DTB) wasn't correctly
  loaded for DL entrants. Tnx DL4NAC and DL6RAI.

- ARRL SS, ARRL 160, ARRL FD : PE (Prince Edward Island) section
  added. Tnx W1NN.

- MicroHAM MKIII interface added. Tnx G0HSA, OM7ZZ.

- When a file error occurs when saving DX-cluster data, the user can
  now Cancel to abort further writing attempts. Tnx DL5MLO.

- Bugfix : All Asian DX contest : Cabrillo CONTEST: line text fixed.
  Tnx VA2EW.

- Exchanges Databases (.DTB files) : Defensive coding to attempt to
  prevent at best against crashes under some circumstances with
  badly-formatted or corrupted databases files. Tnx OK1DSZ @ OK4C.

4.32.0 (Sept 1st, 2020)

- YO DX HF  : Contest rules updated (160m added + points for /MM
  stations).

- callsign.pat updated. Tnx DL6RAI.

- RDAC : RDA.DAT (district list) updated.

- WAE DX side : QTC line numbers displayed for easy retrieval in case
  of repeat request.

- Bugfix : The audio record button is now disabled when recorded audio
  is playing.

- Bugfix : IOTA Mixed : Summary columns weren't consistent with the
  rest of them, and created a bug when used with Unipost
  (cqcontest.net). Tnx DL6RAI.

- All reports dialogs can now be vertically resized to display more
  or less list rows. The window placements are also globally saved.

- Bugfix : When the same callsign was spotted on both sides of a
  sub-band limit (so, it was considered spotted in both modes),
  Ctrl-Up/Down kept grabbing these two callsigns alternately.
  Tnx F5UTN @ TM0HQ.

- ARI Sezioni : Rules and mult list updated. Tnx IV3IYH.

  Mult List : http://download.win-test.com/databases/ARISEC.DAT

- Bugfix : EU HF Championship : The content of the EU_HF.DTB database
  was ignored. Tnx EW2AA.

- File / Update Exch Database : A confirmation dialog is now displayed
  and a backup of the current DTB file is done, before proceeding.

- New Check Partial search processing for VHF+ logs :

  In VHF+ contests logs, you can now enter a partial callsign (in the
  callsign field) and/or a partial locator / grid (in the grid square
  field) to refine searches in the Check Partial wnd (F12).

  The minimum number of chars to start the search for the callsign
  field is set by the contextual menu (3 by default), and set to
  2 characters for the locator.

  Finally, in both fields you can also use wildcards characters '?'
  to represent a character. Ex: "JN?8EQ" will search for all
  callsigns with locator JN08EQ, JN18EQ, JN28EQ, ... JN98EQ.

  Inspired by DL2NBU DOS software. Tnx DL6RAI.

- Bugfix : MMC HF wasn't showing up in the contests of the month in
  July. Tnx DL6RAI.

- LCR review added for ARRL 160, NA Sprint, ARRL Sweepstakes.
  Tnx N6TV.

- Elecraft K4 added. Tnx N6TV.

4.31.0 (June 28, 2020)

- Lua API version string is 1.5.0

- Lua : wtApp:PostMessage, wtApp:SendMessage and wtApp:GetLastError
  added. Tnx F6BEE for inspiration.

  See description and syntax in
  http://download.win-test.com/v4/lua/LuaApiDoc.txt

- ARRL FD : Covid-19 rule exception : Class D stations may work all
  other Field Day stations, including other Class D stations,
  for points. Tnx K6ZB.

- Log Checking Report (LCR) review added in the Tools / Check log
  menu.

  For now, only the following LCR are processed :

  - CQWW DX
  - CQWW WPX
  - ARRL DX
  - ARRL 10m
  - IARU HF
  - EU HF
  - SAC
  - KOS
  - REF HF
  - VHF+ contests if adjudicated with LX

  Mainly, because these LCR are public, or because I had one ;-)

  Any textual (or html) LCR can theorically be implemented,
  as long as I have access to a sample.

  For various reasons, sometimes the "Download LCR" may not work.
  In that case, try to download the LCR with your browser
  and save it in a convenient location (the log directory
  is the best choice). You can "attach" it to your log
  by using the "Save" button in the report dialog.

- Dx-Cluster window (Alt-T) : Number of Macros increased to 8.
  Tnx PA2A.

- Dx-Cluster macro editor : Window enlarged, and the edit field now
  wraps to improve readibility. Tnx PA2A.

- The merge dialog now displays "compact paths".

- NRAU Baltic mults list updated. Tnx LB3RE.

- Review of the exchanges databases files to prevent mixing different
  exchanges between contests. Also, if a contest uses only a part of
  a database file, the rest is kept untouched if the database is
  updated with Win-Test.

- Depending on the contest and, if it applies, whose side you're
  on (DX side or domestic), the callsigns from the master file (namely
  MASTER.SCP/DTA or HF.DTB/SCP) are filtered to display only relevant
  results in the Check Partial and N+1 windows.

- The master file in use can now be directly updated from the
  Internet (like the CTY files) by using the Options / Data files
  / Master file menu, or by using the "Used File list" item in
  the contextual menu of the Check Partial or N+1 windows.

  Note : The recommended default master file to use is MASTER.SCP,
  maintained by Stu K6TU (http://http://supercheckpartial.com/).

  Reminder : You can also use contest-specific master files
  (recommended only for minor national or regional contests)
  named after the list located at
  http://download.win-test.com/files/checkPartial/%23_READ_ME_%23.TXT

  These files do not replace the default master file, but complement
  it at runtime.

- In the contest settings dialog, contests no longer taking place
  have been removed from the list.

- New REBOOT (or RESTARTPC) text command added. It closes the current
  log and restarts the host PC. Tnx F8CRH, F6BEE.

- When the exchanges database is updated, a notification message
  is displayed at the bottom of log. Tnx DL6RAI.

4.30.0 (Jan 16, 2020)

- Bugfix : If the backup volume was unmounted, disabling the next
  backups was failing. Tnx F6HJO. (Task #388)

- HA DX contest rules updated. Tnx HA6OI, HA1AG, F5LIW and others.

- UFT contest rules updated. Tnx F6CEL.

- Bugfix : Under some specific circumstances, the Single-Op Assisted
  category wasn't taken into account when importing such a Cabrillo
  file. Tnx TO1A.

- Bugfix : With multi monitors systems and under some specific
  circumstances, choosing colors with mouse was impossible. Tnx KL0R.

- Bugfix : The headers row was always included in the CSV output file,
  whatever the setting was. Tnx F5LIW.

- Yaesu FTDX101 added. Tnx RA1ANY, RA3AUU.

- Icom IC-9700 added. Tnx F1ULQ.

- WAEDC : Cabrillo output file upgraded to v3 specs.

- Bugfix : The LCD display of the contest recorder wnd wasn't always
  properly updated when using a language different from English.

- WAEDC DX side : Send QTC dialog (Ctrl-L) now displays the maximum
  available QTC to send (if any). You can modify the number of QTC
  to send, or only display the already sent QTC, with F9 (or the
  "QTC / Show sent" button). F8 allows to modify the recipient
  callsign.

- QSO and distinct callsigns counts added in the distinct callsigns
  report when sorted by country.

- "Copy" button added to the log check dialogs, allowing to easily
  paste reports in a spreadsheet.

4.29.0 (July 5, 2019)

- YU DX Contest rules updated. Tnx F5IN.

- Bugfix : When a exception callsign and a prefix were identical in
  the CTY file, and under some specific circumstances, the DXCC lookup
  function could fail. Tnx F5LIW.

- Spot Warnings : When you're spotted, the spot comment, if any, is now
  displayed.

- RSGB HF contests : District Code for Norwich has been changed
  from "NR" to "NK". Tnx F1ICS.

- Bugfix : FOC Marathon : Stats are now displayed on 3 days.
  Tnx F5NZY.

- Bugfix : RSGB AFS : Dupe count on 40m was wrong. Tnx G0HSA.

- Bugfix : REF 160m : The total and final score lines weren't displayed
  in the summary window.

- ADIF export : Output fields reordered and STATION_CALLSIGN field
  added. Tnx YT9TP.

- Bugfix : RTTY : Messages with embedded scripts were hanging Win-Test.
  Tnx N6TV.

- IARU HF : Cabrillo v3 output file implemented. Fixes also task #384.
  Tnx OH6XX, N6TV and others.

4.28.0 (June 15, 2018)

- Bugfix : When no MP3 CODEC were detected, start recording was
  displaying the MP3 settings dialog in an endless loop. Tnx N6TV.

- Single-click actions option added to all windows where it makes
  sense. Tnx K5WQG, N6TV.

- The callsign "6OX" is accepted despite its exotic syntax.

- CQWW RTTY : DC mult added according to the 2018 rules. Tnx W0YK.

- Internal CW keyer (LPT and serial outputs) : Keying compensation
  added (0 to 20 ms) in the Interfaces setup dlg. Tnx N6TV.

- Bugfix : ARI Contest : Serial numbers for DX stations have separate
  numbering per band. Tnx ES5TV.

- Bugfix : Validation controls of the split freq edit field
  strengthened.

- Icom IC-7610 added. Tnx N6TV.

- REF contest : Off-time periods dialog removed. Tnx F5LEN.

- CW / RTTY : Work dupes by default. Tnx F6IRA.

4.27.0 (Jan 4, 2018)

- Bugfix : RAC contest : Despite the rules indicate MIXED (CW + SSB)
  category only entries, the F10 wnd wasn't correctly scaled when using
  a single-mode category. Tnx SP5KP.

- Bugfix : Statistics Wnd (Ctrl-F9) : Under some specific circumstances,
  the log data weren't correctly displayed in the targets tab.
  Tnx F5LIW.

- Bugfix : Auto-repeat mode was broken (silly me !). Tnx VE2FWW, N6TV,
  W4DD and many others.

- DARC XMAS : Sprint logic exchange now applicable for this contest.
  Tnx K3LR and N6TV.

4.26.0 (Nov 19, 2017)

- LZ DX : QSO and DUPES columns were inverted in the summary window
  in single-mode categories, and CW and SSB culumns were swapped
  in Mixed category. Tnx W3SE / ZL3TE.

- SAC : Wire-Only overlay category added. Tnx OH1RX.

- Bugfix : When prefixes or callareas are mults, some special callsigns
  weren't correctly taken into account. Tnx OF100FI/0.

- CSV and text exports : Serial sent text format is identical to the
  format used in the log. Tnx F5LIW.

- Gab wnd (Alt-I) : Can be cleared now with a CLEARGAB text command.

- Bugfix : Status wnd (Alt-J) : Under some specific circumstances, the
  stations count displayed in the title bar was wrong.

4.25.0 (June 28, 2017)

- VHF+ contest : The ODX was broken under some specific circumstances.
  Tnx F5HRY/P.

- The CQ-M Cabrillo files are now following the version 3 specs.

- Bugfix : SPDX Contest : The summary window was broken. Tnx SP5KP,
  F5LIW and others. (Task #380)

- Helvetia contest : New rules 2017 implemented. Tnx HB9AMO and
  others.

- ARI DX : Allowed bands and 10-minute rule adapted to the rules
  2017. Tnx IZ1LBG. (Task #379)

- Bugfix : Asia-Pacific sprint : Win-Test was unabled to write the
  output Cabrillo file. Tnx UA9YE.

- Bugfix : Some AltGr (Ctrl + Alt) keys were not correctly displayed
  when defined in the script manager or the DEFINEKEYS command.

- Bugfix : Under some very specific circumstances of networking
  connection / disconnection and sync enabling / disabling, the log
  file could be corrupted. Tnx PA2A @ PI4CC.

- RSGB AFS : 40m added. Tnx G3RTE.

- The displayed bands selection for the Check Callsign (F9), Check
  DXCC (Alt-M), Check Mult (F10) and Check Zone (Alt-Z) windows is
  now done in a dialog box instead of menu items. Tnx F5LIW.

- NA Sprint SSB : The Multipliers list is updated and is now similar
  to the mult list of the CW/RTTY legs . Also, the equivalence is now
  NA_SPRINT.DAT for all legs, and has been updated on the repository.
  Tnx KA9FOX.

4.24.0 (Jan 20, 2017)

- CAUTION: New network protocol version 1.30 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- Lua API version string is 1.4.0

- Bugfix : Under some circumstances, the rotators wnd was flickering.

- NA Sprint CW/RTTY : Multipliers list updated. Tnx N6TV, N6TR.

  Note : You must update your NA_CW_RTTY_SPRINT.DAT equivalence file
  if you use it, to get credit for the new mults.

- To make the 3830scores.com reporting easier, the summary columns of
  the mixed mode contests are reordered.

- DXPed logs (HF and VHF) : The reports entry fields ignore keys
  which are not digits. Tnx DL6RAI.

- Bugfix : DXPed HF logs : The country list used is now the DXCC
  one, not the "CQWW" one.

- Summary wnd (Alt-S) : Displayed bands can be selected. This
  selection is in sync with the Check Callsign (F9), the Check DXCC
  (Alt-M), the Check Mult (F10) and the Check Zone (Alt-Z) windows.

  Reminder : It's only a display selection to save space : You can
  still QSY and enter Q on the hidden bands. And all bands are taken
  into account in the summary totals.

- 60m band added for the DXPed HF logs.

  NOTES :

  1/ Considering the various freq allocations depending on the
  country, a minimal band plan has been implemented in the Default
  band plan. You can modify it, according to your needs. Your custom
  band plans (if any) must be updated as well.

  2/ DXPed log files containing 60m QSO can't be read with previous
  versions of Win-Test.

  Tnx DL6RAI for testing.

- FT1000 : VFO-B frequency setting enabled. Tnx DL6RAI.

- Bugfix : FT1000 : When setting a split freq, the filter setting
  wasn't retained. Tnx DL6RAI.

- Bugfix : Typo in a menu item. Tnx DL6RAI.

- NAQP : Mult list and various other things updated according to the
  new rules. Tnx KL9A.

- Bugfix : When a callsign was grabbed, the realtime slot of the
  partners windows were not updated.

- ARRL 10m contest : Following the new rules, the multiplier "DF" is
  changed to "CMX". Tnx N6TV, N5KO.

- Bugfix : Cabrillo : The alternate frequency option wasn't working
  for multi-ops logs.

- Lua : wtQso:GetData API : Gridsquare added in the table returned.
  Tnx N6TV.

- If a station type is sticked, its type is checked against the rules
  of a newly created contest file, and can be forced to the default
  Run type if needed. Tnx N6KI and N6TV.

- Bugfix : Under some OS display settings, the Alt-F dialog was
  truncated. Tnx HA3LN.

- Bugfix : After editing logged QSO, the Alt-J QSY timers were not
  always accurate.

4.23.0 (Oct 21, 2016)

- Split Freq dlg : Now accepts offsets from the current frequency.
  Ex : If your freq is 7020 and you enter +1.1, the split freq
  will be adjusted to 7021.1. Negative values (-1.1 for ex.) also work.

- UK/EI DX contest added. Tnx SQ8N.

- Bugfix : WAG DX side : The NM exchange (Non Member) was considered
  as a N multiplier.

- Bugfix : Alt-F4 : The the CAT activity has now decreased , and the
  function was broken for mixed-mode logs. Tnx N6TV.

- Bugfix : Entering any text command in Secondary Radio Window moved
  it to the wrong band. Tnx N6TV. (Task #370/373)

- Secondary Radio wnd : Columns headings added. The color can be
  adjusted with the Colors (contextual) menu. Tnx N6TV.

- Radios : FT891, FTDX1200, FTDX3000 and FTDX5000 added. Tnx N6TV.

- Bugfix : WAE : Under some circumstances, the log and QTC backup
  files were corrupted. Tnx F5LIW.

- Bugfix : VHF+ contests : When a gridsquare of a logged QSO was
  modified, the points weren't correctly computed on the other
  networked computers, leading to a score difference between them.
  Tnx DL8AAU.

- Bugfix : Under some circumstances of simultaneous log openings on
  different machines in a network, Win-Test could crash.
  Tnx W9PA @ K3LR.

- WAE Phone : DX side : The INS and CR keys and buttons are now
  enabled in the transmit QTC dialog. The CR button tags the current
  QTC as sent. The INS button does the same, and makes the next QTC
  as the current one. It clearly makes the QTC transmission much
  easier to follow. Tnx F1HAR.

4.22.0 (August 26, 2016)

- WAE CW : DX side : The CW speed used when sending the QTC is now
  preserved between sessions, and the Rate wnd is updated accordingly.
  No need to juggle with Alt-F9/F10 anymore.

- Bugfix : WAEDC : DX side CW / SSB : The potential QTC weren't
  displayed in the radio wnd (bandmap or list) despite the option
  was checked.

- Callsign Wnd (F9) : Tooltip more readable.

- Bugfix : WAEDC : The left and right arrows now work correctly in the
  dialog to chose the number of QTC to send.

- New behaviour of the $NEXT variable in the QTC transmit messages to
  make life much easier (and less confusing) for the DX stations in
  the WAEDC CW contest.

  - $NEXT must be the first variable in the Ins message. The default
    message is now :

    $NEXT $DONE $TIME $CALLSIGN $SERIAL

    ** Update your current message if it is not **

  - When $NEXT is executed, the active QTC jumps to the next one ONLY
    if the current QTC has been already sent.

  With this new behaviour, the usual QTC transmission sequence is now :

  - Ctrl-L / Enter (or 1 to 9) to chose the number of QTC to send
    (usually 10).
  - After the QTC dlg shows up, exchange the QRV? and the QTC series
    number with the recipient.
  - From now, hit Ins for every QTC to send, one after the other.
  - If the recepient requests a full resend of the QTC just sent,
    use CR. If he requests an individual field, use the appropriate
    Fx key or button. If the QTC is ack'ed, use Ins to send the
    next one.
  - When all QTC of the series have been sent (and acknowledged),
    use Ins one last time (or Plus) to thank and save the QTC series.

  In these conditions, you normally shouldn't need to use the Up/Down
  arrows anymore unless exceptional circumstances.

- CW and RTTY : New $RAWSERIAL variable. Sends the serial number of
  the QSO with leading zeros and without any abbreviation. Now used in
  the default F3 msg (if it applies) to repeat the serial in a more
  traditional way. It also works in the QTC messages.

- Bugfix : QTC transmit dlg : The active QTC wasn't correctly
  highlighted when using the Ctrl-Fx buttons.

- Script manager dialog : Ctrl + Double click on a script brings the
  properties dialog.

- IOTA contest : If the IOTA ref is pre-filled from the callsign field
  content, the new IOTA warning is now displayed if applicable.
  Tnx F5LIW.

- IOTA contest : EXPERIMENTAL : Separate numbering for Multi-One and
  Multi-Two categories : The RUN or RUN1 stations use a sequence of
  odd numbers (starting at 1), and the MULT or RUN2 stations use a
  sequence of even numbers (starting at 2).

- IOTA contest : Multi-Two category added. Tnx G3WVG.

- IOTA contest : The WAE entities list is now used to prefill the
  island reference more accurately (ex GM/s stations). Tnx N6TV.

- The DVK bargraph can now be horizontal (default) or vertical.

- Internal DVK : The first and last 100 ms of the messages are now
  truncated to prevent the keys and mouse clicks to be heard.
  Tnx SM5AJV and N6TV.

- RTTY shortcuts buttons are now a bit thicker to accommodate older
  eyes. Tnx SP5GRM.

- Bugfix : The default Check Partial / N + 1 file for VHF contests was
  HF.DTB instead of VHF.DTB. Tnx DK5KMA.

- Bugfix : When 4.20 and 4.21 were on the same LAN (not recommended),
  with sync enabled, 4.21 was hanging. Tnx N6TV.

- Bugfix : IARU HF : If an HQ was 2 characters long, it was ignored.

- Additional CW and RTTY variables :
  - $LOC4 and $GRID4 are equivalent to $GRIDFIELD.
  - $LOC6 and $GRID6 are equivalent to $GRIDSQUARE or $LOCATOR.

4.21.0 (June 27, 2016)

- Lua API version string is 1.3.0

- Bugfix : The CW "No sound" menu item state wasn't consistent with
  the CW sound status.

- Bugfix : The check mark on Options / Disable Log Sync wasn't
  consistent when no log was opened.

- IARU HF :  Duplicate HQ abbreviations are now managed. (Task #350)

- The login / logout protocols can be now disabled as the other ones
  in the advanced network settings.

- Bugfix : The station name displayed in the network error dlg when
  several masters were on the same LAN wasn't correct.

- Log Sync : Better overall performance. Tnx DJ7TO, DL5MLO and the
  DA0HQ team.

- Cabrillo Options : New options similar to the File / Clean file
  options, but the QSO exclusions (or editions) are *only* temporary
  for the Cabrillo file output.

- ADIF Options : QSO range added.

- Mult Wnd (Alt-M) : The hide clean sweeps and hide never worked
  options are maintained during the text / SYLK copy. Tnx ES5TV.

- Bugfix : Gridsquares map window (Alt-L) : Mouse wheel actions were
  broken since version 4.7.0 !

- Bugfix : Stew Perry contest was using VHF.DTB instead of DEFAULT.SCP.
  Tnx N6TV. (Task #184).

- Tune dlg : For safety, added a 30-second timeout to automatically
  stop tuning no matter what.

- Stew Perry Challenge : Added for March, June and October.

- Bugfix : Serial communications : Under some circumstances,
  especially with some USB drivers under Windows 10, the inbound
  stream was not correctly processed. Tnx Jan @ remoterig.com

- Lua : wtQso:GetData API : stnName and stnFlags added in the table
  returned. Tnx N6TV.

- Bugfix : Voice keyer (DVK) : Under some circumstances, some audio
  output devices may miss in the Interfaces settings dialog.

- Bugfix : French Championship : QSO wih FT entities are now credited
  with 15 pts instead of 6. Tnx F4SGU.

- CW Auto Send : Updated to allow its use when both radios are in RUN
  mode. Tnx SM5AJV, N6TV.

- Lua : wtApp:TextCommand updated to add strStation and
  nNotificationID arguments. Tnx N6TV.

- Standard and additional messages : New import / export features.
  Tnx N6TV.

- Clean log dlg : New option to remove 0 points QSO from the log.
  Tnx K3LR, N6TV.

- Bugfix : Remote dlg : The text command is now limited to 13 chars,
  to comply with the log entry field. Tnx N6TV. (Task #368)

- Radios : IC-7300 added. Tnx N6TV.

- CQ WPX RTTY : M/S entrants are now allowed to 10 band changes.
  Tnx EC1KR.

4.20.0 (Jan. 17, 2016)

- Radios : IC-7600, IC-7800, IC-7850, IC-7851 : New code for a better
  management of these radios. It requires the latest firmwares.
  Tnx N6TV, K3LR, K9LA (Icom America), ICOM France, HRO Sunnyvale (CA),
  AA6W and K6SSJ.

- Radios : FT-991 added. Tnx N6TV, SP5IOU.

- Radio Wnd : New option to enable / disable the RIT display, when
  applicable. Tnx F5LIW, K3LR.

- Bugfix : ARRL 10m : Tools / Check Bad Exchanges was broken.

- PACC contest : Rules 2016. Dutch provinces (for non-PA) and DXCC and
  call areas (for PA) now count as mult per band and per mode when
  taking part in Mixed category. Tnx PA5M.

- French Championship : Rules 2016 applied. Tnx F5LEN.

- Radio Wnd : Ctrl-Up / Ctrl-Down in the list view doesn't lose cursor
  when a Q is entered. Tnx K5KG. (Task #364).

- Bugfix : Under some circumstances, the default contest log names
  were broken.

- LZ DX Contest : New rules 2015 for LZ stations applied. The only
  limitation is the 10-min rule for the M/S station, which is always
  applied for band *or mode* change, independently of the status of
  the station (RUN or MULT). Tnx LZ2CJ.

- ARRL SS : Default CW msgs updated. Tnx W2GD, N6TV.

- ARRL SS : Added new message variable $PREC (precedence) for the ARRL
  Sweepstakes, automatically determined from entry class and power
  level. Tnx N6TV.

- Bugfix : ARRL SS : Correct label for the sections field.

- Log check reports : QSO with own callsign are now ignored.
  Tnx FY5KE.

- Status wnd (Alt-J) : X-min rule timers now ignore QSO with own
  callsign. Tnx FY5KE.

- Check country wnd (F10) : QSO with own callsign are now ignored.
  Tnx FY5KE.

4.19.0 (Oct. 15, 2015)

- CAUTION: New network protocol version 1.29 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- Status Wnd (Alt-J) : Best effort to display the TX freq of the
  radios. Radio brand and model dependent. Tnx N6TV.

  Note : Icom users will need the latest Icom firmware, and the latest
  OmniRig rig definition files (check the N6TV files) to get chances
  to see VFO B displayed for Icom radios, especially if they want to
  use split mode.

- Bugfix : SAC contest : This contest wasn't displayed in October
  if the "This month only" checkbox was enabled despite the SSB leg
  takes place in October. Tnx F5LIW.

- Experimental : VHF+ spots : When the comment is using the
  "Locator<Prop>Locator" format, the second locator is now
  considered as the DX locator. Tnx G3ZAY, F5HRY.

- Bugfix : Rate Wnd (Alt-R). Various QSO rate statistics were
  wrong. Tnx CT1BOH.

- Radio Wnd : Spot mode (according to the used band plan) added in
  the tooltip text.

- Bugfix : FT1000 : The TRX was switched to RTTY-USB for high bands
  instead of RTTY-LSB. Tnx DL6RAI @ P49V.

4.18.0 (Sept. 25, 2015)

- WAE : Receive QTC dlg : Received serials are now formatted with
  leading zeroes if needed. Tnx F5LIW.

- WAE : Receive QTC dlg : Received times with 2 numbers (minutes)
  are now set to the correct hour according to the received time
  of the previous QTC. Tnx F5LIW.

- Bugfix : NA Sprint : Tools / Check log / Search for possible bad
  exchanges was broken. Tnx N6TV.

- Bugfix : Rate Wnd (Alt-R). Various QSO and Mult statistics were
  wrong. Tnx CT1BOH.

- Radios : IC-7100 and IC-7200 added. Tnx N6TV.

- Cabrillo output file (v3) : eMail address tag added.

- Cabrillo output file (v3) : New option to indicate if you wish to
  receive, if eligible, a paper certificate sent via postal mail by
  the contest sponsor. The contest sponsor may or may not honor this
  tag, and if so may or may not use opt-in or opt-out as the default.

- Cabrillo output file : New option to output the "alternate"
  frequency for split QSO. May be useful if the available CAT data for
  your radio can't be used to determine accurately the TX freq vs the
  RX freq.

- Several specific installers lacked the installation of the
  msflxgrd.ocx library. Tnx F5UPO.

- CW : SOUND/NOSOUND and associated menu items : This option is now
  always disabled when Win-Test runs under an operating system after
  Vista included. It means that it will not work for those OS, and
  *may* work on previous OS, depending on the hardware. In all cases,
  it is very recommanded to rely on the TRX internal sidetone instead.

- REG1TEST : The mode code is now output in the QSO records. It can
  be optionally omitted for contests where the mode is not stated in
  the rules, in accordance to the REG1TEST format specifications.

- Bugfix : WAEDC : The 10-min violations check was performed on the RUN
  and MULT stations, while this rule only applies to the RUN stations.
  Tnx DL1EKC.

- WAEDC : The SAVELOG, COPYLOG commands and the automatic backups now
  include the QTC files. Tnx GW3SQX @ GW7O.

- ARRL DX, ARRL 10m and ARRL 160m contests : The Cabrillo output
  files are now compliant with the v3 specs. Tnx F5PHW.

- Edit menu : New item : Apply exchange to every QSO with...(Ctrl-F10)
  When applicable, it allows to update exchanges of every Q whose the
  callsign is identical to the callsign of the current Q, with the
  exchange(s) of this Q.

- Bugfix : Partial (F12) and NP1 (F8) windows : While modifying an
  already entered QSO, the callsign of the original QSO wasn't
  correctly ignored during the searches. Tnx FY5FY.

- Gab Wnd (Alt-I) : New contextual menu item to clear the content
  of the window.

- Bugfix : WAE : Receiving QTC : If the callsign of the QTC sender was
  modified, and the receiving dialog was cancelled, the modification
  remained.

- Cabrillo file : Win-Test now ensures the operators list is correctly
  space-delimited.

- The protocol version is now displayed in the Advanced Settings dlg
  of the network.

- The Win-Test version number is no more extracted from the language
  file DLL, but rather from the exe itself, to get the correct string
  when having mutiple Win-Test versions in the same directory.
  Tnx F5TTU, F6BGC.

- Bugfix : When used in a network environment, a QSO entered on the
  secondary radio had a wrong serial number on the other machines of
  the network. Tnx DL5AOJ.

- Status Wnd (Alt-J) : When using a multi-op network, you can now
  send a remote command to a specific station by opening the context
  menu on this station name and use "Send remote command to XXX...".

- COPYLOG command : Notification added. Tnx TM0HQ.

- Bugfix : Radio wnd : Under some circumstances, when your own
  callsign was entered in the bandmap (Ctrl-Enter), it was displayed
  as a new mult. Tnx TM0HQ.

- Ctrl + PageUp / PageDown now browses the log by 12h steps instead
  of 24h initially. This makes it usable for 24h long contests.

- Bugfix : The action on Options / Disable Log Sync wasn't consistent
  when no log was opened.

- Status Wnd (Alt-J) : When using a multi-op network, you can now
  ping a specific station by opening the context menu on this station
  name and use "Ping XXX". The Win-Test version, the Master,
  Bridgehead, Sync indicators and the propagation time are returned in
  the Gab window (Alt-I). Reminder : You can use the INV (stands for
  Inventory) text command to get a summary of the complete network.

- Bugfix : Toolbar : The tooltip text for the summary icon was missing
  since the very first version of Win-Test ! ;-)

- Enhanced replies to the inventory command (INV) with a log sync
  enabled indicator (S vs s).

- IARU HF : Mult wnd (F10) : AC, R1, R2 and R3 labels updated.

- Contest settings dialog : To prevent any side effect (especially
  with the network), the syntax of the station name is checked,
  and 'exotic' characters are replaced by an underscore if needed.
  Tnx F1UVN @ TM0HQ.

- Alt-F dlg : The read-only station name field is now disabled.

- Bugfix : Alt-F dlg : Under some circumstances, the QSO op. was not
  specified.

4.17.0 (June 30, 2015)

- CAUTION: New network protocol version 1.28 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- IARU 50 MHz (and higher) contests : The PSect field of the
  output files are now in accordance to the REG1TEST specs.
  Tnx F2DX, OK2ZI.

- Bugfix : The ODX per band were sometimes wrong after band
  modifications of specific QSO. Tnx F1PKY @ F5KMB.

- Bugfix : MP3 configuration dialog : Under some circumstances, an
  error loop could occur. Tnx DL6RAI. (Task #363)

- Bugfix : FT2000 : Under some circumstances, read frequencies were
  not consistent. Tnx F8DBF, F4DXW.

- Status Wnd (Alt-J) : New column for the current op. added.
  Cf OPON/OPOFF or LOGIN/LOGOUT commands or use nicknames. Tnx ES5TV.

- Bugfix : For some contests, a QSO entered with your own callsign
  didn't count 0 points. Tnx N6TV. (Task #362)

- Set QSO freq dlg (Alt-F) : Swap main / QSX freq button added.

- Rate Wnd (Alt-R) : When entering in a category where modes can be
  mixed, the elapsed time between band changes now takes account of
  modes as well.

- CQ-M contest : To be compliant with the new rules 2015, there is no
  more multiplier station, even in M/S. Tnx RU3DNN.

- ARI contest : A station can now be set as a MULT station. The 10 min
  timer in the Alt-J wnd considers band and mode changes. Tnx ES5TV.

- OK OM DX : Win-Test is now adapted to comply to the new SSB rules.
  To make things easier, the CW leg is kept unchanged ! Read carefully
  the rules before entering. Tnx ON5GQ.

- Bugfix : MP3 QSO extract : There was a few seconds offset in the
  recording.

- Contest recorder : QSO extraction to a mp3 file : The QSO extraction
  parameters are now 1/ the time before the QSO was _STARTED_ (0 sec
  by default - it means the clip starts at the same time when you
  listen to the QSO with AltGr-Enter) and 2/ the time after the QSO
  was _ENTERED_ (10 sec by default). Tnx ES5TV.

- Bugfix : SP DX contest : When provinces were displayed with the
  "all bands" option *and* alphabetically, the "Z" province was
  missing. Tnx DL6RAI. (Task #360).

- ARRL DX and ARRL 10 : When exporting logs in ADIF, the DC "state"
  is replaced by MD. Tnx F8ATS.

- Lua : wtScript:AssignArgument now takes the strings "true" and
  "false" as boolean arguments. Numeric values do not require
  double quotes. Tnx N6TV.

- Script manager : Properties dlg : Now accepts a default argument
  even if no key is defined for the script. But, in any case, a key
  or a text command must be defined to allow a default argument.
  Tnx N6TV.

4.16.0 (Mar 17, 2015)

- Spanish and German translations updated. Tnx EB2RA and DL6RAI.

- LUA : Because of a conflict name with the wtScript class, the
  wtScript variable (name of the Topmost script) is now replaced with
  wtRootScript. Tnx N6TV.

- RDXC : R7K - Crimea (RK) and R7R - Sevastopol (SE) added to the
  mults list. Use the latest CTY_OBL.DAT accordingly. Tnx RU3DNN.

- Bugfix : REF HF : FS now does count for a French dept instead of a
  DXCC entity. The final scores were not affected by this bug.
  Tnx F4EJL.

- Lua : wtContest:GetMyCallsign() and wtStatus:GetMyStation() added.
  Tnx N6TV.

- Registration dialog : The QR codes of the registration URL are
  enlarged.

- ICOM radios : IC-970, IC-9100 and IC-7850 added. Tnx OK8WW, EA8RM
  and K3LR.

- ARRL DX (DX side) : To strictly comply with the current rules
  (section 5.2.2), the PEI multiplier (VY2) is now labelled PE. The
  STATES.DAT is also accordingly updated on the usual repository
  http://download.win-test.com/files/equivalence/ .

- NA Sprint : Because of the different multipliers per leg, the
  equivalence files must now be NA_SSB_SPRINT.DAT and
  NA_CW_RTTY_SPRINT.DAT. They are available on the usual repository
  http://download.win-test.com/files/equivalence/ . Tnx KD4D and N6TV.

- NA Sprint : DC and the usual 14 Canadian provinces and territories
  are now considered as multipliers for the Phone leg (the MAR mult.
  is no longer used). Tnx KW8N.

- UBA DX : Mult stations are now allowed for Multi-Op (Single TX)
  entries. Also, the 10-min timer for RUN stations is now displayed
  in the status window (Alt-J). Tnx RU3DNN.

- NA Sprint : KL stations are now considered as US stations and their
  state (AK) is now in the states list. KH6 stations are also
  considered as US stations for the Phone leg, and their state (HI) is
  now in the states list. During the CW / RTTY legs, KH6 stations are
  considered as DX stations (not NA). Tnx N6TV.

- ARRL 10m : Mixed mode category forced in the Cabrillo output for the
  M/S entries.

- Script properties : Tooltip added over the key edit field with the
  key code and modifiers values. It can help for the
  wtScript:AssignKeyCode function. Tnx N6TV.

- Scripts manager : Run button added. The selected script is run the
  same way as if it were run by the assigned key (if any),
  and with the argument set in the properties dialog (if any).
  Tnx N6TV.

- Lua : wtScript:AssignFKey and wtScript:AssignKeyCode functions added.
  Tnx N6TV.

- Bugfix : If the default directory at launch time wasn't the app
  directory, the automatic starts of wtDxTelnet and wtRotators were
  failing. Tnx F5LIW.

- Script Manager : Error message added when the SciTE or the script
  editor weren't correctly installed or configured. Tnx DL6RAI.

- Bugfix : Ctrl-Del (delete spot from bandmap) was broken.
  Tnx N6TV. (Task #354)

- Bugfix : Network advanced settings dialog : The last outbound
  protocol was always enabled, despite its setting. Tnx F1HAR.

- New CW and RTTY variables introduced : $GRAB1 to $GRAB9 to grab from
  the partner stack slots, and $GRABRT1 to GRABRT3 to grab from the
  partner realtime slots.

- Bugfix : Common prefixes to GM and GM/s were considered as GM even
  if the WAE list was used. Tnx N6TV. (Task #355)

4.15.0 (Nov 22, 2014)

- CAUTION: New network protocol version 1.27 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- Contest recorder : AltGr+E shortcut added as "Extract and Save
  QSO". Tnx N6TV.

- LZ-DX contest : 10 min. CQWW DX rule applied to the M/S entrants,
  but currently limited to the band changes (the mode changes are
  ignored). Tnx RU3DNN.

- Partner : There are now two different colors for data entered as
  Run or as Support. Useful when there are several partner positions
  for one run. Tnx F5HRY@TM0HQ.

- Bugfix : When a voice message contained several script calls in a
  row, only one out of two was executed. Tnx N6TV.

- Bugfix : ARRL SS : When a callsign is grabbed, the cursor is now
  set to the serial field. Tnx AC6T, N6TV. (Task #353)

- ESM : When not using advanced SO2R with Shift bound to the secondary
  radio, Shift-Enter now has no action. Tnx N6TV.

- Bugfix : Partner window : The SUPPORT / NOSUPPORT (or
  PARTNER / NOPARTNER) commands didn't resize the window properly.

- Bugfix : Partner window contextual menu : The "Remove" item was
  enabled for empty slots while it was supposed to be grayed.

- Bugfix : If the same callsign was in two adjacent slots in the
  Partner stack, only one of them was cleared when the callsign
  was entered in the log.

4.14.0 (Oct 19, 2014)

- CAUTION: New network protocol version 1.26 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- New notes file format and network protocol to ease log corrections
  within Win-Test. Check the new last items of the Tools / Check
  log menu.

- Partner : New properties dialog to set the various options.
  By default, the realtime keystrokes network transmission is disabled
  when switched to the S&P mode. It can be enabled by choice in
  this properties dlg. Tnx TM0HQ & N6TV.

- Bugfix : When several mp3 record files from different stations for
  a given contest were used, the rewind and forward functions led
  to a crash. Tnx DL8AAU@DR9A.

- Bugfix : Lua : An error occurred when calling a script with the
  double-quote key. Tnx N6TV.

- Bugfix : RDAC : The Tools / Check log / Search for bad exchanges
  function was not working for the RDAC contest. Tnx SP5KP

- IARU HF : A '?' indicator is now displayed when the received exchange
  is not an ITU zone, AC, R1, R2 or R3, or not composed of letters
  only.

- Radio wnd : When using a Windows font size option different from
  100%, the VFO displays didn't scale up well. Tnx N6XI, N6TV.

- New option in Tools / Check log / Search for bad exchanges, to
  detect exchanges discrepancies in the log only.

- Merge report redesigned : All conflicts are ordered by time and
  also by station name.

- The Date/Time dialog (Alt-F) now indicates the station who entered
  the QSO. Not editable. Tnx F8CRH@TM0HQ.

- New Goto Callsign edit menu (Shortcut Shift+Ctrl+G) to set the
  cursor on a QSO with a given callsign. By default, the callsign
  of the current QSO is searched. If it is empty (ie if the cursor
  is set to the last (empty) line of the log), a dialog is opened.
  The search is done backwards.

- New CW option to enable/disable the speed bursts (+/-) without
  modifying the messages. Text commands are BURSTS / NOBURSTS.
  Useful to defeat CW skimmers on-demand.

- Interfaces setup dialog : The lists for each COM port are now
  reordered to comply with the most current needs.

- Bugfix : In the Alt-M wnd, when data were ordered by number of
  worked bands/modes, and never worked mults were hidden, the sweep
  clean mults were always displayed, despite this option was set or
  not. Tnx CT1BOH.

4.13.0 (Jun 30, 2014)

- EF6 added as a valid exception callsign. Tnx F6FDR.

- Bugfix : REF DDFM 50 MHz contest : Default CW msgs were using
  $GRIDSQUARE (6-char locator) instead of $GRIDFIELD (4-char locator).
  Tnx F2DX.

- Bugfix : Gab window (Alt-I) : If the content was scrolled back, a
  double-click on a line set an incorrect default recipient in the
  opened Gab/Talk dialog. Tnx F8CRH@F6KRK.

- Bugfix : REF VHF contest : Win-Test was asking for the "departement"
  in the contest settings dialog (was useless), and the help dialog
  was inappropriate. Tnx F5HRY.

- Radio windows - List view : In the "Sort by Mult Type" view, the
  non-mults stations are now sorted by QSO points in descending
  order. Tnx G3WW.

- Radio windows - List view : New sorting option by QSO points in
  descending order, irrelevant of mults, added. Tnx G3WW.

- WRTC 2014 and IARU HF : Check multiplier wnd (F10) : New label for
  HQs "entities" to prevent confusion with DXCC entities. Tnx CT1BOH.

- Log : The column header of the serial sent (if any) is now correctly
  labeled ("No."). Tnx N6TV.

- Options / Log / Align exchanges : New option to line up received
  exchanges in mixed mode. Tnx N6TV.

- WRTC 2014 : Worked Mults wnd (Alt-M). The "copy as text" menu item
  is now enabled. Tnx CT1BOH.

- CQ-M contest : Contest identifier for the Cabrillo and ADIF output
  files were misspelled. Tnx RU3RQ. (Task #348).

- WRTC 2014 : /MM stations are not counting for DXCC entity, and are
  credited depending on their ITU zone. Tnx KM3T.

- WRTC 2014 : The country list used is DXCC (not WAE). Tnx KM3T.

- WRTC 2014 : In the contest configuration dialog, the zone is set
  to 8, the Gridsquare is set to FN42fg and can't be modified.

- The very singular 7QNL (and future 7QAA) callsigns are now accepted.
  Their prefixes are also resolved as 7Q0. Tnx PA3FYM.

- Bugfix : WPX : The prefix of VY2MGY/3 now resolved as VY3. Tnx N6TV.
  (Task #347).

- Lookup function for the DXCC entities resolver refactored to allow
  easier extension for cases like the newly introduced 4Y1A and C7A,
  when callsigns are assigned to two entities.

- RTTY : Fields assignments updated for the NCCC Sprint. Tnx AA2MF.

- King Of Spain contest : SMR multiplier added. Tnx EA4TX.

- Marconi HF : New points rules applied. Tnx IK6BAK.

- Bugfix : Lua : wtApp:CallScript(name, arg) was always casting arg
  to a string. Tnx N6TV.

- Lua : In CW, when chaining wtKeyer:Play() instructions, the word
  space between the string arguments will be omitted if they end with
  a "~".

  Example :

    wtKeyer:Play(string1)
    wtKeyer:Play(string2)

  Will omit the word space between string1 and string2 if string1
  ends with a "~".

  Tnx N6TV.

4.12.0 (Feb 10, 2014)

- Bugfix : UBA DX : The format of the output cabrillo file didn't
  stick to the required specs. Tnx ON5GQ.

- Bugfix : DARC 10 : Under some circumstances, the DOK field was
  cleared while it wasn't necessary. Tnx DJ4MZ.

- DARC 10 : The NM exchange (Non Member) is no more considered as a
  multiplier. Tnx DJ4MZ.

- Radios : IC-7410 added. Tnx DL6RAI.

- Bugfix : Lua : The wtApp:CallScript function was always returning
  a nil value when used with two parameters. Tnx N6TV.

- Script Manager : Various UI enhancements and API bugfixes. Tnx N6TV.

- Bugfix : The log sync enables / disabled setting was not correctly
  saved between logs openings. Tnx DK9TN@ED6A.

- Clear Log : The station type (RUN, MULT, etc.) setting is now
  preserved when this function is performed. Tnx DK9TN@TK4W.

- Network : Time distribution : A warning now pops up when time sync
  frames are received, and the Windows user who started Win-Test
  hasn't enough privilege to modify the system clock. Tnx P40L, N6TV.

- Lua : wtQso:GetData() returned table updated for the specific ARRL
  Sweepstakes contest. The QSO# received is in the "rstReceived"
  index, and the Precedence letter is in the "miscInfo2Received"
  index. Tnx N6TV. (Task #338).

- Mult Window (Alt-M) : New "Hide never worked" option added. Pretty
  experimental for now, depending on the contest. Tnx CT1BOH.

- Radio windows : The spot selected by a right click is now
  highlighted to prevent confusion. The highlight color calculation
  now also works for dark hues. Tnx AD1C@K0RF.

- Stats window : In CQWW DX, the zones / overall display was clipped
  to the last hour when a new zone was worked.

- Radio windows : Time / Spotter and Comments display options added in
  the list view. These settings are common to both views. Tnx CT1BOH.

4.11.0 (Oct 20, 2013)

- Networking : Sockets initializations updated to comply with the
  usage of Win-Test in a Linux / Wine environment. The wtCom.dll
  must be updated (v2.0.4 or better) as well for this usage if needed.
  Tnx AA6KJ.

- Bugfix : CQWW RTTY : The check log tool for the number of allowed
  QSY per hour in M/S was broken. Tnx DL9YAJ @ DR5N.

- Bugfix : Frequency offsets weren't always correctly processed,
  especially on the secondary radio. Tnx DL5AOJ.

- Bugfix : Extra Data files : Depending on the newline character(s)
  and other various parameters, the displayed data could be incorrect.
  Tnx IK0HBN, N6TV.

- ADIF output : Addition of the CREATED_TIMESTAMP field in the header,
  and the CONTEST_ID field in every QSO record, when applicable.

- Bugfix : When a log was entirely entered manually, the date of QSO
  wasn't correctly set when using the "<" or ">" keys to access and
  fill the time field. Tnx F5LEN.

- ADIF Export : The ADIF country code is now added to the QSO record.
  Requires using the latest CTY_WT.DAT or CTY_WT_MOD.DAT country
  files (02 August 2013 or later). Tnx AD1C.

- CQWW DX Contest : The overlay "Classic" category has been added in
  the contest configuration dialog. It only adds the appropriate line
  in the Cabrillo output file.

- WAE Contest : The special calculation for the creation of the offtime
  section in the Cabrillo file has been removed, being now obsolete.
  Tnx DL6RAI.

- WAE Contest : Offtime threshold is now set to one hour.

- Bugfix : Under some circumstances of startup order and various
  settings, a "20 days older or newer log" false alert might be
  triggered. Tnx F6BGC @ TM0HQ.

- Lua : wtQso:GetData() function added. Returns a table with fields
  of the current Qso. The current available keys are "time", "band",
  "mode", "freq", "callsign", "rstSent", "serialSent", "rstReceived",
  "exchReceived", "miscInfoReceived", "miscInfo2Received".

- UFT contest : Win-Test is now adapted to the new rules 2013.
  Tnx F6CEL.

- YU DX contest : Totally rewritten because of the new rules 2013
  (see http://yudx.yu1srs.org.rs/2013/rules.html). Tnx YU0W and F5IN.

- SPDX Contest : The "12 band or mode changes per one clock hour"
  rule is now implemented. A simultaneous change of band *and* mode
  (Ex: 80m CW -> 40m SSB) counts as 2 changes. Tnx SQ2GXO.

- Bugfix : RDAC Contest : Exchanges for callsigns ending with /x
  (x = 0 to 9) are now searched in the database and the log.
  Tnx SP5KP.

- New Tools / Data entry / Priority / Callsign option to ignore any
  freq or band changes when entering digits only in the callsign field.
  Tnx P40L, N6TV.

- Bugfix : AGCW HNY : The (optional) AGCW membership number entry field
  was emptied when it was not supposed to be ! Tnx DJ0ZY.

- Bugfix : Displayed ODX inconstancy under some circumstances when a
  QSO was deleted. Tnx DL6RAI.

- Bugfix : RAEM : The coordinates entry field was emptied when it was
  not supposed to be ! Tnx DJ0ZY.

- RAC Winter and Canada Day Contests : The 10-minute rule for the
  multi-single entrants is now implemented. Tnx VE3JM and N6TV.

- Russian 160 meter : New rules implemented.

  http://www.radio.ru/cq/contest/rule-results/index2012.shtml

  Tnx RZ3DX.

- Lua : wtApp:GetLogFileName() and wtApp:GetIniFileName() functions
  added. Tnx N6TV.

- Bugfix : When using the GOTO function by entering a QSO number
  and Ctrl-G, the pattern analyser warning message (if any) is now
  cleared.

- CQWW DX : The overlay category Xtreme is added in the contest
  configuration dialog, and in the Cabrillo file output as well.
  Tnx KL1A.

- QR Code added in the registration dialog to help mobile phones
  users.

- Bugfix : The modifications entered into the Freq Offsets dialog
  are now taken into account immediately. No need to reload the current
  log. Tnx YL2GD.

- Bugfix : When using a K3, changing band by entering its wavelength
  was sometimes setting the wrong LSB/USB mode. Tnx M0VFC (Task #326)

- Bugfix : Under some circumstances, a random character could be
  entered in the Info field in a DXPed log, when using the Up/Down
  arrows in this field.

4.10.0 (Oct 23, 2012)

- YO DX Contest : The child and log windows are now compliant with
  the chosen mode category (CW, SSB or MIXED). Previously, the mixed
  mode only was assumed.

- Bugfix : NAQP : The K8 mark for "zones window" (Alt-Z) was labeled
  K81 instead. Tnx NX5M.

- Bugfix : Text and CSV files options dialogs : The Del key was
  acting as "Remove all" instead of "Remove".

  Reminder : Shift-Del acts now as "Remove all", Del acts as
  "Remove", Shift-Ins acts as "Add all" and Ins acts as "Add".
  Tnx TM0HQ.

- Bugfix : In the logfile fixing process, the backuped file had a wrong
  file extension (it was always .wtb). Tnx TM0HQ.

- Bugfix : Status wnd (Alt-J) : Not always correctly ordered when
  sorted by freq/name. Tnx TM0HQ.

- ARRL Sweepstakes, ARRL FD and ARRL 160 meter contests : ARRL/RAC
  sections list updated to comply with the four new RAC administrative
  sections (ONN, ONS, ONE, GTA), replacing the split Ontario
  Section. (Task #321)

- Auto CQ : New option in the appropriate dialog to halt the auto CQ
  with the Esc key only. Equivalent text commands are RPTESCONLY and
  NORPTESCONLY. Tnx N6TV.

- ARI Sezioni : Cabrillo output compliant with rules 2012. Tnx I2WIJ.

- ARI DX : Cabrillo output compliant with rules 2012. Tnx I2WIJ.

- IOTA : New rules 2012 implemented :
  - For multi-op (island) stations, display of Band/Mode changes in
    the rate window (Alt-R).
  - Cabrillo file : QSO lines now include RUN or MULT identifiers.
  - The score for World to World QSOs is reduced from 3 points to 2
    points.
  - Island Stations now receive 5 points for World Station QSOs.
  - Island Stations now receive also 5 points when working their
    own Island.

- RDXC : Oblasts window (Alt-Z) updated following the new list 2012.
  Tnx HA1AG, SP5KP, F5IN.

- Bugfix : CQ VHF and CQ 160 : ARRL Section added in the Cabrillo
  output file for US/VE entrants (Task #323). Tnx W9ZRX & N6TV.

- FT1000(D) : The IF filter setting is retained per mode when grabbing
  a spot. Tnx DL6FBL @ DR1A.

- Check partial (F12) and NP1 (F8) wnds : The [UNIQUE] word has now
  its own background and text colors to draw the attention of the
  operator. Tnx CT1BOH.

- Bugfix : Under some concurrency circumstances in a multi-op
  environment, Win-Test could crash when deleting or modifying spots
  in the Alt-A or the radio wnds (Task #318). Tnx N6TV.

- JIDX : Cabrillo file : QSO lines format updated to comply with the
  new format specifications for the multi-op category.
  (See task #317). Tnx N6TV.

4.9.1 (Oct 27, 2011)

- Fix an issue with missing resources which might make WT to crash.

4.9.0 (Oct 26, 2011)

- Problem in Spannish language file fixed. Tks N6TV.

- When a new file is created, the usage of a network drive is checked
  and strongly discouraged to prevent log inconstancy. Tnx VK8DX @ 4W6A

- Bugfix : The exceptions callsigns of the CTY*.DAT files were wrongly
  parsed when operated from another DXCC entity (ex. W6HGF/KH0).
  Tnx JE2UFF.

- WAEDC : Time shift can now be applied to the QTC. Tnx DL8RDL.

- NCCC Sprint : New rule 2011 : 15m QSO are now permitted.
  (See task #312). Tnx N6TV.

- Bugfix : During a Cabrillo import, if the format of the QSO line
  wasn't correct, the error message was off one on the QSO number.
  Tnx W6IZT.

- Bugfix : IARU HF contest : The mode entry was empty in the output
  Cabrillo file for multi-op categories. It is now set to mixed.
  Tnx F1HAR @ TM0HQ.

- Bugfix : K3 : The Kenwood radio protocol was broken when sending
  CAT commands with frequencies above the 3420 MHz band. Tnx W8ZN.

- Bugfix : Task #310 : IARU HF contest : For US/VE stations, the ARRL
  section is now required, instead of the state or the province.
  Tnx N6TV.

- Bugfix : Entering your own callsign in the bandmap (Ctrl-Enter) was
  displaying a "spotted by..." alert. Tnx F5JSD @ TM0HQ.

4.8.0 (june 26, 2011)

- ADIF : PROGRAMID and PROGRAMVERSION fields added in the file header.
  Tnx IZ8MBW.

- Bugfix : Task #308 : JIDX : 160m QSO points counted 1 pt instead of
  4. Tnx N6KI and N6TV.

- LPT Interface : 50 MHz, 144 MHz and 432 (440) MHz band data outputs
  added. Tnx W8ZN and N6TV.

- Callsign check rules : The pathetic 9HOHSJ callsign is now added as
  an exception (like RAEM, JY1 and TX9). Tnx OH2OT, F5HRY.

- PACC contest : New rule 2011 : QSO are now allowed in each mode for
  mixed categories. Tnx PA2A.

- RSGB 160m contest : Single-mode CW-only restriction removed to
  comply with the new rules 2011. QSO and bonuses are now allowed for
  each mode. Tnx G3XSV.

- NAQP : Cabrillo output : The DXCC prefix is now indicated instead
  of "DX" for North American stations outside of K/VE. Tnx WA7BNM.

- DARC XMas contest : New rules 2010 : "NM" is allowed as a exchange
  from the German stations, but is no more credited as a mult.
  Tnx DJ3WE.

- DX Spots window (Alt-A) : New option to enable/disable logging of
  the incoming spots in the .dxc file. It is enabled by default. Under
  some circumstances (slow antivirus inspection, slow HDD, etc.),
  saving every spot (especially when using the RBN) was making Win-Test
  less responsive. The op-entered spots are always saved to allow their
  restoration on log startup. Tnx HA1AG @ ED9M.

- Packet window (Alt-O) : New option to enable/disable logging of
  the packet stream in the .pkt file. It is enabled by default. Under
  some circumstances (slow antivirus inspection, slow HDD, etc.),
  saving the packet data stream (especially when using the RBN) was
  making Win-Test less responsive. Tnx HA1AG @ ED9M.

- Bugfix : Under some circumstances, DXped audio recordings were not
  correctly tagged, the file information dialog was incomplete, and
  the QSO playbacks failed. Tnx VE3EY @ TO3A.

4.7.0 (Dec 2, 2010)

- CW Autosend : Feature temporarily disabled when Alt-Space (grab from
  the RT partner slot), Alt-1..9 (grab from the partner stack) and
  Ctrl-1..9 (exchange with the partner stack) are used.
  Tnx ES5TV, N6TV.

- WinKey : Speed bursts were not executed if located just before the
  $LOGGED variable. Tnx ES5TV.

- ARRL 10m contest : New Mexican multipliers added. The name of the
  database (which is now different from the other ARRL contests) is
  now ARRL_10M.DTB. Several XE stations (around 300) have been added
  in the current file :

  http://download.win-test.com/databases/ARRL_10M.DTB

- Bugfix : Task #300 : WAEDC RTTY : The sent QTC group number was not
  taken into acount by the other connected machines, and therefore the
  QTC numbering was garbled in M/* environment. Tnx DL6RAI.

- Bugfix : Task #266 : WAEDC RTTY : No *New Mult* warning. Tnx DL6RAI.

- Bugfix : WAEDC : Number of QTC to send dialog : Even if some buttons
  were disabled, their associated "number keys" were still active.

- Bugfix : WAEDC : Sending QTC dialog (Ctrl-L) : In "show" context,
  and if messages were sent under some circumstances, Win-Test could
  crash. Tnx IW1QN.

- Bugfix : WAEDC : Under some circumstances, sent QTC were not always
  correctly saved.

- Bugfix : WAEDC : When the number of QTC to be sent is 0 (no more QTC
  available), all "number keys" and Enter are now ignored in the
  appropriate dialog.

- Bugfix : Task #298 : Spacebar key didn't always work properly in the
  ARRL Sweepstakes contest. Tnx N6TV.

- Bugfix : Task #297 : Double-click on Check Multipliers window (F10)
  didn't work in ARRL Sweepstakes. Tnx N6TV

- MouseWheel actions are now compatible with HiRes optical mouses like
  the Microsoft Wireless LASER Mouse 8000. Tnx W9ZRX, N6TV.

- Bugfix : Under some circumstances, if data entered in the time field
  didn't follow the HH:MM or HHMM format, it could lead to a crash.
  Tnx N6TV.

- Bandmap properties : The minimum spot bandwidth is now 0 Hz (!).
  Tnx SM2WMV.

- IC775 : Force narrow IF filters when grabbing callsigns in CW.
  Tnx YL2GD.

4.6.1 (Released only for demo and DxPed versions)

- Bugfix : The default directory name for a "DX expedition (VHF and
  above)" log was wrong. Tnx DJ4MZ.

- Bugfix : When a callsign was entered by a dbl-click in the N+1 or the
  partials wnd, and if this feature was set to automatic, the callsign
  check status wasn't updated. Tnx ES5TV.

- COPYLOGCLEAR text command added. Equivalent to the COPYLOG command
  immediately followed by a CLEARLOG command. Tnx CT1BOH.

- QTC receive dlg : New variable $QTCROW introduced indicating the
  QTC line number where the cursor is located. Mainly used in RTTY
  for asking a resent of a specific line. The default F8 button message
  is now "AGN QTC $QTCROW?" in this mode. Tnx DK4WA.

4.6.0 (Oct 24, 2010)

- CAUTION: New network protocol version 1.25 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- The wtArg (and wtArgument) variables are now local to the called
  script.

- Bugfix : Task #296 : Check mult window (F10) was not updated properly
  when using in ESM mode with S&P mode selected. Tnx N6TV.

- For phone contesting, scripts can be called from the Advanced SO2R
  scenarios with the #SCRIPT or #@SCRIPT notation.

- Bugfix : Under some circumstances, the default filename of a contest
  log could contain invalid characters. Tnx G0ORH.

- Lua scripting : New input API :

  - wtApp:InputUpperText(Prompt, Title, Default)
    If Title or Prompt is empty, a default text is used. Typed letters
    are automatically upper-cased while entering.

- Bugfix : Second zones window : The labels display option was not
  restored.

- Bugfix : When grabbing a callsign in the RTTY window, the realtime
  partner window field wasn't updated. Tnx ES5TV.

- Lua scripting : New wtGab API introduced :

  - wtGab:Send(strText[, strToStation]) sends a gab strText to
    strToStation. If strToStation is omitted, the text is sent
    to the whole network.

- NCCC Sprint : New rules implemented. Tnx K9MMS, N6TV.

- Bugfix : Task #290 : On restart, Win-Test didn't remember the last
  SO2R scenario that was selected. Tnx N6TV.

- CQWW RTTY : In M/S category, the band changes counts are now
  displayed for the RUN and the MULT stations in the rate window
  (Alt-R). Tnx ES5TV.

- Edition keys : To improve the compatibility with CT, Ctrl-B, Ctrl-D
  and Ctrl-F keys are now processed in the log fields. Tnx N5KO, N6TV.

- WAEDC : QTC receive dialog (Alt-L) : New $FIELD variable introduced.
  This variable takes the value "GROUP", "TIME", "CL" or "NR",
  depending on the kind of QTC field where the insertion point is
  located.

- Bugfix : WAEDC : QTC receive dialog (Alt-L). Using the INSERT key in
  this dlg was crashing Win-Test.

- New CW and RTTY options to work dupes or not. If dupes are worked,
  the $QSOB4 variable is ignored. The equivalent text commands are
  WORKDUPE/NOWORKDUPE or WORKDUPEON/WORKDUPEOFF. There is a
  different setting available per mode (CW or RTTY).

- Bugfix : Task #291 : RadioWnd : Ctrl-Up/Down weren't working properly
  in list mode. Tnx ES5TV.

- Bugfix : Under some circumstances, Win-Test could crash when started
  with the CapsLock key engaged.

- Task #205 : The $RxRy variables located in the end of a CW message,
  if any, are automatically appended to the content of the $QSOB4
  message if played. Tnx N6TV.

- The $QSOB4 variable can now include scripts calls.

- The scripts calls in the CW or RTTY messages are now synchronous to
  the CW or the RTTY streams. To execute them asynchronously, they
  can be called with the #@ notation. Example :

  -- script.wts

  wtApp:AlertBox("Hello World!");

  and the CW/RTTY message content is :

  AAA #SCRIPT BBB

  The keyer sends AAA, then "waits" until the user hits the OK
  button in the "Hello World!" alert box to send BBB.

  If the CW/RTTY message content is :

  AAA #@SCRIPT BBB

  The keyer sends AAA and starts the script (and the alert box is
  open), *but* it continues to key the rest of the message ("BBB")
  without waiting the user intervention. This is the asynchronous
  mode.

- Lua scripting : One new wtKeyer API introduced :

  - wtKeyer:Insert(strMessage) : Works for the CW and RTTY keyers.
    When used in a synchroneous script, if gives the possibility
    to "fill-in" data into the CW/RTTY message. It is recommanded
    to use it only in the synchroneous mode (see above) to ensure
    data are inserted in the right place.

  WARNING : strMessage can only contain textual data (no variable
  or script call). It is *not* interpreted by the CW/RTTY parser
  (except the +/- speed bursts).

- Lua scripting : New wtStatus API introduced :

  - wtStatus:GetList() returns a table with names of the stations
    in the network.
  - wtStatus:GetStatus(strStation) returns a table with fields of
    the status of a given station. Returns nil if this station
    doesn't exist. The table keys are "band" "mode" "currentRadio"
    "radio1Freq" "radio2Freq" "radio1IsManual" "radio2IsManual"
    "passFreq" "type" and "qsyStatusId".
  - wtStatus:GetFreq(strBand[, strMode]) returns the "best" pass
    freq for a given band and mode. To determine this frequency,
    it uses the same algorithm as the $FREQnn variable.

- Lua scripting : New wtOtrsp API introduced :

  - wtOtrsp:GetDeviceName() returns the name of the OTRSP attached
    device.
  - wtOtrsp:GetFirmwareVersion() returns the firmware version of the
    OTRSP attached device. NOTE : Some devices do not support this
    API, and return an empty string.
  - wtOtrsp:Send(strCommand) sends a command string to the OTRSP
    attached device. The trailing <CR> character is optional, and is
    appended if needed.

- Scripts manager dialog usability improved. Tnx N6TV.

- OTRSP : If the OTRSP device has controls and if they can generate
  events, dedicated Lua scripts are called when events occur :

  - otrspCrOn.wts and otrspCrOff.wts (not case-sensitive) are called
    when such a control has values 1 and 0 respectively. wtArg is set
    to the control number (0 to 9).
  - otrspCrEvent.wts (not case-sensitive) is called for all states
    of the events. wtArg is set to (256 * cr) + state (cr = control
    number - 1 to 9, and state = value of the state when the event
    occured - 0 to 255).

  WARNING : If the PTT events are used, the control 0 is restricted
  to this usage, and doesn't fire the otrspCrOn/Off/Event.wts
  scripts. If the PTT events are not used, otrspCrEvent is not
  called when an event on this control occured. Only the
  otrspCrOn/Off scripts are executed.

- microHAM devices : When an attached footswitch is used, two
  dedicated Lua scripts named microhamFsOn.wts and microhamFsOff.wts
  (not case-sensitive) are called. wtArg is set the radio number of
  the footswitch (0 for MK/MKII - 0 or 1 for MK2R/MK2R+/u2R depending
  on the footswitch that generated the event).

- Elecraft K3 : To circumvent erratic loss of control when used
  with various other devices, CAT stacked commands are now sent
  in a delayed sequence. Tnx N6TV, N6XI, and others.

- Bugfix : Advanced SO2R CW messages dialog : The Esc and Enter
  keys now work.

- Lua Scripting : New wtMicroham API introduced :

  - wtMicroham:GetDeviceId() returns the ID of the microHAM attached
    device. Check the Lua constants for interpretation.
  - wtMicroham:GetFirmwareVersion() returns the firmware version
    string of the microHAM attached device.
  - wtMicroham:Send(strCommand) sends a command string to the
    microHAM attached device . The trailing <CR> character is
    optional, and is appended if needed.

  Tnx ES5TV, N6TV, OM7ZZ.

- Contest settings dialog : The contest combo box is now divided in
  sections.

- Status Wnd (Alt-J) : Code rewritten to adapt the window columns
  to the contest in progress : The band is displayed if the current
  contest is multi-band. The mode is displayed if the current
  contest is multi-mode, and the type (R, M, etc.) is only
  displayed for Multi-Op HF contests. Also, when the CQWW M/S
  multiplier rule is used, new indicators are displayed in the QSY
  column.

- Status Wnd (Alt-J) : Rewording of "QSY Freq" to "Pass Freq".
  Menu items adapted too.

- Status Wnd (Alt-J) : When operating in SO1R/Multi-Op technique,
  the Radio 2 freq is automatically hidden, and the Radio 1 freq
  is now using the same color as the other items of the line.

- RDA Contest : All DXCC entities are taken into account for
  multipliers, even the Russian ones. Tnx UA2FF and RX3RC.

- COPYLOG text command added : Duplicate the current log file (.wt4)
  in the current log directory with a timestamp added in its name.
  Useful to quickly save the current log right after a contest
  warm-up, just before clearing it (CLEARLOG) and start the contest.
  Tnx DL6RAI for inspiration.

- Bugfix : WAEDC : Clock wnd : QTC in stock was always displayed for
  M/S entrants regardless of their location (EU or DX).

- Bugfix : WAEDC : Clock wnd : QTC in stock value was not immediately
  updated after a Q was received thru the network.

- MP3 Contest Player : You can now select which channel(s) - Left,
  Right or Stereo - to listen to. When Left or Right is selected,
  this channel is sent to both outputs for a more pleasant listening.
  Useful to listen to true SO2R stereo recordings. The shortcuts
  (AltGr+C for Left / AltGr+V for Stereo / AltGr+B for Right) have
  been chosen for their location on the keyboard.

- WAEDC : Received QTC window (Alt-L) : The contest recorder keys
  are now active also in this window.

- Bugfix : EZMaster, MK/MKII/... and OTRSP setup dialogs : The Esc
  and Enter keys were not correctly handled.

- RDA contest : ADIF export : The first two chars of received
  district (if applicable) are saved as STATE field and the district
  (reformatted as XX-dd) is saved as CNTY. Tnx UA2FF.

- RDA contest : For Russian entrants, a QSO with a /P Russian
  station (assumed to be a C1 or C2 stations) is now credited with
  10 pts. Note that using /P for C1 or C2 stations is *not* mandatory
  (Check the note 5.2 of the English rules). Tnx UA6AA.

- WAEDC : Received QTC window (Alt-L) : The ESC key only works if no
  field have been edited (and closes the dialog). If a field has been
  edited, the ESC has no action (except interrupting CW etc.).
  Tnx F5VIH/SV3SJ.

- Bugfix : Transmit QTC window (Ctrl-L) : Under some circumstances,
  the context-oriented background colors were not correctly updated.

- WAEDC : Transmit and Receive QTC windows (Ctrl-L and Alt-L) :
  Modified wordings for some buttons, and easier usability for users,
  especially when using Esc and Ctrl-L/Alt-L to close these
  windows. Tnx DL6RAI, DF9LF, G3TXF.

- WAEDC : Transmit QTC window (Ctrl-L) : In CW or RTTY, if no QTC
  is sent, the Ctrl-L and Esc keys close the dialog with no
  confirmation asked. Tnx DL6RAI.

- WAEDC : Receive QTC window (Alt-L) : If no field is edited, the
  Alt-L and Esc keys close the dialog with no confirmation asked.
  Tnx DL6RAI.

- WAEDC : Receive QTC window (Alt-L) : To improve consistency with
  the log edition keys, a new key set is introduced :

  Alt-Arrows : Moving from one field to another (replace Ctrl-Arrows)
  Shift-Backspace: Delete all the characters left of the cursor
  Shift-Del: Delete all characters under and right of the cursor
  Ctrl-A: Like [Home]
  Ctrl-E: Like [End]
  Ctrl-W: Clear the current field
  Ctrl-K: Like [Shift-Del]
  Ctrl-Z: Undo field edition
  Ctrl-Left arrow: Like [Home]
  Ctrl-Right arrow: Like [End]

  Tnx F5VIH/SV3SJ

- Bugfix : WAEDC : After receiving QTC, the potential QTC counts in
  the bandmaps were not always updated. Tnx DF9LJ.

- Bugfix : WAEDC : Every time a Cabrillo file or a summary file was
  written, the QTC counts were increased. Tnx DF9LJ, DL6RAI, and
  several others.

- WAEDC : If the "Show additional information on QTC traffic" option
  is enabled, the callsign syntax check status messages are no more
  displayed, to free the message line for the QTC status. Only applies
  to the WAEDC. Tnx DJ0ZY.

- LUA scripting : Two new global variables wtScript and wtCurrentScript
  introduced. wtScript contains the name of the top-most called script,
  with no extension, and wtCurrentScript contains the script name
  currently executed (no extension). For example :

  -- foo.wts
  wtApp:AlertBox(wtScript .. " / " .. wtCurrentScript);
  wtApp:CallScript("bar");
  return -1;
  --

  -- bar.wts
  wtApp:AlertBox(wtScript .. " / " .. wtCurrentScript);
  --

  When foo is executed, the first alert box will display "foo / foo"
  and the next one will display "foo / bar".

  Tnx N6TV.

- Check country wnd (F10) : New option to display (or not) the sun
  charts. Tnx N6TV.

- Bugfix : KCJ : TG (Tochigi) and NR (Nara) multipliers were missing
  in the Alt-Z window. Tnx F5IN.

- ESM embedded script : When using the SO2R advanced technique, the
  scenarios messages are used instead of the standard ones.
  Tnx SM2WMV, N6TV and F6IFY.

- Bugfix : NAC 10 : Exchange sent are now 6-positions gridsquares.
  Tnx SM6FKF.

- Remote commands dialog : Various different options for the
  notification are now allowed.

- Script manager : Added the possibility to attach a text command to
  a script. You can even pass a argument with the SCRIPT/ARGUMENT
  syntax (ex : SCRIPT/5 will call script.wts and the wtArg value is
  set to the string "5" - Caution : The argument is *always* passed
  as a string when the script is called from a text command). If no
  argument is specified, the default argument defined in the script
  manager will be used (if any). Tnx N6TV.

- IARU HF : Mult wnd (Alt-M) can now be copied as text (and pasted as
  text or directly in a spreadsheet program). Does not apply for the
  WRTC version that has a different multiplier rule.

- Bugfix (Task #284). Your own call incorrectly counted one HQ if
  such an exchange was entered. Tnx TM0HQ, N6TV.

- IOTA : Even if IOTA.DAT is not installed, IOTA references that are
  syntaxically valid are now taken into account for points credits and
  are written in the Cabrillo file. Tnx SM3CER.

- IOTA : Mult wnd (Alt-M) can now be copied as text (and pasted as text
  or directly in a spreadsheet program). Tnx G3TXF.

- Bugfix : DX cluster (Alt-A) and radio wnds : If the SP or the LP
  value of the spot was 0°, heading was not displayed. Tnx SM5AJV/SE5E.

- Bugfix (Task #282) : Under some circumstances the QSO number
  displayed in the report for possible bad exchanges was wrong.
  Tnx DF1DX.

- The check logs tools reports are now adapted to the mixed contests.

- Enhanced replies to the inventory command (INV) with time master and
  bridgehead indicators (M vs m and B vs b).

- BRIDGEHEAD/NOBRIDGEHEAD text commands added.

- IARU HF : "BA" added to the exception list of the cut numbers
  translation, despite this abbreviation is not listed as the official
  one of the E7HQ Society. Cf http://www.iaru.org/iaru-soc.html
  Tnx UA6AA and many others.

4.5.2 (Jul 3, 2010)

- Fixed a problem with registration in some versions.

4.5.1 (Jun 27, 2010)

- Bugfix : MP3 information files dialog could lead to a crash if no
  mp3 file were present in the current log directory.

- Bugfix : ARI Sezioni - RTTY : Only valid 4 digits codes can be now
  grabbed from the RTTY wnd as an exchange. Tnx IK0CHU.

4.5.0 (Jun 5, 2010)

- CAUTION: New network protocol version 1.24 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

  These network modifications only affect the use of Win-Test in a
  WAN environment, and require wtTunnel 1.12 (to be released) to
  be effective.

- Workaround: YCCC SO2R Box outputs were not working as expected.
  At this time, AUX1 and AUX3 are assigned to Radio1, and AUX2 and
  AUX4 to Radio2. This will be customizable in the future.

- Added a Extraction Feature in Contest Recorder (right-click in
  the Contest Recorder Window, and chose the "Extract and Save QSO"
  menu).

- Contest Recorder: the "rotate file" option were disabling the
  AutoStart one. Fixed. Thanks IK2JUB.

- New microHam device "USB micro2R" supported. Tks OM7ZZ.

- Radio Wnd and DX Cluster Wnd (Alt-A) : New leading indicator (#)
  introduced to tag spots coming from a CW Skimmer (aka the spotter
  callsign ends with "-#").

- Bugfix : IC-7600 : Split was broken. Tnx N3MX, I2WIJ.

- CW cut numbers translation : New option in Tools / Data entry to
  disable the automatic translation. Note that this translation is
  performed on a contest and worked station contextual basis. The
  equivalent text commands are CUTON and CUTOFF. Do not use CUT/NOCUT
  that are reserved for CW cut numbers generation ! Tnx N6TV.

- Bugfix : In M/* configuration, and under certain circumstances, the
  mp3 files list associated with a station in the MP3 file information
  dialog could be wrong.

- ARRL DX : CW cut numbers are translated for DXCC stations worked
  from the US/VE side.

- MP3 setup : Only the CBR codecs are now displayed in the setup
  dialogs. The usage of the ABR codecs (most of the LAME ACM ones) is
  too erratic to be trusted in. Tnx N6TV.

- Text commands : MP3SETUP and SCRIPTS commands added. Tnx N6TV.

- Scripts manager dlg : The delete key now acts like clicking on the
  Delete button.

- Bugfix : REF HF : Cut numbers were translated for TK stations (2A).
  Tnx F5CQ.

- Bugfix : Additional CW messages (Alt-C) : When no log is opened, the
  function keys are now disabled.

- EXPERIMENTAL : New "Always On Top" option in the Options / Windows
  menu. Can also be (re)set with text commands. Tnx N6TV.

- Bugfix : Recorder wnd : Under certain circumstances, the buttons
  tooltips were not always displayed.

- Bugfix : HA DX contest : When working contest from the HA side, cut
  numbers where always translated, whereas it had to be so for non-HA
  callsigns only. Tnx HA3LN.

4.4.0 (Jan 17, 2010)

- Bugfix (#255): K1EL WinKey USB CW timing becomes very poor
  (Farnsworth style) when PTT delay is default 50 ms. This was caused
  by too low hardcoded value (80ms) of the PTT Tail delay. This delay
  is now configurable in the Winkey Properties Dialog Box.
  Tks F5JSD, SM5AJV, KL7RA and N6TV.

- Added some new features of the WK2 (WKUSB) for the PTT Tail.
  Tks F5JSD, K1EL.

- OmniRig supported as an alternative to the WT build-in Radio Control.
  Right-click on the Radio Window then choose "OmniRig Settings" in
  order to properly configure OmniRig for your Radio.

- Bugfix (#253): Input Wave Device was not properly selected in the
  Contest Recorder Module. Tks N6TV, NR5M.

- IC-703 rig added.

- First attempt in OTRSP (Open Two Radio Switching Protocol) protocol
  support. Tested with the YCCC SO2R Box but not in real conditions.
  Tks K1XM.

- MP3 files information dialog : Under certain circumstances, the
  displayed stop time and duration of the selected file were wrong.
  Tnx N6TV.

- Log output : Progress bar implemented. Tnx TF3CW.

- Edit / Move in my log menu item has now text commands equivalents :

  MOVEINMYLOG (or SCROLLMYLOG) and NOMOVEINMYLOG (or NOSCROLLMYLOG)

  Tnx 5B4WN.

- Rate wnd (Alt-R) : Two methods are now available to display the
  elapsed time since the last band changes. Tnx F1NGP and TK5EP.

- Bugfix (#271) : Packet window (Alt-T) was losing focus when the gab
  window was automatically closed. Tnx DL6RAI.

- Bugfix (#272) : Under certain circumstances, pattern checking flags
  were not updated if an entered callsign was modified. Tnx DL6RAI.

- DARC 10 : Leading zeros addition for serial received was broken.
  Tnx DK1AX.

- MRU (Most Recently Used) file list added in the File menu.

- IC-7600 rig added.

- ICOM rigs : Radio list rearranged alphabetically in the Interface
  Setup dialog.

- Bugfix : RTTY wnds : The invert function was also inverting the
  character next to the selection.

- RTTY wnds : Mirror zone enlarged to allow 4-figures serials.

- Bugfix : MP3 files recorded in 2009 couldn't be listened to anymore
  in Win-Test in 2010 ;-) ! Tnx DL6RAI.

- RTTY wnds : Callsigns found in the database or in the log are now
  displayed in bold.

- RTTY wnds : Colors management added.

- Grid Squares wnd : It can now be enlarged to the entire world.
  Tnx F8BBL.

- Grid Squares wnd : New options in the contextual menu to display
  fields only, and to center the map on a specific point more
  easily (it requires the map is NOT centered on the Home QTH in
  the properties dialog).

- Grid Squares wnd : The resolution (low or high) chosen in the
  properties dialog wasn't properly saved.

- Bugfix : Stew Perry : Under certain circumstances, an overflow
  error could happen in distance calculations for Q inside the same
  GridSquare as the entrant. Tnx VE3TA.

- CQWW WPX Contests (Task #269) : Various updates to comply with
  the new rules introduced in 2010. Tnx K5ZD, W0YK.

- ARRL Contests : Default Off-time period set to 30 mins. Tnx CX6VM
  and DL6RAI.

- New "-n" or "--noautoload" switch allowed in the command line to
  disable the autoload log feature. Tnx N6TV (The only Win-Test user
  who runs it from the command line ;-) ).

- Startup time reduced.

- Bugfix (Task #270) : ARRL 10 : When running the contest from the
  DX side, the serial sent was not editable. Tnx CX6VM.

- Bugfix : RTTY wnds : Left-click to activate (and right-click to open
  the contextual menu) in the text area were broken. Also, the
  possibility to Ctrl-Drag these windows has been added.

- Bugfix : ARI 40/80 contest in RTTY : The provinces can now be
  grabbed in the RTTY wnd. Also fixed for the ARI International
  Contest. Tnx IK0CHU.

- CSV and Text exports : HF logs can now export distance and heading.
  CAUTION : To ensure consistency with the VHF logs exports (and many
  geographical processing softwares or online apps), the longitude
  is now positive for East, and negative for West.

- Bugfix : The Inventory and Score broadcast network frames could
  have bad data. Tnx SV3SJ/F5VIH.

- Tools / Check log / Callsigns syntax check added. Uses the pattern
  callsigns rules file (callsign.pat).

- LUA : wtArg can now be used to get the optional argument set in the
  Script Manager or in a #SCRIPT(argument) call. To ensure
  compatibility, wtArgument remains usable.

- Bugfix : Under some circumstances, some key assignments to scripts
  were not working properly. Tnx DJ0ZY.

- Script key assignment dialog : If no key is assigned, the argument
  field is now automatically cleared and disabled.

- Bugfix : After opening a non-empty log, the first PgUp press was
  not updating the child windows.

- Lua : New API to get the type and the manufactuer of the radios :
  wtRadio*:GetTypeId() and wtRadio*:GetManufacturerId().

  Reminder : wtRadio* applies to wtRadio, wtRadioInactive,
  wtRadioPrimary, wtRadioSecondary, wtRadio1 or wtRadio2.

  New Lua WT constants are introduced for this purpose.

  A new directory on our download repository has been created to
  gather the API and the constants lists :

  http://download.win-test.com/v4/lua/

- REF 160 : As non-domestic stations can send non-numeric exchanges
  the CW cut numbers translation is now disabled. Tnx F5IN.

4.3.0 (Nov 23, 2009)

- Italian translation added. Tks IV3IYH!

- Contest Recorder (#253): USB Voice Codec was not detected due to a
  trailing space in the Codec Name. Fixed. Tks N6TV.

- Bugfix: playing back MP3s recorded on different stations was broken.
  Tks FY5KE.

- Search for Possible Bad Exchanges against bad formated serial
  number implemented. Tks N6TV.

- Added some basic checks for ARRL SS in the "Search for Possible
  Bad Exchanges" tool. Tks N6TV.

- Bugfix (#182): Wrong QSX Frequency in Self-generated Spots.
  Tks K1GQ.

- Bugfix (#262): CQ Repeat doesn't stop for Secondary Radio.
  Tks DJ0ZY.

- Bugfix (#259): Pressing Alt-1 in Secondary Radio window moves QSO
  to wrong band. Alt-1/2/3/... are now active only with the Primary
  radio and when the Partner Wnd is open. Tks N6TV.

- Bugfix (#251): NA Sprint - LOCATION record not written to Cabrillo
  file header. Done also for IARU HF, NAQP and NCCC Sprints.
  Tks N6TV.

- Bugfix (#243): WPX contest now requires LOCATION in Cabrillo. Done
  also for CQWW even if it doesn't seem required yet.
  Tks N6TV.

- The '<' and '>' keys are now interpreted by the Secondary Radio
  Window as well, as soon as the SHIFT key is not used for binding
  to the Secondary Radio Window (task #216). Tks N6TV.

- WAE : When using the keyboard mode in the QTC transmitting and
  receiving dialogs, the Enter key was mis-interpreted. And now,
  in CW, the "what you type" field is also updated. Tnx DL6RAI
  and DJ4MZ.

- Lua : New API to play the additional CW/RTTY messages (Alt-C set)

  wtKeyer:PlayAdditionalMsg(AdditionalMsgIndex)

  AdditionalMsgIndex is the index of the Alt-C messages set (1 to
  12). Other are ignored.

  This API is useful when these messages contains variables. If
  not, you can still use wtKeyer:Play("$MSGx").

- Lua : New API introduced to get various interesting directories
  paths :

  wtApp:GetLogPath()         Current log directory path
  wtApp:GetAppPath()         Win-Test installation directory path
  wtApp:GetCfgPath()         \cfg directory path
  wtApp:GetCtyPath()         \countryFiles directory path
  wtApp:GetDatabasePath()    \databases directory path
  wtApp:GetOpPath()          \ops directory path
  wtApp:GetScriptPath()      \scripts directory path
  wtApp:GetExtraPath()       \extras directory path

- WAE : Transmit and Receive QTC windows : Scripts are now allowed in
  the predefined CW/RTTY messages (use the #SCRIPT notation as
  usual). Tnx DL6RAI.

- Ukranian DX contest : Rules 2009 now accept single mode entries
  for DX : Cabrillo file output updated. Tnx F5IN.

- Bugfix : Ukranian DX contest and RDXC : Cut numbers were translated
  even for Oblasts. Tnx F5IN and RK1AA.

- UFT HF : Under some circumstances, the received report was not
  correctly translated with cut numbers. Tnx F5IN.

- CQWW M/S : The 10-minute mult timer in the status window (Alt-J)
  was broken. Tnx FY5KE.

4.2.0 (Oct 18, 2009)

- Bugfix: Conversion of binary file containing QTC from v3 to v4.
  Tks DJ4MZ.

- Better support of Win7 and Wine/Linux.

- Bugfix (#258): Failure of swap radio key to switch rx focus for the
  MK2R+ as long as one not manually changed the rx focus to stereo or
  transmitted anything in CW. Tks GW3NJW, OH1JT, OM7ZZ, W4TV.

- Cosmetic: avoid rx focus leds flickering when switching tx focus.
  Tks OM7ZZ.

- Bugfix (#187): Ctrl-Shift-Tab doesn't appear to toggle RUN / S&P in
  Secondary radio window. Tks N6TV, GW3NJW.

- Bugfix : K3 serial port default setup modified : The number of
  stop bits was wrong - It is now set to one stop bit, according
  to the K3 users manual. Tnx N6TV.

- ON Winter and Spring contests : Sections list updated. Tnx F5IN
  and ON5GQ.

- Bugfix (#257) : CQWW DX RTTY : Cabrillo template modified to match
  the specs. Tnx N6TV.

- Bugfix : CQWW DX RTTY : Allowed band changes modified to 8 in MS
  and M2 categories (rules 2009). Tnx F5JY.

- Bugfix (#164): TI5/NP3D is now parsed as TI. Tnx JE2UFF/W2UFF.

- CTY files : 4U30VIC now considered as 4U1V in an appropriate way.
  Tnx DL6LAU.

- Bugfix : After reloading a WAE log, the QTC count in the Summary
  window was wrong. Tnx DK1AX.

- Scripting : wtQso:GetModeId() and wtKeyer:GrabHighlightedCallsign()
  function added. Note that wtKeyer:GrabHighlightedCallsign() works
  only in RTTY, and relies on the INSERT key option set in the RTTY
  setup dialog.

- New option in the Clock wnd to "wizz" this window a la MSN at
  rounded hours, to draw attention of the op (useful in multi-op
  configurations).

- New feature in Tools / Scripts manager... : Allows to edit, create,
  delete or rename scripts. It's also used to assign a key and/or an
  argument to a script (its value will be available in the wtArgument
  global variable).

- Scripts called by an assigned key can return +1 to be called again
  *after* the WT key processing ooccured. A new API
  wtApp:IsPostKeyProcess() is introduced to distinguish the "pre"-
  process from the "post"-process.

  Example :

  RunSPSwitch.wts  (assigned to Ctrl-Tab) :

  if (wtApp:IsPostKeyProcess()) then
    if (wtQso:IsOperatingModeRun()) then
      wtApp:SetWindowColor(-1, 0, 165, 165);
    else
      wtApp:SetWindowColor(-1, 128, 128, 128);
    end;
  else
    return 1; -- Triggers a post key process call
  end;

  Note : This feature works only for users scripts called with an
  assigned key (and *not* with embedded overriden scripts).

- Scripts can now be called from a CW or a RTTY message. You must use
  the #SCRIPTNAME(ARGUMENT) notation. The argument (and parenthesis)
  are optional. The script will be called synchroneously, but is
  executed in the main thread, meaning that it is not blocking the
  CW/RTTY stream.

- New feature in Options / Script Editor configuration : Allows to use
  any external text editor to edit scripts. The default text editor is
  a custom package of SciTE (Scintilla Text Editor - free and open
  source) available on our repository

  http://download.win-test.com/utils/SciTE_for_Win-Test.zip

  Unzip the package and move the entire SciTE folder in the Win-Test
  installation directory.

- YO DX Contest : Rules 2009 : In mixed mode, a station can be worked
  in both modes. Tnx N2YO.

- Tools / Check log for possible bad exchanges : When the contest do
  not use serial numbers, use the QSO index in the report remarks.
  Tnx F1HAR @ TM0HQ.

- Keys redefinitions : The Pause and Scroll-Lock keys can now be used.
  Be warned that Ctrl-Scroll-Lock and Ctrl-Pause (that are considered
  as "identical" by the system) are used by Windows to cancel dialogs.
  Thus, it is advisable to not use them for key redefinition.

4.1.0 (Aug 6, 2009)

- IOTA contest: "Search for possible bad exchanges" (tools menu)
  implemented.

- Bugfix: The displayed azimuth in the Rotator Window could be wrong
  in the "Stacks" and "Rotors" tabs.

- Rotator Azimuth orders are now based on the locator instead of the
  DXCC on 50 MHz and above. On 50 MHz and 70 MHz, if the locator field
  is empty in the log, then the azimuth is computed against the DXCC
  prefix.

- Bugfix : EUHF : Statistics window (Ctrl-F9) limited to one day.
  Tnx F5VIH/SV3SJ.

- New text commands RUNSP/NORUNSP and RUNSPON/RUNSPOFF to enable or not
  the RUN/S&P switching. Tnx N6TV.

- New contest files : You can now customize the file name and sub dir
  formats. See Options / Log / New contest files properties...
  Tnx N6TV.

- IOTA contest : Default IOTA reference is now guessed, according to
  the new CTY_IOTA.DAT file (must be in the countryFiles directory).
  This file is based on DXCC countries, callsign prefixes, call areas
  and oblasts.

- IOTA contest : Check mult wnd (F10) : IOTA references are now
  autocompleted for check during QSO entry.

- Bugfix : IOTA contest : When an invalid IOTA was entered, clearing
  the field afterwards wasn't clearing the '?' flag.

- New File menu items to explore more easily several WT-related
  directories. Tnx F5VIH/SV3SJ and N6TV.

- DX Window (Alt-A) : Spot can be now passed to the secondary radio or
  the non-active radio. Tnx DL8WAA.

- Bugfixes in Contest Recorder:
	- Infinite loop in MP3 file rotations. Tks DD5FZ.
	- Memory Leak using LAME encoder.
	- MP3 Codec enumeration in the player. WT was not always detecting
	  the appropriate Codec.
	- Playback with Windows VISTA. Note that the LAME Codec is
	  an Encoder Codec only.

- M2/Orion rotators added in wtRotators. Tks IK0HBN.

- The RRTC Cabrillo files are now following the version 3 specs.
  And the contest name is modified as "OZCHR". Tnx F5VIH/SV3SJ.

- CW and RTTY msgs enlarged to 120 characters.

- Extra information files : Multiple spaces or tabs can now separate
  the callsign from the data. Tnx G0ORH.

- New File dialog : Ensures the validity of the entered file name.
  Tnx DJ7MGQ.

- ESM : S&P : When the entered callsign is a dupe, WT now blocks call.
  To override this behaviour, use F4 to call and F2 to send exchange
  (by default). Tnx GW3NJW.

- VHF+ contests : Mode is now displayed in the main log wnd if the
  contest has been set to handle several modes (Mixed or All modes).
  Tnx DK2ZF and DL5NAH.

- Bugfix : When radios were swapped (*), the ESM QSO status was
  somewhat messy.

- Bugfix : For some contests, the letters for cut numbers were
  inappropriately translated.

- Bugfix : After a WT v3 file conversion, the main window caption was
  not updated.

- Bugfix : MP3 files information : The file date was off by one
  month. Tnx F5VIH/SV3SJ.

- Bugfix : Cabrillo Import : The station name for all worked QSO was
  CABRILLO. Now, it uses the name entered in the Contest Settings
  dialog. Tnx F5VIH/SV3SJ.

- Bugfix : Callsign text color wasn't reset after F11 or empty
  callsign if the callsign check wasn't automatic. Tnx DJ0ZY.

- Bugfix : Delete QSO : Several structures inconstancies fixed when
  a Q was deleted in the middle of the log.

- Bugfix: In REG1TEST exports (European Standard File for V/UHF
  Contests), QSO logged in mode different than CW or SSB was not well
  formatted. Tks DL5NAH.

- Bugfix : Options / Log / Colors...  menu was broken. Tnx F5LIW.

- Bugfix : Check Country wnd (F10) : Sun status bars now display
  "NO DATA" when SS and SR are not computed (JW, JX etc.). Tnx DJ0ZY.

- Bugfix (Task #245) : Network advanced settings : The Bridgehead
  setting was not saved. Tnx KL7RA and N6TV.

- Bugfix : Opening a .wtb file in the command line, by drag'n'drop or
  a double-click on it was starting an infinite loop. Tnx N6TV.

4.0.1 (June 30, 2009)

- Bugfix: Options / Toolbar setting was ignored on startup. Tnx N6TV.
- Bugfix: ESM was broken. Tnx F1HAR.
- Bugfix: Registration Key was broken.

4.0.0 (jun 26, 2009)

First release of Win-Test version 4

Minimum requirements : WinXP (2k not tested but may mork - feedbacks
welcome). PIII 500 MHz - 64 MB RAM - 800 x 600 screen res.

Summary of the new features:

- Rotators Controls

- Integrated MP3 contest recorder and player: Use the Options / MP3
  configuration to set the audo device that will record and play the
  file, the various sampling and bit rate settings. You can also set
  a maximum filesize. Over this limit, additional files will be
  automatically created. To start recording click on the record button
  of the window (a blinking red square will be displayed in the clock
  window too). Once the contest is over, click on the record button
  again to stop recording. Now, you can browse your log with usual
  arrow keys and to listen to a specific Q but clicking the Play button
  or use the AltGr-Enter combination (some keyboard do not have an
  AltGr key, so use Ctrl+Alt instead). You can also go back and forward
  with the adapted buttons or use AltGr-Left and Right. To pause/play,
  you can use the AltGr-Space combination.

- ESM (Enter Sends Message): Enabled/Disabled by the Tools/Data entry/
  ESM Enabled menu. You can also use the ESM/NOESM or ESMON/ESMOFF
  text commmands. It relies on the following messages assignation :

  F1 : CQ
  F2 : Sent report
  F4 : Mycall
  F5 : Logged callsign ($LOGGED)
  F7 : ? (or "Again ?" in phone)
  INSERT : Callsign + sent report
  PLUS : TU + enter Q

  When the ESM is enabled, as the return key *can't* be used anymore
  to log silently a QSO, the key combination Ctrl+Plus has been
  introduced and added for this purpose.

- Variable speed for the integrated voice keyer : An exclusive Win-Test
  feature! You can play your voice files at a different speed (between
  -20% and +70%) from the original recording speed. Record your voice
  files at normal speed, and use Alt-F9/F10 (as in CW mode) to play
  them at a different speed. The speed in displayed at the bottom of
  the (Rate) Alt-R window.

- On the fly callsign pattern check based on the K1TTT callsign.pat
  file (over 400 rules applied today). Use the Tools / Data entry /
  Callsign check menu option. You are encouraged to report the author
  any mistakes or improvements of this file (k1ttt@arrl.net). The file
  is located in the cfg directory (see below).

- Improved F10 window with graphical indication of the sun status on
  both sides of the QSO.

- Keyboard mode (Alt-K) enhanced. The backspace is not supported yet
  and replaced by "E E " like you do when you use a regular key.

- Data (.wt4) and notes (.not) files can be transferred thru the WT
  network without needing any file or directory sharing. Very
  convenient to gather all logs in a multi-stations environment once
  the contest is over. Use the Tools / Download thru the network...
  menu.

- Enhanced compatibility with Vista and Seven (Auxiliary and ini files
  are now stored in directories these OS accept with no additional
  rights:

  Windows XP : Documents and Settings\All users\Application Data\
               Win-Test\
  Windows Vista : ProgramData\Win-Test\

  Note that these directories may be hidden by Windows Explorer.
  Check the Folders Options of Windows Explorer.

  Several sub-directories are created and used by Win-Test. Their
  names are self-explanatory.

3.27.0 (Jun 9, 2009)

- Log entry : In CW, and when applicable (depending on the contest and
  station worked), letters for cut numbers are translated. Only works
  for newly entered QSOs. Tnx N6TV.

- New option in the bandmap properties to randomize a small offset
  (-100 Hz/0/+100 Hz) of the transmitting frequency of a grabbed spot.
  Works only in CW mode. Tnx F5VIH/SV3SJ.

- Several typos fixed. Tnx DL6RAI.

3.26.0 (Mar 26, 2009)

- Partner window : Delete item added to the contextual menu. You can
  also use a Ctrl-Dbl-Click a la Bandmap. No confirmation asked.

- RTTY windows : The middle mouse button acts the same as the left
  mouse button in the stream display, except that selection (if any)
  is stacked in the Partner window.

- RTTY and CW : New variables.

  $CURRENT (or $CURRENTCALL) : Sends the callsign of the current QSO
  *despite* the presence of a $CR (always executed on message keypress)
  later in the message.

  $NEXT (or $NEXTCALL) : Sends the callsign of the next QSO line when
  a $CR is included in the message.

  $PREV (or $PREVCALL) : Sends the callsign of the previous QSO line.

  $GRABPARTNER : Grabs the first callsign from the Partner window and
  insert it in the callsign field. The exchange guessing is performed
  (or not) according to the manual callsign entering setting (Tools /
  Data entry / Exchange guessing).

  To summarize, you can now enter a QSO (with correction or not),
  grab another callsign from the Partner window and send his report
  in one keystroke, by using :

  $CORRECT TU $CR NOW $GRABPARTNER $NEXT $F2 (w/correction)

  or

  $CURRENT TU $CR NOW $GRABPARTNER $NEXT $F2 (full call)

  ($F2 is supposed to be the sent report)

  If you want to manually grab a callsign from the Partner window
  you can use :

  $PREV TU NOW $LOGGED $F2    ($F2 is supposed to be the sent report)

  1/ Use the enter key to silently enter the current Q
  2/ Grab the next callsign from the Partner wnd (dbl-click or Alt-n)
  3/ Send the above message

- Custom variables support added. Mostly designed for the DXPed mode,
  this feature allows to create custom variables and set the value
  very quickly. Example : $REGION or $UP for a split up value.

  Use the Options / CW (or RTTY) / Custom variables... menu to set
  the names and the value of these variables to be used in your CW or
  RTTY messages. You can also use the VARIABLES text command.

  You can also easily set a variable value by entering its name in
  the callsign and "Enter". WARNING : Don't chose a variable name
  that is already used or it won't work...

  Tnx K5AC @ K5D.

- Yaesu FT-450 supported. Tnx F8IJV, F6DEX.

- Yaesu FT-950 supported. Tnx EA8AY.

- ARRL DX and ARRL 10 : KH6 and KL7 stations are now exclusively
  identified as being not located in HI and AK by the CTY*.DAT file.
  Tnx AD1C and G4MJS.

- CW and RTTY keyers : $FREQnn (like $FREQ160, $FREQ80 etc.) variables
  added. Sends the freq of the primary radio of the first networked
  station found on this band with the following priority : R, R+, M,
  and M+. In addition, in CW, if the frequency is round, no decimal
  point (or kHz) are send. If not, the decimal point is replaced by
  an R. Ex 14021.0 is sent as 14021 and 14021.1 is sent as 14021R1.

- Status Window (Alt-J) : To improve consistency across the software,
  new contextual menu item to Pass a frequency to the Sub VFO of the
  active radio (if the radio permits). An Alt-Dbl-Click on the
  frequency works too, like in the bandmaps windows.

- Sked Window (Alt-B) : To improve consistency across the software,
  an Alt-Dbl-Click on a sked passes its frequency to the Sub VFO of
  the active radio (if the radio permits), like in the bandmaps.
  windows.

- CW / RTTY : The leading zeros setting is now different for each
  mode, but the text commands (LZ/NOLZ etc.) remain the same.
  Tnx N6TV, KR7X.

- RTTY setup : New option to favor or not auto-highlighted mults
  when using the Ins key. Tnx TK5EP.

- RTTY wnds : New option in the contextual menu to "invert"
  (Letters / Figures) the selection. Tnx DL6RAI.

- RTTY wnds : The 599nn, 599nnn and 599nnnn reports are now correctly
  interpreted and the 599 part is stripped. Tnx DL4NER.

- PACC contest new rules : Non-PA stations are no more restricted to
  mixed mode. The Cabrillo output has been consequently updated.
  Tnx F5IN.

- Bugfix : Under certain conditions the CLEARLOGNOW text command
  could lead to a crash. Tnx DL6RAI @ DQ4W.

- Bugfix : UBA Spring contests : Sections were missing in the
  section list displayed in the Alt-Z wnd. Tnx F5IN, ON7TK.

- Bugfix : ARRL Contests : The content of the ARRL-SECTION or LOCATION
  field of the Cabrillo output file can be modified to comply with
  the ARRL/RAC sections list. Tnx W2NRA.

- Bugfix : (Task #241) Minimum offtime for CQWW 160 is now 30 min.
  Tnx K1DG.

- Bugfix : NAQP and NA Sprint RTTY : The $MYNAME wasn't working in
  this mode. Tnx YV5TX.

- Bugfix : (Task #239) Packet monitor wnd (Alt-O) : Scrollbar issues
  when its content is over 65535 lines. So, this wnd is now limited
  to the last 65535 lines. Tnx G4MJS.

- Bugfix : CQWW WPX now appears in the current month contest if we
  are in february (because of the RTTY leg). Tnx DL6RAI.

3.25.1 (Feb 13, 2009)

- ALT+F3 and K3: inverted frequencies into an ALT-F3 Spot. Tks W9ZRX.

3.25.0 (Feb 13, 2009)

- CQWW WPX RTTY : Rules 2009 : The band-change limit for M/S is
  increased to 8 per hour.

- DX Cluster Wnd (Alt-A) : New option to display only the op-entered
  spots. Tnx YL2GD.

- CQWW 160 : Zones wnd : Copy as text enabled. Tnx G3TXF.

- CQWW WPX : RTTY M/S => Numbering sequence for whole log for M/S and
  numbering per band for the other M/? categories.

- Bugfix : Stats wnd (Ctrl-F9) : If the contest spread over two days
  (CQWW 160 rules 2009 for example), it was impossible to export
  a target file over 48 hrs. Tnx OK1VWK @ OL7R.

- Bugfix : Stats wnd (Ctrl-F9) : If the contest spread over two days
  (CQWW 160 rules 2009 for example), some drawings were broken.

- Bugfix : Task #211 : NA Sprint : Network protocol was broken.
  Tnx N6TV.

- Bugfix : Task #236 : FOC Marathon : The exchange filling function
  failed after a band change. Tnx N6TV.

- Bugfix : Task #233 : Rate Wnd (Alt-R) : CQWW 160 : Under certain
  circumstances the pts per QSO calculation was wrong.
  Tnx DL1ELY, DL6RAI.

- Bugfix : Task #230 : Options / Windows / Default layout... was
  crashing Win-Test. Tnx N6TV.

- Bugfix : NCCC Sprint : Canadian Maritime "provinces" are now
  using the MAR identifiers, like for the NA Sprint. N6TV.

- Bugfix: Task #228: wrong QSX frequency in spots with K3. Also apply
  to Kenwood Radios. Tks W9ZRX, N6TV.

3.24.0 (Jan 15, 2009)

- CQWW WPX : New rules 2009 : In M/S category the trailing 0/1
  indicator in the Cabrillo file now indicates if a callsign has been
  worked by a RUN or a MULT station.

- RAEM Contest implemented. Tnx F5IN.

- Keyboard mode : New options in Options / CW and Option / RTTY to
  enable or not keys remapping while in keyboard mode. Cf Task #172.
  Tnx N6TV.

- Contest settings dlg : The exchange help message box pop-ups if it
  is required and empty. Tnx W7UPF, N6TV.

- CQWW 160 : Win-Test is now compliant with the new rules 2009.

- Sked window (Alt-B) : You can send the sked freq in the sub VFO if
  applicable. Tnx TM2Y.

- CTY files : The "virtual" 0VER entity (if any) is ignored. The VER*
  callsigns too.

- WAE messages : $LOGGEDCALL (or $LOGGED) can now be used in these
  messages. Tnx DK4WA.

- Clock wnd : The RUN/S&P indicator is displayed only if this switch
  is enabled (Tools / Data entry menu). Tnx F1HAR @ FY5KE.

- Statistics : All text reports are now formatted with | separators
  instead of ! chars. Tnx N6TV.

- Bugfix : NAQP and SCCC Sprint : VO1/VO2 province is now NL instead
  of NF. Tnx NX5M.

- Bugfix : Rate wnd (Alt-R) : Under some circumstances, the
  calculations were wrong for monoband contests. Tnx AC0W.

- Bugfix : ARRL 10m : US/VE multipliers weren't correctly displayed
  in the Check Multipliers wnd (F10). Tnx CX6VM.

- Bugfix : Task #221 : ARRL SS Cabrillo file import failed. Tnx N6TV.

- Bugfix : Task #171

- Bugfix : ARRL 160 : ADIF file export now uses the ARRL_SECT field.
  Also fixed for the ARRL SS, ARRL FD and the ARRL 10 uses the
  STATE or VE_PROV field when applicable. Tnx AD1C, W1EQ.

- Bugfix : Task #222 : M/S log import now correctly assigns the RUN
  and MULT flags following the new Cabrillo implementation.
  Tnx I4UFH, N6TV.

- Bugfix : Task #218 : The exchange help in the contest configuration
  now works for the ARRL SS. Tnx N6TV.

- Bugfix : ARRL SS : Serial sent is now editable (Edit / Serial sent)
  Tnx N6TV.

- Bugfix : WAE RTTY : QTC transmission : A QSO with a 000 as serial
  number was interrupting the transmission of the series. Tnx DK4WA.

- Bugfix : MK setup dlg : Under some circumstances, chosen options
  were deleted when setting the router path. Tnx FY5KE.

- Bugfix: Task #214 - QSX frequency (if any) was missing in ALT-F3 when
  spotting the previously logged QSO. Tks DL4NER, NQ4I, W9ZRX, N6TV.

- Bugfix: Task #215 (Clicking on QSX spots (split) doesn't work right
  with Yaesu radios) - fix to be tested.

- Bugfix : Some AltGr (Alt+Crtl) shortcuts were also lauching either
  Alt or Ctrl ones. Fixed.

3.23.0 (Oct 22, 2008)

- Spanish language is now included. Thanks EB2CYQ for this excellent
  job!

- CQWW RTTY : ADIF export : Task #213 - US State (or VE province) is
  now exported when applicable. Tnx N6TV.

- Radios : Omni VII process reviewed and fixed. Note that the TenTec
  protocol has some limitations Win-Test can't circumvent. For example
  Win-Test can't know which VFO is transmitting.

  A big "thanks" to F5FLN (owner of RFPA/RFHam http://www.rfpa.com/ and
  http://www.rfham.com/) who lent us an Omni VII for testing.

  Tnx F5LVL.

- RTTY keyboard mode (Alt-K) : The Ctrl-M and Ctrl-Enter combinations
  now send linefeeds. Tnx DJ4MZ, N6TV.

3.22.0 (Sep 16, 2008)

- CAUTION: New network protocol version 1.23 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- Voice Keyer module rewritten.

- CQWW M/S Category : The Cabrillo file format now uses a different
  indicator whether the QSO has been worked with a RUN or a MULT
  station. Tnx K1EA, F6BEE.

- RDA Contest : Russian stations : DXCC countries are now counted
  per band. Tnx UA1ACC.

- RDA Contest : R1FJ and R1MV are now considered as Russian Stations
  and their RDA is processed as valid. Tnx G3TXF, OR2A and others.

- The bridgehead concept has been revised to decrease the required
  bandwidth for log synchronization across a WAN. This new
  implementation is only effective when used with the updated
  WtTunnel v1.10. The updated WtTunnel suite will be available only
  for the next IARU HF contest, and, as usual, its use will be
  restricted to the HQ stations.

- Radio wnds : Ctrl-Up/Down are now usable with all sorting options.

- WAEDC : DX side : QTC-in-stock count is now displayed in the Clock
  wnd. Tnx K5KG.

- WAEDC : Radio wnds : New option in the list view to display the
  "potential QTCers". Tnx IZ3EYZ.

- RRTC (Russian Radiosport Team Championship) added. Tnx RA3AUU.

- New text commands added :
  - AUTORELOAD: Equ. to Options / Load contest at startup / Enabled
  - NOAUTORELOAD: Equ. to Options / Load contest at startup / Disabled

- Bugfix : WAE : Radio wnds : List view : The "potential QTC" option
  was not working correctly. Tnx IZ3EYZ.

- Bugfix : Radio wnds : Bandmap view : Scale 1:8 menu item was not
  working. Tnx TM1W.

- Bugfix : ARRL FD. Some ARRL sections weren't considered :
  AK, PAC, PR and VI. Tnx VE2FU, N6TV

- Bugfix : ARRL FD. QSO between home stations are now tagged as invalid
  and count as 0 pts. Tnx VE2FU.

- Bugfix : Helvetia VHF/UHF/Microwave Contest : Locator partial check
  is now working the same way as the other VHF+ contests. Tnx HB9CZF.

- Bugfix: Split Mode with IC7700. Tks K3LR.

3.21.0 (June 23, 2008)

- CAUTION: New network protocol version 1.22 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- Operators management : Reserved for Multi-Ops : When an operator logs
  in, Win-Test now automatically tries to run an executable (.exe ,
  .bat or .com) named op_"callsign" which must be located in the
  Win-Test installation directory. For example, if DL6RAI logs in, WT
  will try to run op_dl6rai.exe (or .bat or .com), if this file exists.
  If the callsign includes a "/" character, it will be replaced by an
  underscore ("_"). This feature may be useful to automate various
  actions. Tnx DK4YJ for giving the idea.

- NA RTTY Sprint : The special "legal dupe" rule being abandonned for
  this mode, Win-Test is now processing dupes the same way as for
  the SSB and CW legs. Tnx W0YK.

- Win-Test now manages a lock mechanism to prevent several program
  instances running on the same machine to open the same log.
  Tnx N6TV.

- CW and RTTY messages dlg : Keystrokes are now automatically
  upper-cased while entering.

- Partial QTH locator search enhanced (Shift - F10) :
  - Only applies to the VHF+ contests
  - Partial locator can be entered in the callsign field
    - or -
  - Partial locator can be entered in the locator field
    with four characters at least

- Automatic CQ repeat : New options in the setting dialog to use
  this function for functions keys different from F1, depending
  on the mode. Can be useful, for example, in Phone when using
  CQ messages in different languages.

- Automatic CQ repeat : The repeat interval can be set even if
  the function is disabled.

- CW Autosend : Setting dlg slightly modified to split the
  Enable / Disable toggle from the minimum entered chars setting.

- CW Autosend : The triggering chars count now starts after the
  first '/' if there is one in the callsign. Tnx ES5TV.

- Shift and NumLock bindings settings are now ignored when using an
  operating technique different from the Advanced SO2R. Tnx SM5AJV.

- New option in the help menu to display text command tips for
  menu items. The equivalent text commands for this option are
  TXTCMDTIP / NOTXTCMDTIP, or TEXTCMDTIP / NOTEXTCMDTIP. Tnx N6TV.

- CW/RTTY Messages options : New option to ignore the S&P messages
  when switching to the S&P operating mode. Only the Sprint logic for
  the Insert key acts as expected, if enabled. Tnx ES5TV and N6TV.

- CW/RTTY Messages options : The Sprint logic for the Insert Key now
  also applies for the AP Sprint. Tnx N6TV.

- New $NEXTSERIAL and $PREVSERIAL CW and RTTY variables. Sends the
  next or the previous serial number of the current QSO line.
  Tnx ES5TV.

- New text commands added :

  - WKSETUP: Equivalent to Options / WinKey configuration...
  - EZSETUP: Equivalent to Options / EZMaster configuration...
  - MKSETUP: Equivalent to Options / MK/MKII/MK2R configuration...
  - RTTYSETUP: Equivalent to Options / RTTY configuration...
  - QUICKQSL: Equivalent to Tools / Intelligent Quick QSL...
  - AUTOCQ/NOAUTOCQ: Enables/disables the Repeat mode
  - CQAUTO/NOCQAUTO: (ditto)
  - CWAUTO/NOCWAUTO: Enables/disable the CW Auto Send
  - AUTOCW/NOAUTOCW: (ditto)
  - CWAUTOON/CWAUTOOFF: (ditto)
  - AUTOCWON/AUTOCWOFF: (ditto)
  - RPTDELAY: Equivalent to Tools / Automatic CQ repeat, with
    the focus set to the repeat interval field
  - CTYFILE(S) / COUNTRYFILE(S): Eq. to Options / Data files /
    Country files...

- RUN / S&P operating : When the repeat mode is enabled, changing to
  S&P operating disables the repeat and the autosend modes. Tnx ES5TV.

- Alt-F : QSO operator added to the editable fields. Modifications,
  if any, are propagated across the network.

- New feature added in the Tools menu to allow the correction of the
  operator for a range of QSO.

  Even if this tool is more supposed to be used after a contest, or a
  DXPed, to correct a wrong or forgotten entry, each correction is
  broadcasted to the other stns of the network by default. You can
  disable this broadcasting to save time, if not needed.

  The easiest way to correct a range of Q, is to set the cursor log
  on the first Q to correct and select the menu item. The operator
  combo will be then already set. Then, adjust the last Q to correct
  by using the arrow keys (and optionally the band(s) and mode(s)).

  Note that corrections are pretty CPU intensive and it may take
  a certain amount of time for large logs, because each QSO
  modification requires internal structures to be
  updated.

  Note : Hesitating and wise users are encouraged to perform a backup
  of their log before proceeding. These corrections can't be cancelled
  while they are progress, to avoid any log inconsistancy...

  Tnx G3TXF and F6IFY.

- WinKey properties : New options to set speed with the WK pot. only,
  or the WT commands when using the "Sync speed" option.

_ User Interface : Following the programming guidelines, all menu
  items requesting additional information to complete are now ending
  with an ellipsis.

- Bugfix : Several bugfixes and improvements on the WinKey speed.
  Tasks #122, 162 and various reports.
  Tnx N6TV, K1EL, F6IFY, OM7ZZ and many others.

- Bugfix : Task #128. CW and RTTY messages dialog now handle
  the Enter and Esc keys as expected. Tnx N6TV.

- Bugfix : WAE QTC transmitting and receiving messages dialog now
  handle the Enter and Esc keys as expected.

- Bugfix : QuickQsl dialog : The Enter and Esc keys work as expected
  while editing the messages.

- Bugfix : Task #173 : The decimal point is now accepted when editing
  QSO frequency or QSX frequency in the Alt-F dlg. Tnx N6TV

- Bugfix : Task #138 : In S&P, F1 was setting the CQ frequency.
  Tnx SV3SJ/F5VIH.

- Bugfix : RTTY windows : Under some circumstances, the automatic
  grabbing with the INSERT key was broken. Tnx W0YK.

3.20.0 (May 14, 2008)

- Bugfix: Black Bandmap with FT-847/FT-897. Tks G4FAL.

- King Of Spain contest : Points per QSO updated following the
  official URE rules. Tnx EA5FQ.

- RTTY wnds : A new (C) button (stands for "Clear", like on a
  calculator) added to clear the TX/RX window; Tnx G3SVD and N6TV.

- RTTY wnds : The mouse wheel now acts like in the other Win-Test
  child windows. It means that you scan scroll, or goto the start
  or the end of the window (by using Shift + Wheel), or change
  the font size a la Firefox/Mozilla by using Ctrl + Wheel. The small
  icon to quickly scroll to the end of the window (located in the
  title bar of the window) is also enabled.

- RTTY wnds : Shift + Click on a message button opens it for edition.

- Log exports : New export LogSearch format to comply with Marios
  5B4WN log search php script. In the options dialog, you can specify
  a range of Q to be exported, and zip the output file (so its name
  will be "blahblah.LGS.ZIP"). Tnx TX5C and 5B4WN.

- Added a LogSearch export option in the Automatic Backup function.
  In this case, the entire log will be exported (the range option
  of the log exports dialog doesn't apply), *but* the zip option set
  is applied.

  Note: Contrarily to the WTB backup, the LogSearch exports are not
  done in a separate background thread. Thus, it is not recommanded
  to enable this option on a running station because WT will be
  unavailable for logging for a while every time an export is in
  progress. During this period of time, an empty file named
  "LOCK" is created in the backup directory, and deleted once the
  export is completed. This ensures file integrity check for a third
  party application using the export file.

- New report in Tools / Check log menu to display all distinct
  callsigns of a log, and band(s)/mode(s) worked by each station.
  You can sort this report by callsign, by number of Q and by country.
  This report can also be opened in the Windows notepad.
  Tnx WA1S @ TX5C.

- Keyboard switching for international teams with different keyboards.
  To help these users, a new switching dialog is added in the
  Tools / Data entry menu. It is enabled only if several keyboards
  are installed in your system. You can also access this dialog
  by entering the text commands KEYBOARD or KEYB for short.

  We remind you that you can also switch keyboard by using the text
  command KEYB/xxx where xxx is the abbreviated language code
  described there :

  http://www.microsoft.com/globaldev/reference/winxp/langtla.mspx

  For example : KEYB/FRA, KEYB/ENU or KEYB/ENG etc.

  For convenience, this abbreviation is also mentionned in the
  keyboard switching dialog.

- Rate wnd (Alt-R) : By default for new logs, the calculated offtime
  is now based on the contest rule. You can still use a custom setting
  to check your operating (in)efficiency. If the contest rule is
  unknown, 15 minutes will be used. Tnx DL6RAI, N6TV and others.

- Interfaces : New option in the MK/MKII/MK2 setting dialog to check
  if the microHAM router software is running. Tnx F2JD @ FO5A/MM ;-)

- Interfaces : New option in the MK/MKII/MK2 setting dialog to start
  the microHAM router if it not running yet.

- Interfaces : When a COM port can't be opened, you now have the
  possibility to retry opening, to continue with this port closed for
  this session only, or to disable it permanently.

- Log wnd : WT can now display a QSO count over 99999 in DXPed mode.
  Tnx ES5TV @ VP6DX.

- Packet parser modified to comply with the CWSkimmer telnet
  pseudo-cluster syntax (the # char is now accepted). Tnx N4ZR.

- Startup : If Win-Test is started with the Ctrl key down, it
  doesn't automatically load the previous opened log.

- Merge dialog : In the "Add file" dialog, you can now select multiple
  files at once. Tnx TX5C.

- Merge dialog : New button to designate the master file. Tnx TX5C.

- Merge dialog : New option to load the master file once merging
  is completed.

- New continent field available in the CSV and TXT export files.
  Tnx VA7DX @ TX5C.

- Callsign checks are now a bit more restrictive to prevent typing
  errors. Tnx WA1S @ TX5C.

- DXPed mode : You can now specify the duration of the operation
  (between 1 and 15 days) in the contest settings dialog, to fit
  the stats wnd horizontal range (Ctrl-F9). You have to enlarge
  this wnd if needed. Tnx TX5C.

- DXPed mode : Default Insert key msg modified (no more dupe check).
  F3 default message also modified to "$LOGGEDCALL ?". Tnx TX5C.

- Bugfix : ARI DX contest : Typo in the provinces list : FO
  instead of FC (I4). Tnx G3TXF.

- Bugfix : RTTY wnds : If text was selected and the font size
  was modified, the selection rectangle wasn't modified, and
  further selection on received text before the size modification
  was wrong.

- Bugfix : Task #170. HamCap Propagation forecast now also works
  with the callsign entered in the secondary radio window. Tnx N6TV.

- Bugfix : Task #192. CheckPartial (F8) and N+1 (F12) wnds : Dupes
  display failed when callsigns were entered in the secondary
  radio wnd. Tnx N6TV.

- Bugfix : Task #193. Data files specified in command line launch
  with no extension generated erroneous extra files names. Tnx N6TV.

- Bugfix : Task #194. CheckCallsign wnd (F9) wasn't working for the
  ARRL VHF contests (and probably other VHF+ contests). Tnx K1TR.

- Bugfix : Task #191. When using a WinKey, the paddles activation
  cancels the repeat mode if enabled. Tnx N6TV.

- Bugfix : Radio wnds : Under some specific circumstances, the bandmap
  view could display garbage.

- Bugfix : The CSV export settings weren't saved. Tnx N6TV.

3.19.0 (Jan 22, 2008)

- Bugfix: The "elapsed time since the last QSO" bargraph was not
  displayed anymore. Fixed.

- Bugfix: Orion II Radios not properly set when grabbing QSX spots
  from the bandmap. Close bug report #159. Tks K1GQ (KC1XX).

- Added IC-7700 and Tentec Orion II in the list of supported radios.

- Bugfix: Task #174 of the BTS : Using [Alt-F1/F2] to fix band of
  already logged QSO entered on the secondary radio was changing the
  rig, which is not expected. Fixed. Tks N6TV.

- NAQP M/2 (only) : Edit current op. name menu item added. The
  equivalent text commands are OPNAME or MYNAME. Tnx N4CU.

- Radio Wnd / Bandmap view : Max. zoom extended. Tnx G3RXQ.

- ARRL RTTY Round-Up implemented. Tnx F6IFY.

- Basic Operators management

  Foreword : This feature is very limited, and will *not* be further
  extended in this major version of Win-Test (v3). It is mainly added
  to help DXPeditioners for the web log search scripts, and for
  various DX or contesters challenges (RRDXA etc.)

  New text commands : OPON (or LOGIN), OPOFF (or LOGOUT).

  This feature is only available to multi-op logs.

  If you entered a list of operators in the contest settings dialog
  when creating the log, it will be parsed to init the combo-box. You
  can also add ops "on the fly" to this combo box.

  If you add nicknames to ops of this list (joe, jack, william,
  averell, josette or whatever - letters and numbers are accepted,
  allowing exotic nicks like l33t etc.), you can enter them as text
  commands to quickly change operator, without using the OPON command.

  Op. callsigns are limited to 7 chars, while nicks are limited
  to 13 chars.

  The operator changing is propagated across the network, meaning
  that if you login on a station, you will be automagically logged
  out of the previous one you were logged on (if any).

  The ADIF file export includes the op callsign in the QSO record, if
  an op. has been defined for that QSO.

  The text and CSV export files are also enhanced to allow the
  inclusion the op. callsign.

- ARRL 160 : The Cabrillo file now marks empty exchanges (for DX side
  stations) with "---" to comply with the ARRL robot. Tnx F5IN, N5KO.

- New KEYB text command : Designed for international multi-op teams.
  You can now switch keyboard to use in WT with a KEYB/xxx text command
  following the abbreviated language code described there :

  http://www.microsoft.com/globaldev/reference/winxp/langtla.mspx

  For example : KEYB/FRA, KEYB/ENU or KEYB/ENG etc.

  Caution : The keyboards layouts must have been installed in the
  Windows language bar before using !

  This portion of code is CERN-approved.

  Tnx F6IFY, F5VIH/SV3SJ.

- Grammar : Objectives renamed as Targets. Tnx G3TXF.

- ARRL SS : The licence year log entry field title is now Chk (stands
  for Check). Tnx N6TV.

- ARRL SS : New $CHECK variable added to send your licence year.
  This variable only works for this contest. Tnx N6TV.

- CTY files : To strengthen the parsing of these files, all trailing
  spaces are now ignored. Tnx W9ZRX and AD1C.

- CTY files : The parser now supports leading equal symbols (=) of the
  future CTY files. Tnx AD1C.

- Bugfix : NAQP : Cabrillo file : Op name field was broken in M/2. And
  Transmitter ID added in M/2 only. Tnx N4CU, N6TV, N5KO.

- Bugfix : CQWW 160 : Default band (160) was broken. Tnx DL6RAI.

- Bugfix : Left-handed users who used the appropriate Windows mouse
  settings weren't able to move the Clock and SSB bargraph windows.
  Tnx JQ1BVI.

- Bugfix : ARRL SS : The exchange guessings were not reset when the
  callsign was modified. Tnx N6TV.

- Bugfix : Tools : Check exchanges : Inconsistent behaviour under
  certain circumstances.

- Bugfix : When opening or creating an empty log, it was locked from
  the OS point of view, even after closing it in WT. Tnx N6TV.

- Bugfix : Ctrl-K : Partials and N+1 wnds weren't updated. Tnx N6TV.

3.18.0 (Nov 3, 2007)

- MK2R/MK2R+: WT does now display the firmware version number of the
  device in the "detected" message shown at the startup.

- WT can now control the microKeyer through the microHam protocol as
  well. This is useful to control the USB Device Router DVK which
  should give better result in audio and radio switching than using
  the WT integrated Voice Keyer.

  Tks microHam company.

- Some improvements done in the microHam MKII protocol support. This
  version of Win-Test does now request USB device Router v5.0.3 or
  later.

- < and > key behaviours changed. Regardless the SO2R status,
	< key will now switch to the previous field of the main log
	> key will now switch to the next field of the main log

- Bugfix: MK2R/MK2R+ was not configurable anymore. Fixed. Tks OH2UA.

- Bugfix: IC-275/475/1275 communication problems fixed. Tks IK2JUB.

- Bugfix: Frequency Offset fixed with IC-735.

- Bugfix: With an FT1000MP and some other rigs, band map follows TX
  freq instead of RX freq when operating Split. Tks N6TV.

- ARRL SS : Stats are now displayed on 3 days. Tnx N6TV.

- ARRL SS : Every QSO field must be filled to enter it. Tnx N6TV.

- ARRL SS : Dupe warning now indicated the received serial of the
  former QSO. Tnx N6TV.

3.17.0 (Oct 21, 2007)

- CAUTION:  New network protocol version 1.21 released

  Reminder: If you use WT in a networked environment, you must have
  the same WT version on all machines!

- The microHAM micro KEYER II is now supported. WT can control this
  interface using the microHAM protocol in order to use the DVK.

  For that, create/select a free COM port for "Control:" in the
  "microHAM USB Device Router", then select "microHAM MKII" as a
  connected device for the corresponding COM port in the "Interface
  Configuration" window of WT.

  Tks microHAM company for great support!

- Asia Pacific Sprint added.

- JARTS WW RTTY Contest added.

- LPT address can be set between 0200 and FFFF (hex). Tnx VE5ZX

- Bugfix : Sprint logic feature (CW messages option) was not working
  for the EU Sprint. Tnx S51DS.

- Bugfix : Under certain circumstances, the correct local help files
  were not opened. Tnx W9ZRX.

- Bugfix : CQWW RTTY : Except under certain circumstances, the zone
  wasn't filled for K/VE when a QSO has been made with the current
  stn on another band. Tnx DL5AXX, T93Y.

- Bugfix : Task #141 - NA Sprint : Alaska stations (KL) entered in
  the log are now listed with an AK exchange in the Cabrillo file.
  This also applies to the NCCC Sprint. Tnx N6TV.

- Bugfix: When entering a QSX freq for a spot, WT was picking up the
  same transmit freq and re-listed that as the QSX instead of picking
  the second VFO freq. Tks NQ4I.

- Bugfix: Under some circumstances, the Map (Grayline) Window was not
  properly opened when opening a new log. Fixed.

3.16.0 (Sep 7, 2007)

- Intelligent Quick QSL can now be adaptative according to the Instant
  Rate. See the "Intelligent Quick QSL configuration..." window (in
  menu "Tools") for details. Tks CT1BOH.

- Added new macro $QQSLRESET. This macro reset the timer or the
  counter like if the long QSL message were just sent. It makes sense
  to use this macro in each message you send your callsign in like
  CQ (F1 key) or MYCALL (F4 key). That way, you won't send a long
  QSL message after sending your call a few seconds before.
  Tks CT1BOH.

- Added new macros $FREQP and $FREQS - Feature request #8. These new
  macros send accordingly the frequency of the Primary radio and the
  frequency of the Secondary radio. Tks OH4JFN.

- New qualifications to the Kenwood Radios (as well as radios based
  on the same protocol, like SDR-1000, Elecraft):
  - Under certain circumstances, the mode was not read correctly
    at the startup of Win-Test
  - Added the BandMap "Pass to Sub VFO" feature
  - When entering a frequency in the callsign field, the RIT is
    cleared (as far as it is enabled).

- Edition of the Frequency of a logged QSO - Feature request #117.
  In addition to its Date and Time (ALT+F shortcut, or in menu Edit).
  Tks DL4NER.

- Alt-F9/F10 now always change the CW speed by 2 WPM up or down,
  regardless of the current CW speed (can be odd or even). Tks N6TV.

- F11 also wipes the time field if done on the last QSO in the log.

- CQIR contest added.

  For the IRTS 75-year anniversary, make 75 QSO and you enter a
  draw to win a week for two in Kinnitty Casle (flights included).
  For detailled rules, see http://www.irts.ie/CQIR

- SARTG RTTY contest added.

- LOTW contest added.

- SCC Championship RTTY contest added. Requires CTY_LUPROV.DAT file.

- CQWW RTTY : When an US/VE stn is worked, entering his state/province
  is now mandatory. Tnx F6IFY.

- Keyboard mode dialog (Alt-K) revisited. The dlg labels are more
  descriptive than before, and in RTTY you can chain predefined msgs
  with keystrokes, as in CW. The only difference is that in RTTY,
  [Esc] empties the TX buffer, but let the PTT ON, so you can enter
  keystrokes again, unless you close the window (which resets the PTT).

- Spots warning : New option to be warned when spotted on the
  current band/mode only. Tnx I4UFH.

- Radio windows : Markers and segments files can also be set with
  the bandmap display contextual menu.

- Bufix: SWAPing two radios (in SO2R mode) in a mixed mode contest
  might get Mode changes hazardous! In addition, VFO-B programming
  when at least one of the Radio is an Icom gave over. Tks MM0BQI.

- Bugfix: Chaining 1-char long CW messages or using the CW Keyboard
  Mode with WinKey was sometimes causing speed changes (speed was
  actually set to the pot speed). Fixed. Tks DL5AXX.

- Bugfix: RTTY was set using the upper side band for frequencies
  above 10 MHz. Fixed. Tks VE2FWW.

- Bugfix: QTC might be hidden when for portable stations (like N1AA/6).
  Fixed. Tks DJ0ZY.

- Bugfix: Closing QTC session with "+" causes QSO entry problem if
  the serial number is not set. Bug report #123. Fixed. Tks DL1IAO.

- Bugfix: Task #137: "PTT to Wrong Radio after sending something to
  2nd radio". In SO2R, if using Alternate CQ, the TX focus stays on
  "wrong radio" when starting QSO. In addition, the TX focus also
  stays on the secondary radio when one sends something on it. Both
  fixed. Tks OH2UA.

- Bugfix: Task #130: "Broken TRX-Control with TenTec Orion". After
  about 30 min, communication with Orion trx was not working anymore.
  Fixed. Tks DJ0ZY.

- Bugfix : WAEDC contest : In the QTC transmit or receive dialogs,
  the CR and + keys didn't work as expected in SSB mode. Tnx ES5TV.

- Bugfix : WAEDC contest : The ADIF STX field wasn't set. Tnx F5UKL.

- Bugfix : Stats wnd (Ctrl-F9) : Under certain circumstances, the
  displayed graph wasn't correct on this window opening. Tnx DJ0ZY.

- Bugfix : Some mixup in the parity labels and abbreviations of the
  COM properties dialog. It is advisable to check your COM settings,
  especially if some of your interfaces use Even or Odd parities.
  Tnx DG7RO.

- Bugfix : Notes are stored in the local .NOT file even if outbound
  protocol is disabled. Tnx N6TV.

- Bugfix : [Esc] didn't always stop messages keying (CW or RTTY).
  Bug report #132. Tnx DJ0ZY.

- Bugfix : Under certain circumstances, Cabrillo v3 files import
  failed. Tnx F5LEN.

3.15.0 (Aug 8, 2007)

- New set of CW/RTTY variables dedicated to the WAE

  Receive QTC window:
	$MYCALL:	Send my callsign
	$VALID:		Save everything and close the window
	$QTC:		Send <group>/<number>
	$NEXT:		Move focus to the next QTC line

  Transmit QTC window:
	$MYCALL:	Send my callsign
	$VALID:		Save everything and close the window
	$QTC:		Send <group>/<number>
	$NEXT:		Move focus down to the next QTC line
	$13:		Send carriage return character (specific to RTTY)
	$TIME:		Send time of the current QTC
	$CALLSIGN:	Send callsign of the current QTC
	$SERIAL:	Send serial number of the current QTC
	$DONE:		If all QTC are sent: mimic the + key
	$SERIE:		Send the QTC series (specific to RTTY)

- The CW/RTTY messages specific to the WAE contest (QTC
  Receive/Transmit) windows can now be redefined in the menu
  "Options | CW/RTTY | Modify WAE messages...".

  It is also possible to modify the label texts of the buttons for
  both the "QTC Transmit" and the "QTC Receive" windows. The variable
  $QTC can be used and will be replaced by the appropriate QTC
  group/number in the "QTC Transmit" window.

- RTTY leg of the WAE contest now supported in beta test.
  QTC groups and series will be highlighted in the RTTY window.

  Assuming you receive the following sequence:

  QTC: 65/2 QTC: 65/2
  0917-GI8HXY-146
  0918-G8UBJ-068

  First click on one of the highlighted "QTC: 65/2": this will
  automatically open the "QTC Receive" window and fill the
  QTC group field.

  Then click on each QTC serie highlighted lines. Again, they
  will be passed automatically to the "QTC Receive" window.

- Sub VFO programming from the bandmap: added for Tentec Orion, FT-2000,
  FTDX-9000

- SWAP Radios feature rewritten. To be tested with various rigs!

- CW-Reverse mode added for some Radios:
	- Orion
	- All kenwood Radios supporting CW-Reverse
	- All radios using a Kenwood-based protocol which are supporting
	  CW-Reverse (Elecraft, SDR-1000).
	- All Icom which are supporting CW-Reverse.
	- FT-1000MP/MkV, FT-2000, FTDX-9000
  Other rigs can be considered as far as the protocol can handle it.
  Please tell us!
  There is no setting in WT in order to enable/disable this feature.
  Just set the CW Reverse on the radio, WT will remember that setting
  for the next time the mode must be programmed onto the radio.

- ARRL Field Day: LOG layout reorganized.

- FT-1000MP: RIT is cleared but status is preserved when frequency
  change. Tks N6TV.

- V/UHF and 50/70/V/UHF contests with gridsquares as mults and one
  point per QSO. Tnx G4HSU & G4PIQ.

- Bugfix: In the WAE contest, opening the QTC Receive/Transmit window
  was not working as expected. Fixed. Tks IZ3EYZ.

- Bugfix: Polling Rate Combo Box of the "Interface Configuration"
  window was empty. Fixed.

- Bugfix: Transmitting status in the Secondary Radio fixed in
  RTTY mode. Tested with no SO2R interface.

- Bugfix: Selecting a single non-alphanumeric in the RTTY windows
  issued a in crash. Fixed. Tks DL6RAI.

- Bugfix: The CQ repeat mode was not activated when clicking on the
 "F1" button of the RTTY wnd. Fixed. Tks VE2FWW.

- Bugfix: Under certain circumstances, a dupe QSO was not credited to
  0 point in both NCCC Sprint and NA RTTY Sprint contests. Tks N6TV.

- Bugfix: FT-2000 / FT-9000, the active VFO in WT was thrall to the
  to RX VFO of the radio. Correct way is to thrall the TX VFO of the
  radio. Fixed. Tks G4IRN.

- Bugfix: VFO B programming of the Orion fixed. In addition, a timer
  now ensures to always wait at least 100ms between each commands
  sending. Tks SM6CNN.

- Bugfix: NAQP, NA Sprint and NCCC: Database Updates was saving
  the OP Name insteed of the State/Province/Country. Fixed. Tks N6TV.

- Bugfix: ARRL Field Day: ARRL/RAC official sections modified
  according to the rules. Tks VE3SY, 9A5CW, N6TV.

- Bugfix: In RTTY, QSOB4 was not working anymore. Fixed. Tks IN3JJI.

- Bugfix : All V/UHF contests : A QSO with own callsign gave one
  point.

- Bugfix : CW smartcorrect : Text commands are ignored now. Tnx N6TV.

3.14.0 (Jul 25, 2007)

- Done some improvements and bugfixes in the NAQP contest. It now uses
  a specific "Equivalent State/Province" file: NAQP.DAT. It also uses
  the Cabrillo v3 specs for generating logs for the contest sponsor.
  The RTTY leg also supported.

- Added NCCC Sprint (NS) contest.

- The Run and S&P radio buttons of the Secondary Radio Window are
  now hidden when S&P mode is not active. Tks CT1BOH.

- New text command "MESSAGES" to open the "Standard CW/RTTY messages
  configuration" window (menu "Options | CW/RTTY | Modify Standard
  Messages). Text command "MSGS" is an equivalent. Tks N6TV.

- Elecraft K3 added to the list of supported radios. Tks F6BEE.

- Run/S&P switching capability menu renamed to improve the user
  interface.

- Bgfix : IOTA contest (and several others) : The guessed exchange
  was not correct. Tnx DL4CF.

- Bugfix: WT Windows of an imported Cabrillo log were not opened
  at startup. In addition, WT was loosing Focus. Fixed. Tks N6TV,
  I4UFH.

- Bugfix: Under certain circumstances, the exchange was not filled in
  for stations previously worked. Fixed. Tks N6TV.

3.13.0 (Jul 23, 2007)

- CAUTION:  New network protocol version 1.20 released

  Reminder:  If you use WT in a networked environment, you must have
  the same WT version on all machines!

- The generated CABRILLO files for both CQWW DX and WPX are now in
  the CABRILLO V3 Format.

- Cabrillo V3 (in addition to Cabrillo V2) can be imported.

- NAQP fields reorganized. Unfortunately, this inverted the "OP name"
  and "State/Province/Country" field in the WTB binary file. It means
  that if you open an old NAQP file done with Win-Test, the "OP name"
  and "State/Province/Country" will be on the wrong places. There is
  a workaround if you want to open an old NAQP file with the latest
  version of Win-Test: revert to an old WT version and generate a
  Cabrillo file from it. Then install again the latest Win-Test version,
  and import the generated Cabrillo. My apologies for these troubles
  but it was making sense to invert these fields in order to be more
  efficient with that contest, as well as with NA Sprint, NCCC...
  which share some of the same code.

- NA Sprint contest added. Log for the contest sponsor is generated
  using the CABRILLO V3 specifications. Note that the State/Province
  will contain DX for non-US/VE stations whatever the operator logged
  in the field. Tks W0YK, N5KO, K3LR, N6TV and others.

- Added support of the new TenTec Omni VII radio, which is actually
  based on the Jupiter command sets.

- Added a Search & Pounce Operating Mode feature in order to have
  two different sets of CW/RTTY messages:  one when running, and one
  when searching multipliers.

  The Run and S&P sets of messages are editable in the "Messages" Tab
  of the "Standard CW/RTTY Messages Configuration..." window.

  Use CTRL+TAB to switch between RUN and S&P mode on the Primary Radio.
  The status of this mode is shown in the clock window. To change the
  mode of the Secondary Radio Window, use either SHIFT+CTRL+TAB or a
  mouse click on the appropriate control in the Secondary Radio Window.

  It is possible to configure WT to automatically wipe the logged QSO
  or populate the Band Map when the operator changes the radio
  frequency, as soon as the Search & pounce mode is activated on that
  radio. This can be configurated from the "Band Map Properties"
  (right click in the Band Map windows).

  NB: Search & Pounce is not activated by default. This can be done
  in the menu "Tools | Data Entry | Search and Pounce".

- The $QSOB4 content macro can be redefined in the "Options" Tab of
  the "Standard CW/RTTY Messages Configuration..." window. That macro
  doesn't support any variable in, except $MYCALL. Tks N6TV.

- "Sprint Logic" feature added. Applicable in the EU Sprint, NA
  Sprint and the NCCC Sprint contests. When activated, WT decides which
  INSERT CW/RTTY Message must be sent according to the "Rcvd QSO
  Number" field.

  When that field is empty, WT assumes that the operator just called
  CQ, and then sends the INSERT message of the "RUN" mode.

  When that field is not empty, WT assumes that the operator just
  replied to a CQ, and then sends the INSERT message of the "S&P"
  mode.

  This feature can be enbled/disabled in the "Options" Tab of the
  "Standard CW/RTTY Messages Configuration..." window. Other
  contests are not affected by this option.

  Tks N6TV, K3LR, K0XP, N2NL and many others.

- New option to "Stay in Field when moving in the log", in order
  to avoid having the cursor always back on the callsign field.
  Option is in menu "Option | Log".

- Summary wnd (Alt-S) : New option to include or not the dupes in
  the QSO counts and the avg calculations.

- REG1TEST files : The New Country flag in VHF+ contests is now
  set in an appropriate manner. Tnx HB9DFD.

- QSO deletion : The warning message is now more informative.
  Tnx N6TV.

- Bugfix: In the specific case where one was operating a contest
  with a separate serial number per band, changing band on the
  Secondary Radio when the cursor was not in the last position
  of the log in the Primary Radio, the serial number set for the
  Secondary Radio might be wrong. Fixed.

- Bugfix: The Precedence field were not corrected in the log when
  modified in a previous logged QSO. Fixed.

- Bugfix: The Multiplier window was always showing DXCC for all
  bands, even for a contest which the band doesn't care in for
  DXCC multipliers. Fixed. Tks N6TV.

- Bugfix : The INVENTORY command was filtered by WtTunnelSrv and
  could only be used within a LAN. Tnx F6IFY.

- Bugfix : Internal CW generator : Under certain circumstances, the
  inter characters space was dropped. Tnx TA2RC, OH2UA.

- Bugfix : Log display : When working CW or RTTY, a 5-char received
  exchange was truncated. Tnx F5HRY/TM0HQ.

- Bugfix : When using Ctrl-K to delete characters behind the cursor
  in CW, and under other certain circumstances, $LOGGED was not
  updated. Tnx N6TV, CT1BOH.

- Bugfix : Under certain circumstances there was no separator space
  between zones in the Alt-Z wnd, when marks were displayed.

3.12.0 (Jul 11, 2007)

- Frequency Offsets (ie when the rig is used with a transverter) added.
  Settings can be done in the menu "Options | Frequency Offsets".

- Helvetia VHF/UHF/Microwave contest added. Tnx HB9DFD, HB9DUP, HB9CEX
  and others...

- IOTA contest : If an IOTA ref is entered in the appropriate field of
  the log, *only* QSOs with this IOTA are displayed in the multipliers
  wnd (F10). Tnx MM0BQI.

- IOTA contest : If an island reference is entered in the Exchange input
  field of the contest configuration dialog, the CW messages include
  it in the predefined messages. Tnx TA2RC.

- The summary file (.sum) now uses the standard CRLF newline characters.
  Tnx DL6RAI.

- Internal CW generator (LPT and COM outputs) : The PTT hold time is
  shortened. It is abt one dot long now. Tnx YT1NT.

- DXpedition HD : Dupes count added in the summary wnd, and DUPE
  indicator added at the end of log lines, if applicable. Tnx G4IRN.

- Bugfix : REG1TEST output log was broken.

- Bugfix : CQWW WPX M/2 : Under certain conditions, the serial
  number sent wasn't consistant when a spot was grabbed. Tnx DL6RAI.

- Bugfix : Some english spellings fixed. Tnx G3TXF

3.11.1 (Jul 1th, 2007)

- The worked states window was showing K3 twice. Fixed. Tks NX5M.

3.11.0 (may 18, 2007)

- CAUTION : New network protocol version 1.18 released

  Reminder : If you use WT in a networked environment, you must have
  the same WT version on all machines !

- Help files : Online help now leads to the Win-Test wiki site. Every
  dialog and child window has its own help page.

  Special tnx to the wiki team M0CLW, DL6RAI, DL4NER, I2WIJ.

- VHF+ contests : Distances can be expressed in miles :

  New option to display distances in miles in all windows except the
  stats windows where new items were added (Miles and avg mi/QSO) to
  ensure compatibility and consistancy.

  The objectives keywords allowed for distances are now :

  Distance in km => KM DISTKM
  Avg distance in km => AVGKM KMAVG
  Distance in miles => MI DISTMI MILES
  Avg distance in miles => AVGMI MIAVG

  To avoid any confusion, the DIST and DISTANCE keywords are no more
  valid.

  A new field has also been added in the export function to get
  QSO distance in miles.

  Tnx K3LR, W9ZRX.

- Gridsquares map (Alt-L) : The current gridsquare (4-chars) is
  displayed even if the callsign field is empty. Tnx DK5TX.

- Interface setup dialog : The last part of the IP broadcast address
  can now be different from 255. Tnx SP5ELA.

- Field Day IARU Rgn 1 (RSGB) : CW and SSB legs have now different
  method of scoring, according to the different RSGB rules.
  Tnx G3TXF, GM0ELP, G3UFY and others...

- JIDX contest : 160m band added for the CW leg. Tnx F5IN.

- ARI contests : The (IS0) Medio Campidano province abbreviation
  changed from MD to VS. Tnx ON5GQ.

- RDXC : SH oblast renamed to YA (official abbreviation, according to
  the RDXC website). The WT_OBL.DAT and OBLASTS.DAT file are now
  updated accordingly. Tnx HA1AG.

- New option in the Options / Automatic backup dlg to notify the user
  when a backup is completed by a warning under the log lines.

- Markers files (.mkr extension) : If the comment includes a valid
  4-char or 6-char grid square, the tooltip displays the heading and
  the distance to this grid square. It also displays the marker label
  if it is not entirely visible in the bandmap wnd.

- Bugfix : Helvetia (H26) contest : Mixed category allows only one
  QSO per band, whatever mode used. And Cabrillo output log in multi
  category now mentions the mode category (CW, SSB, or MIXED).
  Tnx DJ3WE and HB9CZF.

- Bugfix : Spelling and grammar mistakes in menus and dialogs.
  Tnx ES5TV, DL6RAI.

- Bugfix : WPX contest : Some very long and fake callsigns (like
  SIROCCO92, EIOLEKUIN0, WWWWWWWWWWWWW1 or such) could crash WT.
  Tnx ES5TV and 9A5CW.

3.10.1 (Mar 22, 2007)

- Maintenance version.

3.10.0 (Mar 22, 2007)

- Bugfix: $TR1 and $TR2 macros were not working using the microHam
  MK2R interface. Fixed. Tks OH2UA.

- New tool : Time shifting, in the Tools menu.

  You can time shift selected Qsos by any amount of time in both
  directions. You can apply the time shift for the entire log, for the
  Qso entered by your own station, for Qso entered by several stns,
  or for a range of Qsos.

  Even if this tool is more supposed to be used after a contest,
  to correct a wrong clock setting, each time correction is
  broadcasted to the other stns of the network by default. You can
  disable this broadcasting to save time, if not needed.

  Note that time shifting is pretty CPU intensive and it may take
  a certain amount of time for large logs, because each Qso
  modification requires internal structures (mainly statistics) to be
  updated.

  Note : Hesitating and wise users are encouraged to perform a backup
  of their log before proceeding. Time shifting can't be cancelled
  while it is in progress, to avoid any log inconsistancy..

- Main log window : New option in Options / Log menu to hide the QSO
  number column. Tnx RW3AH, SM3WMV.

- Main log and secondary radio windows : To ease reading, the received
  RS(T) and the received exchange are now separated by an half space
  wide blank area.

  Note that it is still *one unique* field. It is only a display trick.

- New feature : Band segments for bandmaps

  You can now display segments in the bandmap tab of the radio
  windows. Segments are defined by textual files with a .seg extension
  located in the Win-Test directory. You can use and display up
  to 10 files simultaneously, by selecting them in the Options /
  Data files / Segments files... menu.

  Note that, because of the available area constraints, you can't have
  more than 5 segments displayed per band for a given frequency.

  You can display or not the loaded segments by using the contextual
  menu item Display Options / Segments / Display. This setting can be
  different for each radio.

  The syntax of the segments files is very basic, and are very easy
  to create with a simple text editor like notepad.

  A segment is defined by its minimum frequency (in kHz), its maximum
  frequency (in kHz) and an optional tooltip (30 chars max.). The two
  frequencies can be linked by an hyphen.

  Example :

  14150-14350 Extra licences SSB

  A directive is also allowed :

  # COLOR color => Sets the color of the following segments of
    the file

  The allowed colors are :

  White, Black, Red, Green, Blue, Yellow, Magenta, Cyan.

  The case of the color is irrelevant. If no color is specified, the
  segments will be yellow.

  Example :

  # COLOR blue
  #
  14150-14350 Extra licences SSB

  will display this segment in blue on the bandmap. Its associated
  tooltip will be "Extra licences SSB".

  The segments order, and potential overlaps in the file are irrelevant.
  WT will take care to display them in an optimized way.

  Two sample files are located in our repository :

  http://download.win-test.com/files/segments/

  UsSegmentsDetailled.seg displays all band segments for every US
  licence type.

  UsSegments.seg displays all band segments in which all US licencees
  are potentially active.

  You can make your own band segments files for other countries,
  regions, etc. and share them with the WT community if you want.

  Tnx DL1MGB for inspiration.

- New feature : Markers for bandmaps.

  You can now display markers in the bandmap tab of the radio
  windows. Markers are defined by textual files with a .mkr extension
  located in the Win-Test directory. You can use and display up
  to 10 files simultaneously, by selecting them in the Options /
  Data files / Markers files... menu.

  You can display or not the loaded markers by using the contextual
  menu item Display Options / Markers / Display. This setting can be
  different for each radio.

  The syntax of the markers files is very basic, and are very easy
  to create with a simple text editor like notepad.

  A marker is defined by its frequency (in kHz), its label (one word)
  and an optional tooltip (30 chars max.).

  Example :

  14100 Bcn NCDXC Beacon

  Two directives are also allowed :

  # BACKGROUND color => Sets the bg color of the following markers of
  the file. If no color is specified, the default color is green.
  # TEXT color => Sets the text color of the following markers of the
  file. If no color is specified, the default color is black.

  The allowed colors are :

  White, Black, Red, Green, Blue, Yellow, Magenta, Cyan.

  The case of the color is irrelevant.

  Example :

  # BACKGROUND white
  # TEXT green
  #
  14100 Bcn NCDXF Beacon

  will display a white marker with "Bcn" green text. The associated
  tooltip will be "NCDXF Beacon".

  As usual, you can double-click on a marker to set the current
  radio on the freq. of the marker.

  A sample file is located in our repository :

  http://download.win-test.com/files/markers/

  called NcdxfBeacons.mkr. It displays markers for each NCDXF beacon.

  You can build your own markers files (VHF beacons etc.) and share it
  with the WT community if you want.

  Tnx DL1MGB for inspiration.

- WPX contest : Mult wnd (Alt-M). Band selection menu item removed.
  It also applies for the RDAC contest. Tnx I4UFH.

3.9.0 (Mar 13, 2007)

- Added a tool for searching the logged exchanges which are
  potentially bad according to the database or to the other QSO made
  with the same station during the contest. Works for CQWW, ARRL DX or
  any contest in which there is something which apparent to a zone. It
  also works for the VHF contest when a gridsquare is logged.
  Look at this tool in menu "Tools | Check Log | Search for possible
  Bad Exchanges".

- Added a tool for searching N+1 for each unique logged callsign
  in the log. A unique callsign is considered as this as soon as it
  appears only one time in the log (contact only on one band and
  mode, and no dupe).
  N+1 can be searched against the log, the callsign database (master
  database) or both.
  It is possible to disable the N+1 search for the unique callsigns
  which are known in the callsign database.
  Look at this tool in menu "Tools | Check Log | Show Uniques".

- Coordinates (Long/Lat) expressed as decimal degrees added in the
  fields list which can be exported in text or CSV format. They are
  calculated from the country file used when the log was created, or
  the gridsquare received, if any (mostly in VHF+ contests).

- QSO time in Unix time stamp format, frequency in MHz and QSX in MHz
  also added in the fields list which can be exported in text or CSV
  format.

- RDXC : Summary wnd (Alt-S) : Dupe column added for mixed category,
  and consistancy check between the mixed category and a monomode
  category :

  - QSO column : Includes QSOs (even invalid ones) but not the dupes
  - Dupes column : Includes dupes only
  - Avg column = Total pts for the band / QSO column (see above).

  Tnx I2WIJ

- Bugfix: "$TR1" and "$TR2" commands were not working in SSB when
  placed at the end of a scenario. Fixed.

3.8.6 (Feb 26, 2007)

- Bugfix: Workaround: Reverting back to the old way to ESCape a voice
  message. This is an emergency fix, just before a major contest.
  Tks EI3JE and I2WIJ.

- Bugfix: The RTTY additional RTTY message (ALT-C) was producing CW.
  Tks DL1IAO.

- Bugfix: When Keyboard Mode (ALT-K) is initiated during an F-key
  message ALT-K will not accept any more input when the type ahead
  buffer got empty (i.e. when typing too slow). Fixed. Tks DL1IAO.

- Bugfix: When pressing INS in an empty log line, no serial number is
  sent. Fixed. Tks DL1IAO.

- It is now possible to use any "$MACROS" ($F1, $F2...) in the
  additional messages as well. Tks N1FIC.

- Child wnds positions, sizes, colors and Z-orders are saved in a
  "smarter way" than before. Tnx DL6RAI.

- Dot character (.) added in the CW generator. Tnx IK7JWY.

- Bugfix : WPX RTTY : 160m band removed. Tnx F5CQ.

- Bugfix : WPX RTTY : Scoring updated. Tnx F5CQ.

- Bugfix : WPX RTTY : Serial numbering for M/2 category is now
  compliant with the rules : One numbering sequence per transmitter.

3.8.4 (Feb 8, 2007)

- Spots wnd (Alt-A) and radio wnds : New shortcuts introduced :

  - Ctrl + Dbl click on a spot deletes this spot (no warning)
  - Alt + Dbl click on a spot loads the sub VFO (if applicable)

  Tnx DL4NER, W9ZRX @ K3LR and G3OZF.

- Edited spots are now considered as op-entered and are transmitted
  across the network. Tnx DL6RAI.

- Check partial window contextual menu items regarding the 2-char
  options re-labelled to improve the user interface. Tnx DL6RAI.

- Data entered in the contest settings dialog are now trimmed.
  Tnx W9ZRX @ K3LR.

- The CW Narrow Filter is now set on the IC-765. Tks DK4YJ & K8BB.
  Done also for the IC-756. Tks F5VIH/SV3SJ.

- Bugfix: Frequency was not read correctly on a FT-1000 when inserting
  a spot in the bandmap. The Split mode was not working either. Fixed.
  Tks N8TR.

- Bugfix: DK4YJ reported that sending mode information to his IC-765
  always changes the filter bandwidth to 2.4 KHz in CW. For this
  reason, ALT+F4 now changes the mode of the radio only when
  necessary. Tks DK4YJ.

- Bugfix: With the "Independent speed" option in WinKey ticked,
  using ++ or -- in the message was changing speed to the paddle
  speed. Tks VE2FU.

- Bugfix: the * key used to switch radios in SO2R caused an Icom
  radio that is being switched to always activate the VFO-A as
  default. Fixed. Tks K8BB.

- Bugfix: Station names containing a space in the first position
  of the string was misordered in the "Send GAB" window. Fixed.
  Tnx W9ZRX @ K3LR.

- Bugfix: Tentec Omni VI support is now based on the Generic Icom
  settings. Tks K7SV, DK4YJ and F6IFY.

- Bugfix: Entering Split on any Icom radios was always setting
  the mode to SSB, regardless of the current mode. Fixed. Tks K3LR.

- Bugfix: Protocol issue with either the FT-2000 or the FTDX-9000:
  grabbing a callsign from the bandmap was activating the split
  on the radio. Tks F8CIL, G4IRN.

3.8.0 (Jan 18, 2007)

- Radio wnd / Bandmap tab : New CQ and QSY cursors to display the last
  CQ freq and the QSY freq of the band. These cursors can be displayed
  or not, according to the contextual menu settings (Display options).

- NAQP contest : When entering a NA QSO, WT now ensures all field are
  filled. Tnx K8BB.

- Summary columns re-order for:
	- the ARRL DX to BAND/QSO/MULTS/DXCC/DUPES
	- the CQWW DX to BAND/QSO/CQ/DXCC/DUPES/POINTS/AVG
  which is the usually used order. Tks K3LR.

- MicroHAM MK2R SO2R Protocol is now fully supported. To enable it:

  - in microHAM USB Device Router, check "microHAM SO2R protocol on
    COM port" in the "SO2R" tab. You can also specify "SO2R protocol
	controled" for RADIO 1 and/or RADIO 2 in the "ACC" tab if you
	want to let Win-Test control the ACC outputs to switch the
	antennas.

  - in Win-Test: select "MicroHAM MK2R" on the COM port the USB
    Device Router is attached to for SO2R control. As it is a
	virtual COM port, the COM port configuration (bauds, parity...)
	has no effect: you can choose anything.

  The new macro $MK2R=<cmd> has been added in order to send any
  protocol to the MK2R from a scenario. This can be usefull to set
  a specific audio configuration which is not a standard R1R1, R1R2
  or R2R2. For example, $MK2R=FRD100000010000 will configure
  the headphones audio to "Left=RADIO1,MAIN VFO and
  Right=Radio1,SUB VFO". Please report to the SO2R protocol
  specification of the MK2R to get details on the FRDxxxxxxxxxx
  command as well as on other ones.

  Note that WinKey and PTT/CW events of the Win-Test integrated
  keyers are not handled by the protocol. It means that if you
  want to use Win-Key or the WT integrated keyers you must
  configure then separately. The PTT/CW signals can share the
  COM port used for the SO2R control. WinKey will required a
  different COM port in any case.

- In RTTY Configuration Window: Added two options:

    - MMTTY window stays on top: when enable, the MMTTY window will
	  be always visible

	- Only show FFT spectrum, waterfall and XY scope: when enable,
	  the MMTTY window is minimized, and does not show the Menu nor
	  the Command Buttons.

- Added a new "RTTY" entry in menu "Options" to allow modifying the
  standard and additionnal messages. Also allowed to access the
  messages entry in the menu "Command".

- Bugfix: Internal keyer + Winkey. Tks G3SJJ.

- Bugfix: the "Copy-Paste the previous QSO" function is now available
  only when the cursor is on the last line of the log. Tks DL6RAI.

- Bugfix: TXing in RTTY was not canceled anymore pressing the ESC Key.
  Fixed. Tks F2JD.

- Bugfix: Focus problem with MMTTY is fixed.

- Bugfix: using a SO2R interface based on LPT port, in a message like
  "$F1 $TR2 $MSG1", the $TR2 macro had no effect. Fixed. Tks S51TA.

- Bugfix: Using WinKey, the CW speed of the paddle was changing
  under certain circumstances. Fixed. Tks DJ3WE and G3SJJ.

- Bugfix : NAQP contest : Under some circumstances, the SPC field was
  cleared while editing the QSO. Tnx K8BB.

- Bugfix : PACC contest : From PA side, working PA stns gave credit for
  province. Now, it only gives credit for PA DXCC country. Tnx PC2A.

3.7.0 (Dec 1th, 2006)

- The "Goto QSO" command now checks if the QSO where we want to move
  from is valid. It also validates that QSO before moving.

- Bandmap properties : You can now set two different lifetimes for DX
  cluster spots and op-entered callsigns. The maximum DX cluster spots
  lifetime is 60 minutes, and the op-entered spots lifetime is 120
  minutes. Tnx ES5TV.

- Main log wnd : Any entered Q by a MULT stn which is not a mult is
  tagged with an "!!!!" indicator.

- Radio wnds : The last used tab is saved as default for further
  reloading or new log creation. Tnx ES5TV.

- Stats wnd : The last used tab is saved as default for further
  reloading or new log creation.

- The QSX freq of a cross-band spot is now ignored. Tnx DL4NER.

- Corrupted files can now be fixed once an error is detected while
  loading. The original file is saved with an "_err" suffix appended
  to its name. CAUTION : This fix function doesn't work with corrupted
  data described here :

  http://www.f5mzn.org/pipermail/support/2006-November/072424.html

- Real-time scoring informations entry fields added in the contest
  settings dialog : DXCC prefix, WAZ and ITU zones, State/Prov/Other.
  *These data are only useful for real-time scoring* and are not used
  for other purposes in Win-Test. They are not yet available in the
  SUMMARY network frames (to come). Tnx 5B4WN/G0WWW.

- The initial CW speed for new files can now be set by using the
  Options | CW | Initial speed... menu item; Tnx I2WIJ.

- You can now record 5 different station infos (callsign, name,
  address, etc.) presets (also called station profiles) in the contest
  settings dialog.

- Bugfix: packet cluster window content was lost after any change
  in the "Interface Configuration" window. Fixed.

- Bugfix: with the "Spot entered or sent by the operator, Log Fields
  are cleared" activated, sending a spot for the QSO logged above
  was clearing the line on the screen. Fixed. BTW, WT now takes
  the last QSO logged on the current station (if any) rather than the
  last QSO logged on any station of the network.

- Bugfix: REPEAT mode was not working with WinKey, nor the TX LED in
  the secondary radio window. Fixed. Tks F5JSD.

- Bugfix : When grabbing a spot, the N+1 and checkPartial wnds were
  not updated. Tnx DL4NER.

- Bugfix : The default "+" CW message wasn't including a trailing space
  after the $CORRECT variable. This error leaded to a bad
  implementation of the $CORRECT variable, and an extra space was
  inserted if the default message wasn't used. Tnx PA2A, DL4NER and
  others.

3.6.2 (Nov 23, 2006)

- Bugfix: in SO2R, repeat mode was not interrupted by a transmission
  on the secondary radio when using the SHIFT key. Fixed.
  Tks CT1ILT (CT6A).

- Bugfix: entering a callsign in the bandmap with an SO2R setup
  using two FT-1000D/MP/MK5 or two FT-100 or two FT-900 was in
  certain conditions inserting the entry into the wrong bandmap.
  Tks CT1BOH (CT3NT), CU2/OH2UA.


3.6.1 (Nov 21, 2006)

- Bugfix: Double click on the WTB file was broken. Fixed. Tks
  I2WIJ.

- Bugfix: In SO2R Advanced Mode, when the secondary radio was
  bound with CAPS LOCK, automatic CQ was always stopping as soon as
  the operator pressed any key. Fixed. Tks CT1ILT (6Y3T, CT6A).

3.6.0 (Nov 20, 2006)

- CAUTION : New network protocol version 1.17 released

  Reminder : If you use WT in a networked environment, you must have
  the same WT version on all machines !

- Added command line arguments:
  wt.exe [--alternative-ini|-i <inifile>] [WTB file to load]
  Tks DL6RAI.

- Added a "Polling Rate" option in the Interface Configuration
  Windows. Note that it is not exactly the Polling Rate which is
  defined here, but the delay before polling the radio again after
  the previous sequence is done. This delay is not so accurate with
  every radio. Check by yourself to see what is the value which fits
  the best your needs!

- SteppIR controler is now supported with an Y cable. Special thanks
  to G3BJ.

- Main window : Extra large font added. Tnx W2RU.

- New graphics in the rate wnd (Alt-R) : Instant continents
  distribution. Uses the same moving parameters as the instant rates
  chart. Tnx CT1BOH.

- Rate wnd (Alt-R) : New options to display or hide non-essential
  sections of this wnd.

- New text commands QSX and NOQSX (equivalent to SPLIT and NOSPLIT).

- New text command REMAPKEYS (equivalent to DEFINEKEYS)

- Partner wnd : New real-time feature to display the callsign field
  of the partner(s) log(s) while he (she) is entering a callsign.
  See the contextual menu of this window. A runner can have up to
  three different support partners. To grab the first real-time slot,
  use Alt-Space. In all cases, you can also double-click on any
  callsign of this window. Tnx K3LR

- DX cluster (Alt-A) and radio wnds : A "*" indicator is displayed
  before the spot callsign when there is a QSX for this spot. Tnx K3LR.

- Send spot dlg (Alt-F3) : The log fields clearing after a spot has
  been sent is applied the same way as the self-entered spots (see the
  bandmaps properties contextual menu dialog).

- Score sending : "Send now!" menu item added in the summary contextual
  menu. It is enabled only if the score sending is enabled.

- Commands | Station type : The settings can now be sticked to the
  computer. If so, it will be used for any newly created logs.
  Tnx K3LR.

- Stats wnd (Ctrl-F9) : DXPed : Stats period extended to 4 days.

- DXPed HF and VHF+ logs : The ADIF export includes the info field in
  the NOTES ADIF field. Tnx FY1FL.

- Status wnd (Alt-J) : The list can now be sorted by band and by
  stations names if several stations are on the same band.

- Bugfix : Most of the VHF+ contests didn't have a final score line
  in the summary window (Alt-S), which prevented any real-time score
  posting. Tnx F5LEN.

- Bugfix : Alt-F4 set the radio in split (even if it originally wasn't)
  and a QSX freq in the nirvana ! Tnx DL6RAI, DL4NER and others.

- Bugfix: FT-1000MP in SO2R mode: in Split Mode, swaping radios was
  inverting TX and RX frequencies on the FT-1000MP/Mk5. Tks EA5BY
  and F5CWU.

- Bugfix: Could not enter a QSO to the bandmap from 2nd radio window.
  Everytime a callsign was typed to 2nd radio window and CTRL-Enter was
  pressed, the QSO was set in main radio band map to the exact QRG
  of the main radio. Fixed. Tks OH2UA.

- Bugfix: Using WinKey, the $CORRECT variable was sending the logged
  callsign in every case, even if the callsign was not changed by the
  operator. Tks G3BJ (G5W).

- Bugfix: the selection of the active Sound Card when more than one
  is available was broken. Fixed.

- Bugfix: a short delay might be introduced when ESCaping (stopping)
  a recorded message played by the Internal Voice Keyer. Tks K3LR.

- Bugfix: stereo signal was not working on LPT port Pin 5. Fixed.
  Tks 5B4WN/G0WWW & GM0GAV.

3.5.0 (Oct 22, 2006)

- CAUTION : New network protocol version 1.16 released

  Reminder : If you use WT in a networked environment, you must have
  the same WT version on all machines !

- Added CTRL+S as a shortcut for the menu "Commands | Swap the
  frequency on both radios". Tks EA5FV & co.

- CheckPartial and N+1 SCP files : If a DEFAULT.SCP or DEFAULT.DTA is
  in the WT directory, it will be used as default file for partial
  and N+1 checks instead of contest-specific default file. Tnx ES5TV.

- When a log is opened in a networked environment, the date of the
  first QSO must match the others logs date with 20 days tolerance. If
  not, a warning is issued and the network and the sync are disabled
  by default on this machine. You can override this behaviour if you
  really know what you're doing!

- NRAU Activity Contest (NAC) : 50 and 70 MHz added. Tnx SM3PZG.

- TXT and CSV file exports : New fields added : Date (DD-Mmm-YYYY),
  date (DD-Mmm-YY), Freq in Hz, QSX in kHz and Hz.

- Bugfix : RELOAD'ing a file was disabling the integrated keyer
  (Phone or CW) and could lead to a major crash under some particular
  circumstances.

- Bugfix : NRAU Activity Contest (NAC) : Bonus points per new
  gridsquare are now considered in the score. Tnx DL1OJ.

- Bugfix : NRAU Activity Contest (NAC) : The spacebar now loops
  the cursor between callsign, received RST and gridquare fields.
  Tnx DL1OJ.

- Bugfix : MMTTY windows were closing themself after 10s. Fixed.
  Tks everybody! :)

3.4.5 (Oct. 8, 2006)

- Added two "Intelligent Quick Qsl" Macros: $QQSLT and $QQSLC. When
  used, these macros send two different confirmation messages, one
  a short QSL message (like TU or EE) and one long QSL message
  (like TU F5MZN).

  A timer ($QQSLT macro) or a counter ($QQSLC macro) are associated
  with these macros to determine if either a short or a long QSL
  message is to be transmitted.

  That way you can send a most of the time a short QSL message to
  confirm the QSO in a pileup, sending your full callsign automatically
  every minute or 5 QSO only.

  You can adapt the counter or timer values as well as the short
  and long messages in the "Intelligent Quick QSL" configuration
  window, from the Tools menu.

  You can use the $QQSLC and $QQSLT macros either in the CW/RTTY
  Messages or in the advanced SO2R scenarios. It is also possible to
  use the feature in SSB (SO1R and SO2R not avanced) but this needs a
  specific configuration in the SSB tab of "Intelligent Quick QSL"
  configuration window.

- Caps Lock can now be used to bind the keyboard to the Secondary
  Radio Window. This can be enabled or disabled in the Operating
  menu. Tks SM3WMV.

- Signal "Headphones Control" (called "RX Focus" in the MK2R
  microHam SO2R interface) is now available on LPT, pin 4. This
  signal allows to control which radio you want to listen in the
  Headphones. Must be enabled in the LPT Configuration Window.
  Low = RADIO 1, High = RADIO 2.

- Signal "Headphones Control" and "Stereo RX Audio" are now
  available on either DTR or RTS pins of any serial COM ports.
  That way, the MK2R microHam SO2R interface can be fully
  controlled through a single USB cable.

- Microham MK2R interface is now supported in SO2R Advanced
  mode.

- QSY wizard wnd : Ensure that HamCAP is alive and that the
  chart tab is in the one selected in the Options | HamCAP | Tab
  menu. If not, the label "Disabled" is displayed in the window.
  Tnx SM3WMV.

- Worldmap window : New option to display only the terminator of
  the greyline. If chosen, a small sun symbol also is displayed
  on the map.

- Secondary radio wnd : When a binding key is used (see Operating
  menu), the color background of the QSO area is changed. Tnx F6IFY

- Secondary radio wnd : Complete color management, similar to the
  other child wnds.

- Check Partial files : WT now accepts the master.dta (CT format) or
  master.scp (textual) files as default check partial files for the
  HF contests. Note that the scp format is a bit quicker to load than
  the dta format.

- Ctrl-W in the sent report or exchange fields now resets this field
  to the default 59 or 599 report (depending on the mode). Tnx LX1NO.

- To enhance the CT compatibility, Ctrl-K now deletes the content of
  the current field, from the cursor position to the end of the field.
  It also works for the secondary radio with the Shift key, if this
  option is engaged in the Operating menu.

- Register dialog : The light-headed licencees can now enter their
  account customer number to recall it when needed.

- New options to start and stop locally wtDxTelnet in the
  Options / DX cluster menu. wtDxTelnet *must* be installed in the
  same directory as WT (which is its default installation directory).

- Macros added in the Packet Dlg window (Alt-T). To edit a macro
  button Shift-Click on it. Note that the Conn and Bye btns are still
  disabled for now. This should be improved in the future.

- Numerous new labelling and graphics elements resizing to accomodate
  with the German language version. Tnx DL6RAI.

- Split freq dlg (Minus key) : The entered freq is checked against the
  current band. Tnx W9ZRX.

- CheckPartial files : If a general contest-specific file is loaded,
  no band, mode or band/mode default file is loaded.

- ON Contest 80m, 6m and 2m added. Tnx F5IN.

- Bugfix : UBA Spring contests : Small inconstancies in the UBA
  sections list. Tnx F5IN.

- Bugfix : CQWW RTTY : The guessed zone from a previous entered Q was
  not filled if using the spacebar guessing. Tnx DJ1OJ and DL6RAI.

- Bugfix : Packet Dlg wnd (Alt-T) : SH/WWV and SH/WCY were sharing the
  same accelerator key (Alt-W). Now, SH/WCY uses Alt-Y.

- Bugfix : Under some conditions, WWV announcements coming from
  DXNet packet clusters were not always considered.

- Bugfix : The taskbar was flashing if the Packet Dlg (Alt-T) was in
  foreground, and a private gab was received.

- Bugfix : The WCY and WWV text commands were closing the solar
  activity wnd if it was opened, instead of changing data source.

- Bugfix : Packet Dlg (Alt-T). Even when using the macros and shortcuts
  buttons, the focus is now always set to the entry field.

- Bugfix : CQWW RTTY : When changing band by Alt-F1/F2, the
  states/provinces window was not updated. Tnx DL6RAI @ DQ4W.

- Bugfix : CQWW RTTY : Under some conditions, the zone and the
  state/province fields weren't updated after grab. Tnx DL6RAI @ DQ4W.

- Bugfix: Sending a spot with ALT+F3 with split activated
  was not transmitting the RX frequency correctly. Fixed. Tks
  W9ZRX & K3LR.

- Bugfix: CTRL + ENTER in split mode fixed. Tks W9ZRX & K3LR.

3.3.5 (Sep 20, 2006)

- CAUTION : New network protocol version 1.15 released

  Reminder : If you use WT in a networked environment, you must have
  the same WT version on all machines !

- Added support for the Yaesu FTDX-9000 radio. Tks VE6SH, OM7ZZ.

- Added support for the Yaesu FT-2000 radio.

- Added support for the Yaesu FT-857. Tks M0CRY.

- Icom radios: CI-V mode is back again as an option (you can now
  decide if you want to poll the radio or use the CI-V mode). This
  option is available in the "Interface configuration" window. Tks
  W9ZRX, K3LR.

- Programming an Icom radio is now more reliable (a check is done to
  ensure that the radio got the protocol) and more faster. Tks
  W9ZRX, K3LR.

- New option to start (resp. stop) wtDxTelnet when WT is started
  (resp. stopped) automatically in the Options / DX cluster menu.
  wtDxTelnet *must* be installed in the same directory as WT (which
  is its default installation directory).

- New RESTART text command, to (guess what ?) restart Win-Test.

- QSX are now parsed from the packet stream and are handled in the
  bandmaps and the DX cluster spots wnd (Alt-A). The split freq
  is also handled when spots are entered by the op with Ctrl-Enter
  (or Ctrl-J). Tnx K3LR.

- CQWW Contest : RTTY leg implemented. This implementation is not
  totally complete but is fully usable to take part in the competition
  It will be improved later, especially when the new databases designs
  (including multi-field guessing) will be implemented.

- Child wnds : Font size : New menu items added to get larger and
  smaller font by one point, and a new "Other..." item to set a
  non-listed font size. Tnx W9ZRX @ K3LR.

- CheckPartial and N + 1 files can now be different of the "database"
  DTB file associated with the contest.

  WT now accept SCP (stands Super Check Partial) plain text files
  (one callsign per line - no ordering required), DTA CT files and
  DTB files for compatibility.

  The preferred format is SCP (plain text).

  Furthermore, WT now also accepts specialised CheckPartial files by
  band and by mode for a given contest. This improves log accurancy
  and QSO rates.

  Please, read :

  http://download.win-test.com/files/checkPartial/%23_READ_ME_%23.TXT

  for more informations.

- CheckPartial (F8) and N+1 (F12) wnds : New contextual menu item to
  list the used files for the searches.

- WAE Contest : EU Side : The new multiplier warning now claims "New
  multiplier" instead of "New prefix". The multiplier indicator in the
  bandmap status has also been changed from C (Country) to M (Mult).
  Tnx DL1MGB.

- Bugfix : SAC contest : In M/M category only, the serial numbering is
  different for each band. Tnx SM6DYK.

- Bugfix : SAC contest : The CW variable $SERIAL wasn't included in
  the default messages. Tnx I2WIJ and F5IN.

- Bugfix : Internal CW keyer : If a message was interrupted by ESC
  while a burst was sent, the speed didn't revert to the original
  speed. Tnx OH2UA, OH1JT and F6IFY.

- Bugfix: IC-7800 was not controlled as expected. Fixed. Tks W9ZRX,
  K3LR.

- Bugfix: under CW autosending mode, pressing ESC was disabling
  this feature in any case which was not always wished. From now,
  pressing ESC will disable autosending mode as soon as the key
  in not pressed when the radio is transmitting or if the caret
  is not in the callsign field. Tks ES5TV, UA6AA.

3.2.0 (Aug 30, 2006)

- CIS contest : Adapted to the new rules 2006 (bands : 160m to 10m).
  The Contests of the month faeture is also updated. Tnx F5IN.

- CheckPartial (F12) and N+1 (F8) windows : New option in the
  contextual menu to limit searches to the available space of these
  windows.

  It is only useful for very slow configurations : For a given
  callsign, once the window is filled, no more search is performed,
  even if the window is resized.

  By default, this option is disabled, meaning that if more matching
  callsigns are available (because [+n] is displayed), you can now
  display them by enlarging these windows on the fly.

- New network protocol advanced settings dlg in the interface settings
  dlg.

  *CAUTION* : Modifications of the default settings must be considered
  with an extreme attention. It is reserved for very particular
  configurations or purposes, mainly used by expert users. You're on
  your own !

  We offer some preset example configurations :

  - Silent time master : Can be used if the computer is used to *only*
    distribute an accurate clock. It will not appear in the status
    wnd of the other networked computers, but it will be listed in
    an INVENTORY command. Note that NO QSO will be recorded on
    (and sent from) this machine with this preset.

  - Silent backup : Can be used if the computer is *only* used for
    this purpose : It will not appear in the status window of the
    other networked computers, but will be listed in a INVENTORY
    command.

  - Packet sharing : Can be used if different stations are networked
    with different callsigns, do not want a common log, but want to
    share a commun packet stream. Can be used for several single-ops
    stations for example.

  - Silent log rebuilding : Can be used if you need to rebuild from
    scratch a complete log from networked stations, without appearing
    in the status wnd of the other networked computers, but will be
    listed in a INVENTORY command.

- RDA Contest : Cursor positioning after exchange guessing modified,
  depending on the guessed region or district and the callsign.
  Tnx HA1AG, UA6AA.

- User interface : You can now drag any child wnd (except the RTTY
  windows) by using the Ctrl key (held down) and left-click anywhere
  in the wnd. It avoids to click strictly in the title bar region.

- TOEC contest : It is now held in September instead of August. Thus,
  the "Contests of the month" checkbox feature is updated. Tnx F5IN.

- New feature : Flexible and powerful bandplans management. See (among
  others) the Options / Bandplans menu item.

- Partner wnd : You can now enter data from the secondary radio wnd.
  Tnx OH4JFN.

- Partner wnd : New "No band/mode filtering" contextual option added.
  Might be useful in some unusual cases.

- New options in the integrated voice keyer settings to mute or not
  the microphone input.

  Reminder : These settings can be modified on the fly with the
  following text commands :

  - MIC : Enables the mic input when the VK is not playing
  - NOMIC :  Mutes the mic input when the VK is not playing (*)
  - MICWHENPLAY : Enables the mic input when the VK is playing
  - NOMICWHENPLAY : Mutes the mic input when the VK is playing (*)

  (*) Default settings.

- Band changes Alt-F1/F2 : WT is now compliant with WL and CT :

  ALT-F1  Next lower band   20 -> 40 -> 80 -> 160 -> 10 -> 15 -> 20
  ALT-F2  Next higher band  20 -> 15 -> 10 -> 160 -> 80 -> 40 -> 20

  "Lower" means "Lower frequency"...

  The menu item labels, and the toolbar tooltips are consistent with
  this behaviour.

  Tnx I2WIJ, DL4NER, F6BEE.

- New Options / Windows / Default opened windows feature. This dialog
  allows you to select the default windows which are opened when a
  new contest log is created.

- Check partial wnd (F12) and N+1 (F8) wnd : A double click on a
  callsign inserts it in the callsign field. Tnx F6IRF.

- New extra informations window (Alt-X => Stands for eXtra).

  This window displays data included in .xdt (eXtra DaTa) files.
  These files are textual and have a very basic "Callsign Data"
  syntax.

  The # TITLE directive is used to display a title in the wnd.

  You can set up to 10 default extra data files by a new menu
  (Options / Data files / Default data files). These files will be
  opened with every log. They must be located in the WT installation
  directory.

  You can also add log-specific extra data files by using the
  "Extra files..." item in the contextual menu of this wnd.
  There is no limitation to the location and the number of these
  log-specific files.

  Some usages of this new feature :

  - VHFers can have a database of stations QRV on such or such band,
    to ask for a QSY.
  - Operators names
  - List of WT users ;-)
  - etc...

  This feature is tailored to deal with few thousands of callsigns
  only. Don't try it with millions of lines !

  If you modify an .xdt file while it is in use, you must reload it
  by using the "Reload files" item menu.

  The # VARIABLE directive allows you to sent the extra information
  in a CW message by using a variable name. The variable name
  *must* begin with the $ character.

  Example : # VARIABLE $OPNAME will substitute the $OPNAME string
  in the CW messages with the extra info included in this file, if
  the sent callsign has matching data.

  *CAUTION* : The variable subsitution only works with the internal
  CW keyer for now.

- To enhance CT compatibility, Alt-F5 saves the current mode and freq
  as the Run freq/mode. It means you can use this command to "store"
  these data without using the F1 key.

- ADIF export : If a power level is set in the contest setup dialog,
  this string is exported in the <TX_PWR> field of every QSO record.
  Tnx W4TME.

- ADIF export : New option to include the contest name in the NOTES
  field of every QSO. Tnx W4TME.

- Cabrillo export : New option to exclude modes in the Cabrillo file.
  Tnx TM0HQ.

- Bugfix : CheckPartial wnd (F12) : In some cases, the result list
  was wrong if the pattern started or ended with a question mark.

- Bugfix : N+1 wnd (F8) : If the wnd width was smaller than one result
  cell, WT crashed. Tnx DJ3WE.

- Bugfix : CheckPartial wnd (F12) : In some cases, the result list was
  truncated, although there was more available empty space.

- Bugfix : Some frequency fields (especially in dialogs) didn't accept
  the dot character.

- Bugfix : Partner wnd : Ctrl-# (exchange current callsign with line #)
  was crashing partner WTs.

- Bugfix : WAEDC : After entering the keyboard mode while the QTC
  window was opened (Alt-L), WT was crashing on the first keypress.
  Tnx DL1MGB.

- Bugfix : Internal CW keyer : Speed modifications by Alt-F9/F10
  during the +/- "bursts" *should* work now. Tnx OH2UA, OH4JFN, F5VIH
  and others.

- Bugfix : Check country wnd (F10) : The geographical and timezone
  exceptions included in the CTY_WT_MOD.DAT weren't used in the WAE,
  RGSB 15/10 and PACC contests. Tnx F5IN.

- Bugfix : After entering a freq, and hitting Alt-Up, the keyer sent
  the freq instead of the callsign ! Tnx F6BEE.

3.1.0 (Jul 27, 2006)

- CAUTION : New network protocol version 1.14 released

  Reminder : If you use WT in a networked environment, you must have
  the same protocol version on all machines !

- Reverse mult check (Shift-F10) : If the mults are mode-dependent,
  (IOTA contest, ARRL 10 for ex.) worked stations are ordered by band
  and mode.

- Check mult wnd (F10) : When automatic update is engaged, any
  modification in the received exchange field updates this wnd
  accordingly. Tnx OH4JFN.

- Check mult wnd (F10) : New CQWW DX display policy for all displayed
  bands :

  1/ The exact callsign is searched
  2/ If not found, the same country with the same zone is searched
  3/ If not found, the same country whatever zone is searched

  In all cases a zone indicator is also displayed :

  'Z' means the current zone is already worked in the current country.
  'z' means the current zone is already worked in another country.

  Tnx OH4JFN.

- Contest settings dlg : New button to help filling the exchange field.

- COM properties dlg : New button to set default settings depending
  on the COM port usage. Must be tested in the real world !

- New Tools / Data entry / Remap slash to portable in VHF+ and FD
  option. This only works for callsign field in the log, for all
  VHF+ (DXPed included) and Field Day contests.

- Automatic and on-demand backups (Options / Automatic backup) : You
  can now get one different timestamped file per backup.
  Tnx DL5MLO @ DA0HQ.

- Backups : If a backup fails, you are asked if you want to disable
  the next automatic backups, if any.

- Partner wnd : When a QSO is entered, or got from the network, the
  logged callsign is checked against the content of the partner wnd,
  and accordingly removed from it. Tnx DL1MGB & DL6RAI @ DA0HQ.

- Partner wnd : When automatic exchange guessing is enabled, any
  grabbed callsign from the partner wnd is checked and exchange field
  is filled accordingly. The check partial and N+1 windows are now
  also updated. Tnx DL1MGB & DL6RAI @ DA0HQ.

- Sked wnd (Alt-B) : Pops up for a hot sked only if the main WT window
  is not iconic, to avoid visual annoyance.

- Commands / Remote command menu item added. Only enabled if there
  are several stns on the network.

- Remote command dlg : You can now also locally apply the entered
  command.

- Send gab dialog (Alt-G) : If the text starts with "/me", it is
  replaced with the station name, and the text is emphasized with
  leading and trailing star character (*), a la IRC.

- Status Wnd (Alt-J) : You can now enable (or disable) logging a
  summary of the network activity. Might be useful for network basic
  troubleshootings. This log uses the .ntk (stands for NeTworK) file
  extension.

- Bugfix : Under some circumstances, when a sync was in progress,
  multipliers tables were totally messed up ! Tnx TM0HQ and DA0HQ

- Bugfix : Automatic backup dlg : Setting the backup file path was
  disabling the automatic backup. Tnx DL5MLO @ DA0HQ.

- Bugfix : Merge progress bar title was corrupted. It now displays the
  master file name.

- Bugfix : If clocks were not in sync, the offtime timer could display
  negative time ! Tnx TM0HQ.

- Bugfix : INV (or INVENTORY) command : All networked stations were
  getting back the status, although only the sender was supposed to.

- Bugfix : Sked wnd (Alt-B) : Under some circumstances, the scrollbar
  was not initialized as expected.

3.0.7 (July 6 2006)

- Bugfix: CW Auto Sending mode was not working if the logged callsign
  had a single letter in the prefix. Tks 5B4AGC.

- Taskbar flashing on gab received is now optional and disabled by
  default. Use the Gab wnd (Alt-I) contextual menu to enable it.

3.0.6

- Bugfix: With Kenwood or K2 radios, CW-R was detected as SSB.
  Fixed. Tks DJ1YFK.

- MMTTY is now started only if RTTY is one of the available mode
  according to the Contest Settings. Tks G3BJ.

3.0.5

- Added "Data Files | Country Files" in the "Options" menu. This
  allows to select which CTY file to use (CTY.DAT, CTY_WT.DAT or
  CTY_WT_MOD.DAT). You can have information regarding these various
  files at http://download.win-test.com/databases/READ_ME.TXT

  It is also possible to download the CTY files from the WT website
  directly from the "Country Files" dialog window.

- Bugfix: PARTNER window was not operating correctly in CW. Fixed.
  Tks ES5TV.

- Fixed various problems with FT-1000MP Mark V in mixed mode
  contests. Tks DL6FBL.

- User interface : If WT is minimised or is not the topmost window,
  its icon now blinks in the taskbar when a new gab is received.

- CW - Serial numbers : A custom table can now be used for serial cut
  numbers. See Options / CW / Serial numbers submenu. Tnx ES5TV.

- QSY wizard wnd : The scoring method is now working with all relevant
  contests. Tnx 5B4WN.

- CW auto sending : NOCWAUTO text command added, to be compliant with
  the current syntax of the other text commands.

3.0.1

- Added an CW Auto Sending mode which can be used to send report to
  the station as soon as the operator logged at least 3 or 4
  characters in the callsign field. See in "Options | CW" menu.

  At least one digit must be entered in the callsign field to enable
  the CW Auto Sending Mode.

  Pressing ESC always disables the CW Auto Sending Mode for the current
  QSO.

  F11 always enables it again.

  Character commands associated with: CWAUTOOFF, CWAUTO3, CWAUTO4.

  Tks WRTC teams!

- Added in File menu and Export from V3 to V2 file format. Export to
  the Editest format (a very old MS-DOS logger) is not available
  anymore.

3.0.0 (Jun 18, 2006)

- Version 3 released

2.32.1 (Jun 18, 2006)

- Rate wnd (Alt-R) : Times elapsed since the last bands changes are now
  displayed in the rate wnd. It works for all categories (except M/M
  in which it is irrelevant). Tnx OH4JFN.

- Keyboard mode dlg (Alt-K) : The Escape key aborts transmission if a
  transmission is in progress (as before), but also closes the dlg if
  there is no transmission in progress. Alt-K also closes this dlg in
  all cases. Tnx OH4JFN.

- Bugfix : ARI sezioni : In mixed mode, the sezioni names for numbers
  0001 to 0999 were not displayed in the F10 wnd. Tnx IZ7AUH

2.32.0 (Jun 10, 2006)

- Added ARRL Field Day Contest. There is one limitation with the GOTA
  stations which must use a separe log and cannot be networked with the
  other stations. Tks KG4RZY and N1ND.

- Added NRAU Activity Contest (NAC). Tks DL1OJ.

2.31.0 (May 21, 2006)

- QSY column can be hidden in the status window (ALT+J) in the right
  click menu. Tks OH4JFN.

- "Pass frequency to SUB VFO" (FT-1000MP only) was not working with
  primary radio. Tks OH4JFN & F6BEE.

- "Pass frequency to SUB VFO" added in the Announcements window. Still
  limited to the FT-1000MP radios.

- Added the new "$LATCH" variable in the scenarios. Tks ES5TV.

- Added support of the "$CR" variable for the SSB scenarios. NB: the
  + key still mimics F3 + ENTER. The $CR variable might be useful if
  you want to have more than one "Thanks" message (like a long one
  including your callsign and a short one). Tested with EZM only.
  Tks ES5TV.

- Added an option in the contextual menu (right click) of the
  "status" window to swap frequency and mode with a remote station
  across the network. This would also fix the bug reported by ES5TV:
  "With FT1000/FT-1000MPs, changing Active Radio in TX/RX Split mode
  back and forth swaps the 2 VFOs"

- ARI DX and ARI 40/80 contests : Italian provinces list updated from
  the official ARI contest site. Tnx ON5GQ.

- Bugfix : Radio wnd - Bandmap view : The "Delete" contextual wasn't
  working anymore and the scale value wasn't in the right menu item.
  Tnx F5IN.

2.30.1 (May 1st, 2006)

- Bugfix: F5 CW message was not interrupted using Escape when CW was
  generated by the WT internal morse keyer. Fixed. Tks DL6RAI.

- Bugfix : IOTA contest : The exchange entry field in the contest
  settings dialog was disabled. Tnx CT1DRB.

2.30.0

- Added "Pass frequency to SUB VFO" right click option in the bandmap.
  Works only with FT-1000-MP for now.

- Bugfix: "band" and "power" information of the CATEGORY field of an
  imported Cabrillo file are now optionals for the MULTI-*
  categories. WT will assume that band is "ALL" and power is "HIGH"
  if these informations are missing. Tks M0CLW.

- Bugfix: Related only to the DXPedition mode: when setting another
  key than SPACE for switching to INFO field (e.g. TAB), one still
  cannot use a SPACE caracter as part of the INFO message
  (e.g. "OP JOHN"). As soon as SPACE is typed, cursor switches back
  to CALLSIGN field. Fixed. Tks F5JSD.

- FM is now allowed in DXPed logs, HF and VHF. Tnx DJ5MW.

- Mode is now displayed in the VHF DXPed log.

- Local and full announcements are now displayed in the gab window
  (Alt-G) if the text contains your callsign.

- CQWW WPX : The offtime lines of the Cabrillo files are now removed.
  Tnx F5CQ.

- EU Sprint : The default CW messages are now compliant with the rules.
  Tnx F5CQ.

- Bugfix : In VHF DXPed, bands higher than 5700 were not displayed in
  the summary wnd (Alt-S).

2.29.1 (Mar 24, 2006)

- When op is populating the bandmap (Ctrl-Enter), new option to only
  clear the log fields if it is a dupe. See the bandmap properties
  dialog. Note : The old setting is cleared and deprecated.
  Tnx OH2UA.

- If a network error is detected (different network versions, etc...),
  the station name which detected the error is now displayed in the
  error alert. Tnx DL5MLO.

- Bugfix : RDXC scoring : UA2 stations and R1ANF are now credited
  with 10 pts (and double mult). Tnx HB9CZF, I2WIJ and RW1AC.

- Bugfix : Cabrillo import : RDXC serial numbering was failing.
  Tnx DL6RAI @ DQ4W

- Bugfix : In VHF contests, callsigns weren't displayed in the DX
  Announcements window (Alt-A). Tnx DK5TX.

- Bugfix: wtCom.dll was messing up with zillion of debug Message
  Boxes. Fixed.

- Bugfix: FT-900 was not working. Many tks to OE3KLU and EA5FV.

- Bugfix: WT was unstable as soon as a Sophos antivirus was running
  on the computer. Fixed. Tks DL6RAI.

- Bugfix: Configuring the interfaces twice with no contest opened
  was getting WT unstable. Fixed. Tks DL6RAI

2.29.0 (Mar 17, 2006)

- Mixed-mode compliant in SO2R mode with no radio connected. Tks
  HA1AG.

- Added FlexRadio SDR-1000 (tks KG4RZY) and Elecraft K2.

- Russian DX Contest : MO2T (aka Multi-2) category added. Tnx F5IN.

- Russian DX Contest : In MOST and MO2T categories, serial numbering
  per band implemented, now allowed in the rules.

- File management errors processing strengthened. Tnx DL6RAI.

- Bugfix : Bandmap list view : Guessed exchange was not displayed
  even if the option was enabled.

2.28.0 (Feb 22, 2006)

- Added IC-7000 support.

- The WinKey PTT of the EZMaster does now work as well even when using
  the internal Win-Test CW keyer. Tks OH2UA/CU2A and I4UFH.

- New setting in Options / Spots warnings to get a warning when you're
  spotted.

- Self-spot detector enabled.

2.27.0 (Feb 18, 2006)

- Improved a bit WinKey when the "independent speed" is not enabled.

- New European Generic 50/70/VHF/UHF (without mult) contest added.
  Tnx G4BUO.

- New European Generic 50/70/VHF/UHF (mults = gridsquares) contest
  added.

- Sked window code totally rewritten. It now has the same look'n feel
  as the other child windows, with the font options etc...

- Skeds are checked against each entered QSO, and deleted if needed.
  Tnx DL8WAA.

- A warning is now displayed 5 mins before a sked (and the sked window
  pops up if it was closed), or when a station is passed.

- The spot bandwiths for each mode are now adjustable in the Properties
  dialog of the bandmaps. Tnx DL6RAI, DK4YJ and several others !

- Keyboard mode (Alt-K) : Alt-K (or Return/Enter) now closes the dialog,
  The Escape keys stops transmission, and Alt-F9/F10 (speed down/up)
  are allowed. Tnx DK4WA.

- Bandmap window : In the graphical view, display options added to
  show headings (LP is optional). Tnx YT1XX.

- Validity controls strengthened in callsigns and frequency edit
  fields.

- Bugfix: In SO2R avanced mode, changing the active scenario using
  AltGr + number was getting the logged callsign wiped out. Fixed.
  Tks OH2UA.

- Bugfix : PACC contest : QSO are now allowed only once per band.
  Tnx DK2PH.

2.26.2 (Feb 11, 2006)

- PACC Contest implementation rewritten to fit to the current rules.
  Tnx F5IN.

- Bugfix : On file opening, the CheckPartial wnd (F12) wasn't properly
  sized. Tnx F5TVL, F8DBF.

2.26.1 (Feb 10, 2006)

- Notice for EZMaster users: this version best works with at least
  firmware 1.37.

- Bugfix: LPT address port was always 0x378 regardless the address
  defined in the LPT configuration dialog. Tks YT1XX/YT5T.

- Bugfix : PACC Contest was broken. Tnx DM9CM.

- Bugfix : Graphical resources leak found in BandMap windows code, which
  could lead to unexpected bahaviour in tight environments (especially
  under Win98). Tnx F6HJO and ON5GQ.

2.26.0-beta (Feb 3, 2006)

- FOC Marathon added. The associated database is FOC_MARATHON.DTB.
  Tnx EI5DI, SM6BGA, G4BUO

- Bugfix: The internal voice keyer was not working properly until the
  "CW and PTT (pin 17 and 17)" option was ticked in the "LPT1
   properties" dialog box. Tks G4BUO.

- Bugfix: Cabrillo import module for the ARRL Sweepstakes was missing.

- Bugfix: Using the * key to swap active radio when TXing was
  delayed. Tks F8CRH.

- Bugfix: With an EZMaster used in CW, the ESC key was not reverting
  the headphone status to the initial value. Tks G3BJ and F8CRH.

- Bugfix: the halfspace character (^) was not working with WinKey.
  Tks OH4JFN and K1EL.

- Bugfix: Pressing the frontpanel A/B button of the EZMaster is now
  detected by Win-Test. Tks F5TNI.

- Pressing ESC in the advanced SO2R "Alternate CQ" scenario now
  switches back as active the radio primary radio. Tks F5TNI.

- Bugfix : The SSB VuMeter works again.

2.25.0 (January 20, 2006)

- NAQP added.

- Operating time added in the summary file, and in the "Copy as text"
  contextual menu item.

- Language : After changing language you can ask Win-Test to restart
  automatically.

- Bugfix: Iambic A and Iambic B settings were swapped over in the
  Winkey configuration dialog box. Tks G0OPB.

2.24.0 (January 13, 2006)

- NRAU Baltic Contest added. The associated database is NRAU_BALTIC.DTB.
  Tnx SM0W and SM3CER.

- HA DX Contest added. Tnx F5IN and HA1TJ.

- DXped HF and VHF : Objectives files features disabled.

- Network : WT now warns when a new computer on the network is not set
  in the same mode category (CW, Phone, Mixed, etc.) as the others.

- SSB VuMeter : You can now modify its size by using the usual
  Ctrl + MouseWheel. Totally useless, but funny !

- WinKey is now calibrated. That would get the speed of the generated
  CW more accurate.

- Bugfix : CW half abbreviation : Only the leading zeroes are translated
  to T signs. Tnx G4IRN.

- Bugfix : RSGB AFS : The contest name in the Cabrillo file (and the
  summary) was wrong. Tnx G4IRN.

- Bugfix : Contests of the month filter was not working as expected.
  Tnx GM4AFF and F5VIH/SV3SJ.

- Bugfix : Displaying the marks of the zone window (Alt-Z) was leading
  to a major crash.

- Bugfix: Some IC751/761/781 was not getting frequency from the radio.

2.23.0 (January 4, 2006)

- German language added. Special thanks to Ben, DL6RAI, who provided
  the translation into German!
  NB: some texts might still appear in english. This is mainly
  because we are not 100% synchronized between the developement steps
  and the translation. Thank you for your comprehension!

- RSGB Affiliated Societies Team Contest added. Tnx M0CLW.

- DARC 10m contest added. Tnx DJ5MW.

- Added Alpha Power Amplifier band change control (Alpha 87A) through
  the serial port. Tks NT1Y.

- N+1 check algorithm speed dramatically improved.

- Contest settings dialog : "Contests of the month" checkbox added.
  When creating a new contest file, and if this box is checked, the
  contest list is build with contests which take place in the
  current month. Tnx F1HAR.

- DXPeds : Summary QSO count columns enlarged to allow more than
  99 999 Q per mode ! Should be enough... Tnx F5JSD.

- Bugfix : The AGCW.DAT and AGCW_HNY.DTB files were outdated. These
  files are now updated, and available on our usual download
  directory :

  http://download.win-test.com/databases/

  Tnx DL6RAI for building these files.

- Bugfix : AGCW HNY contest : The "DX" exchange in the contest settings
  dlg is now accepted and considered as "Non-member". Tnx DL6RAI

- Bugfix : In some screen resolutions, the sked dialog (Alt-E) was
  not properly displayed.

- Bugfix : Callsigns including a "?" were accepted by mistake.

- Bugfix : DARC Xmas : A station now counts only once per band.
  Tnx DJ5MW

- Bugfix : Set date/time QSO dialog data validity strengthened.

- Bugfix : The RAEM callsign is now considered as valid.

2.22.0 (December 21, 2005)

- AGCW Happy New Year contest added. Needs the AGCW.DAT file. The
  associated database is AGCW_HNY.DTB. Tnx F5TNI, F5IN & OM7ZZ.

- Russian 160m contest added. Tnx F5IN and RU3AX.

- DARC Xmas contest added. Needs the DOK_XMAS.DAT file. Uses the
  WAG_DL.DTB database. Tnx DL6RAI.

- Added a DXPedition mode for VHF and above.

- EU Sprint and DARC Xmas contests : The stats window is limited to
  one day only. Tnx DL6RAI.

- Added an option to show/hide an "Info" field for the DXPedition
  mode. That can be useful to enter such miscellaneous informations
  like the operator's name or QTH.

  See in the "option" menu. The operator can select which key
  can be used to access this field between SPACEBAR, "<" (or ">")
  and TAB. The "<" and ">" keys are actually always active.

- Stew Perry contest : The points column header was named "Mult"
  instead of "Pts" by error.

- Bugfix: IC751/761/781 was not getting frequency from the radio.
  Tks I4UFH.

- Bugfix: with old Icom radios, it is necessary to send the MODE
  change before the FREQUENCY change for QSYing on a new frequency
  from the software. Tks I4UFH.

- Bugfix: the position of the cursor in a field was not memorized
  when pressing the space bar to switch to the next field. Fixed.

- Bugfix: In SO1R technique, SHIFT F1/F2/... commands were routing
  the messages to the secondary radio which is of course not correct.
  Fixed. Tks I4UFH.

- The summary broadcasting frames now contain a transactionID to
  maintain consistency among all the received frames for the client
  applications. The specifications of these frames have been updated
  in the document located here :

  http://download.win-test.com/utils/SummaryBroadcastingSpecs.txt

  A new network version (1.10) has been then released.

- The summary SCORE frame now includes the TIME-ON value, expressed
  in minutes. See the new specs in the link above.

- WAG Contest : Databases associated with this contest have been
  created :

  - WAG_DL.DTB for the German side of the contest
  - WAG_DX.DTB for the DX side of the contest

  These databases are available in the usual directory :
  http://download.win-test.com/databases/

- DXPed mode : The CheckCountry window (F10) now displays the current
  country status on other bands. To check if the current callsign
  has been worked on the other bands and modes, use the CheckCallsign
  window (F9). Tnx F5JSD.

- CheckCallsign wnd (F9) : Worked bands and modes count of the current
  callsign is now displayed in the top-left area of the window.

- Log window : After using the tab key to jump to the sent RST,
  the cursor is now positionned on the S part of the report.

- CW : SmartCorrection : If the modified suffix has one letter only,
  the whole callsign is sent. Tnx ops @ TM2Y.

- CW : SmartCorrection : If the original and the modified suffixes
  both include "/" characters and they only differ after the slash
  character, this remaining part will be sent.

  Ex : Original = SP1AAA/2 - Modified = SP1AAA/3 => "/3" will be
  sent only.

2.21.2 (December 9, 2005)

- Bugfix: with WinKey, in either SO1R or SO2R technique mode, the +/-
  signs in CW messages were not managed as expected. Tks M0CLW!

2.21.1 (December 9, 2005)

- Bugfix: the + and - signs were increasing/decreasing the CW speed
  by 2 WPM rather than by 4. Fixed. Tks M0CLW.

- Bugfix: MKSWAP and MKREVERSE renamed WKSWAP and WKREVERSE. Tnx I4UFH.

- Bugfix: the pot speed changes with the EZMaster WinKey were not
  working as expected for the paddle. Fixed. Tks G3BJ.

- Import dialog : The wtb file name is now automatically filled (if
  empty) with the selected Cabrillo (or Editest) file name. Tnx DL6RAI.

- Merge dialog : After adding a file to merge, the add file dialog
  is set to the last used directory.

- Added the wtfra.dll language file in the distro which contains the
  French translation. English is now included in the main core and the
  wteng.dll file is not needed anymore.

2.21.0 (December 8, 2005)

- Bugfix: in ARRL Sweepstakes, pressing the TAB key issued in a
  software crash. Fixed. Tks N3KS.

- When the software is sending a CW message with $spacebar on radio 1,
  the software was actually "pressing spacebar" in the Secondary Radio
  window if SHIFT is pressed ("Shift Binds to the Secondary Radio"
  feature). Fixed. Tks OH2JFN.

- Bugfix: setting SO1R Technique after either SO2R or SO2R Advanced
  has been used was not resetting the scenario macros. Fixed.
  Tks I4UFH.

- Added 4 new COM ports, which now changes the number of supported
  COM ports up to 12.

- Added a tool for checking the log against the QSO worked on the
  multiplier station which are not Mults (see in "Tools" menu)!

- CW speed is reset to the current value at the beginning of
  each message.

- Bug fix: PTT delay in WinKey was 10 times longer than expected! Tks
  OM7ZZ.

- Rewritten part of the WinKey API. This is intentended to fix the
  speed variation problems. Tks GM4FDM, G5W, HB9CZF, OM7ZZ, W4TV.

- Added an option in the "WinKey Properties" window to swap paddles.
  One can also use the text commands "MKSWAP" or "MKREVERSE" in the
  callsign field to swap the paddles on the fly. Tks TM2Y, M0CLW.

- Bugfix: Latch mode with EZMaster was not working in CW. Fixed. Tks
  G3BJ and OH2HU.

- The QSY and mult checks dialog windows are now modeless, which allows
  to modify QSO while the report is displayed. A double click on a
  report line moves the log to the offending QSO and you can edit it.
  A subset of shortcuts is also allowed (namely Alt-F1/F2, Ctrl-F1/F2,
  Alt-Y and Alt-F).

- ARRL 160 : Stats window (Ctrl-F9) now displays three days instead of
  two. Tnx F5IN.

- ARRL 160 : The associated databases names are now :

  - ARRL_160_DX.DTB for the DX side entries stations
  - ARRL_160_USVE.DTB for the US and VE entries stations

  Tnx F5IN for the creation of the current bases.

- ARI 40/80 meters contest added. The associated database is ARI.DTB.
  Tnx IZ7AUH. [Note : It is a domestic Italian contest only]

- UFT HF contest added. Needs the UFT.DAT file. The associated database
  is UFT_HF.DTB. Tnx F5IN and F6ENO.

- The Alt-F4 feature (to return to the last CQ freq) has been modified
  to be compliant with mixed contests.

- Bugfix : ARRL 160 : Dupes count was always 0 in the summary window
  and in the summary file. Tnx F6FGZ.

- Bugfix : Callsigns including a decimal point were accepted by
  mistake ! Tnx F6DZS @ TM2Y.

- Bugfix : The tooltip windows do not display buttons in the windows
  taskbar anymore.

- Bugfix : Summary broadcasting periodicity value was wrongly saved in
  the ini file.

- Bugfix : 4U50VIC was considered as OE in CQWW.

2.20 (November 18, 2005)

- ARRL Sweepstakes added. The precedence is determined according to
  the operating class. The section must be entered in the Exchange
  field.

- New export function in the MAKELOG dialog to make plain text exports
  files. The options dialog allows to choose the fields and to order
  them. You can also choose to mark (with a "-" char) the empty data
  fields. This can be useful when processing the file with a (g)awk
  script. You can also optionnaly set a comma as the decimal separator
  (for French users).

- New export function in the MAKELOG dialog to make CSV (Comma Separated
  Values) exports files. The options dialog allows to choose the fields
  and to order them. You can also choose to include an header line with
  fields titles. You can also optionnaly set a comma as the decimal
  separator (for French users).

- Summary broadcasting on the network can be enabled in the summary wnd
  (Alt-S) contextual menu. You must have enabled the time distributing
  (ie being the "time master") to allow the summary broadcasting. This
  allows other applications to get the current score in real time and
  upload it on the Internet, or other. The complete specifications of
  the UDP frames regarding this feature will be available soon !
  Tnx DJ1YFK and G0WWW.

- Bugfix: scrollbar in the Packet Window (ALT+O) fixed when more
  than 32767 lines are displayed. Tks FY5KE.

- Added a tool for checking the log against the QSY violations.
  Available for multiop stations according to the rules in
  Tools menu.

- Bugfix: Reverse database lookup of gridsquares is working again
  with the V/UHF contests. Tks DL8NAS.

- Bugfix: polling timeout increased with IC-751. Tks I4UFH.

- REF 160 m added.

- CIS DX Contest added. Needs the CTY_CIS.DAT file. Tnx F5IN for his
  precious help !

- CW Speed can be set down to 12 WPM. Tks DK4VW.

- Spots (Alt-A) and Bandmap windows : The callsigns of the spots you
  entered yourself are now prefixed by a tilde (~) character. Tnx M0BBB.

- RSGB 21/28 MHz Contest added.

- SAC : Scandinavian side : Mult wnd (Alt-M) : The "Copy as text"
  function is now working. Tnx OH2UA.

- Bugfix : WAG Contest : From domestic side, the DOK starting with
  numbers (like 45DTK, 25IBB or 25SR3) were reformatted as serial
  numbers. Tnx DL6RAI

- Bugfix : WAG Contest : From domestic side, the "Guess Exchange"
  function failed for the log, the CheckPartial and N+1 windows.
  Tnx DL6RAI.

- Bugfix : Ratesheet (Ctrl-F9) - Objectives tab. In some conditions,
  the compared points graphical representation was out of range.
  Tnx I4UFH

2.19.7

- Bugfix: Total points was wrong in the IARU R1 FD RSGB. Tks G0VGS.

2.19.6

- Bugfix: Cabrillo file generation was broken. Fixed. Tks I4UFH.

- IARU R1 FIELD DAY RSGB: removed 160.

2.19.5

- Bugfix: restoring a QSO manually deleted by the operator is not
  possible. Nevertheless, the "Restore QSO" option of the "Edit" menu
  was still active. Tks F6GNZ.

- Bugfix: RSGB FD R1: fixed the scoring. Tks EI5DI, G0VGS and
  M0CLW. BTW, don't forgot to tell that you are /P in the
  callsign field in the contest setting dialog window.

- Alt-F4 : When returning to your last Run freq with Alt-F4, all edit
  fields are cleared. Tnx F5IN.

- Your club name can now be specified in the contest parameters dialog.
  It is included by default in the Cabrillo file. You can exclude it
  in the Cabrillo options dialog (useful when your club is not
  affiliated to the ARRL and you submit an ARRL contest log).
  Tnx DL6RAI.

- Bugfix : The "Swap radios" menu wasn't working even if its
  shortcut (*) was. Tnx OH2UA.

2.19.4 (August 26, 2005)

- WAE contest: arrow-keys navigate between the lines in the QTC
  Receive window. Tks DJ5MW and DL3NCI.

- WAE contest: keyboard shortcut added on the "To station" button
  (Alt+S) and on the "QTC" (Alt+Q) button. Tks DL3NCI.

- WAE contest: bugfix: when within the QTC receiving/transmitting
  window the Alt-K keyboard CW was broken. Fixed. Tks I2WIJ.

- WAE contest: bugfix (DX side): in certain conditions, a QTC was
  sent twice. Tks DL1MGB and the BCC team @A61AJ.

- WAE contest: bugfix (DX side): in certain conditions, the counter
  for total QTCs available on stock was out of sync. Tks DL6RAI and
  the BCC team @A61AJ.

- WAE contest (DX side): The QTC group numbers which was sent
  before are now visible in the "QTC transmit" window. Tks DL6RAI
  and the BCC team @A61AJ.

- Added a way to swap the frequency of radio 1 with the frequency
  of radio 2. See the menu "Swap frequency of both radios" in the
  "Command" menu, or use the text command "SWAP" in the logged
  callsign field. Tks CT1BOH.

- YO DX Contest : QSO with own country is now credited with 1 point
  (2005 rules change). Tnx ON5GQ.

- Packet commands dlg : All typed commands are stored in a buffer. You
  can recall up the last 10 sent commands by using the up and down
  arrows keys.

- Bandmap wnds : WAE contest : New options to display available QTC in
  both tabs. Tnx DK4YJ and DL3NCI.

- Bandmap wnds : Dupes and invalid callsigns are displayed in bold
  italics font when either VFO is right on the freq. Tnx OK2FD.

- Log edit fields : Feature request #39. When a question mark
  character ('?') is entered in an edit field, the cursor will be
  automatically positioned to this character when moving to this field
  by spacebar or tab or ">". Tnx I4UFH.

- Bugfix : In Multi-Op setup some windows weren't updated at once when
  a QSO came from the network. Tnx DL6RAI @A61AJ.

- Bugfix : Rate wnd (Alt-R) : WAE contest : Pts per QSO and pts per
  mult were wrong. Tnx OK2FD.

- Bugfix : In the ARRL U/VHF and CQWW VHF contest, using the all modes
  category was leading to a major crash. Tnx K1EP.

2.19.3-beta (August 12, 2005) [Not released]

- WAE contest: bugfix (DX side): it is not allowed anymore to send
  QTC on dupe QSOs. Tks BCC team @A61AJ.

2.19.2-beta (August 11, 2005)

- WAE contest: in ALT-L window "QTC Receiving", hitting ENTER (CR)
  on the last raw of the table was sending TU and close the
  window. It is now necessary to explicitly validate the QTCs. That
  way, the operator can have a last check before closing the window.
  Tks I2WIJ.

- WAE contest: bugfix: when you type ctrl-enter (by accident) while
  the QTC-window is open, the window closes itself and all QTCs go
  into nirvana. Tks DJ5MW.

- WAE contest: bugfix: QTC groups was not managed properly through
  the network. Tks DL6RAI and the BCC groups at A61AJ.

- Main wnd : New options in the Options / Log display / Headers
  sub-menu to set left or centered alignment. Tnx G0VGS.

- Main wnd : Spots warnings : New option to hide dupes and invalid
  callsigns.

- EU HF Championship : Band changes (including mode changes for the
  Mixed category) are now displayed in the Rate (Alt-R) wnd. Tnx M0CLW.

- CheckPartial (F12) wnd : New options in the contextual menu to allow
  one to start searches when two chars only are entered in the callsign
  field. You can also use this feature for searching in-log calls only,
  too. Tnx HB9CZF and G4BUO.

- RDA Contest : The packet data stream is now parsed and any valid
  RDA ref. specified in the comment area is taken into account for
  multiplier checking.

- Bugfix : IOTA Contest : The warning message located beneath the
  callsign field for a new IOTA extracted from the packet stream
  announced "New country" instead of "New IOTA". Tnx F5JSD and M0CLW.

- Bugfix : RDA Contest : Summary wnd (Alt-S) : The avg pts column was
  too narrow to display numbers >= 10.00.

- Bugfix : EU HF Championship and REF Contest : The 00 multiplier
  was no more considered and displayed as worked in the "Zones"
  wnd (Alt-Z).

2.19.1-beta (August 1st, 2005)

- WAE contest: added more information on the QTC status in the second
  warning line (below the log). Tks DL6RAI.

- WAE contest: in the Alt+L QTC window, the lines which correspond to
  the QTC counts that are going to be received (according to the group
  of QTC entered by the operator) are now colored in a light green.
  This will help the operator to see when he logged all the QTC,
  especially when the group of QTC is not 10.
  Tks I2WIJ.

- WAE contest: Option | WAEDC: added an option to display more
  informations about the QTC status in the second warning line below
  the log. Tks DL6RAI.

- WAE contest: some modifications in the Alt+L window. Added the
  CW variable $GRNR (send gr/num of the received QTC) *only* available
  for the messages of the ALT+L window. NB; these messages can be
  changed in the WT.INI file if necessary. Tks I2WIJ.

- CW : $SERIAL now sends the previous serial number only when the
  callsign *and* the rcvd report (*and* the extra info if relevant)
  are all empty. Tnx HB9CZF.

- Bugfix : Solar data : When asking WWV or WCY data from DX cluster
  with SH/WWV or SH/WCY commands, only the current day was considered.
  Tnx F1HAR.

- Bugfix : IOTA Contest : Summary wnd (Alt-S) : The avg pts column was
  too narrow to display numbers >= 10.00.

2.19.0-beta (July 20, 2005)

- Bugfix: bugged epilogue detection in EZMaster fixed. This will speed
  up radio polling. Tks I4UFH.

- WAE contest: when a station is a new mult the program now says
  "new country" instead of "new prefix" for DX side participants.
  Tks DL1MGB.

- WAE contest: the message "QTC OK" is now replaced by "QTC needed"
  or "QTC available". Tks DJ5MW.

- WAE contest: available/needed QTC is now displayed even if the
  logged callsign is a dupe. Tks DJ5MW, DL1MGB.

- WAE contest: added a confirmation popup window to ask the
  operator if he's really sure to abort a QTC series.

- WAE contest: bugfix: when operating DX-side, logging a non EU
  station was messing up the internal QTC database. Fixed.
  Tks DL1MGB and DL6RAI.

- WAE contest: the transmitted QTC number can now be changed on the
  fly in the "Transmitting QTC" dialog box, just clicking on the
  "QTC" button. Tks DL1MGB, DL6RAI.

- WAE contest: while transmitting the QTCs, [INS] is now additionally
  moving down to the next QTC line so that when a QTC is confirmed by
  the receiving station, you just press [INS] again to continue.
  When all QTC are sent, pressing again [INS] will send the [+]
  message (TU) and validate. Tks DL6RAI.

- WAE contest: added a "S" shortcut in the "Choose the desired
  number of QTC you want to send" (CTRL+L) window to "Show (only)"
  the QTC with a station. That way, you can check or reopen the
  "Transmit QTC" window for a station even if there is no more
  QTC available with this station. Tks DL6RAI.

- RateSheet (Ctrl-F9) : WAEDC : Two new data types can now be displayed
  in the data and objectives tabs : "QSO + QTC w/ dupes" and "QSO + QTC
  w/o dupes". Of course, they are only available within a WAEDC log.
  Tnx DL6RAI.

- Text commands : RELOADNOW and REOPENNOW added. They mimic the RELOAD
  (or REOPEN) commands, but do not display the contest configuration
  dialog.

- DX cluster dlg : Alt-T : Feature request #40: You can now choose the
  DX cluster type you're connected to with the Options / DX cluster
  shortcuts / Syntax menu items. The syntax of the sent ommands with
  the shortcut buttons will be adapted accordingly. Tnx I4UFH.

- DX cluster dlg : Alt-T : You can now set the spots count for all
  band shortcuts buttons with the Options / DX cluster shortcuts / Spots
  count menu items.

- DX cluster dlg : Alt-T : You can now set the solar informations count
  for WWV and WCY shortcuts buttons with the Options / DX cluster
  shortcuts / Solar infos count menu items.

- Reverse zone check (Shift-F10) : Feature request #52 : When it is
  applicable, the DXCC countries having the specified zone in the
  callsign field are displayed in the first line of the window. Note
  that "official pfx" only are displayed (and not the exceptions).
  Tnx I4UFH.

- Text commands : Feature request #43 : You can now enter the kHz only of
  the current band. To avoid conflict with band changes, you can set
  the priority to the band or the frequency.

  Example : You're on 20 meters, and enter "15" (Enter).

  - If the priority is set to the band, you will QSY to 15 meters. To
    move to 14015 you can use "015" or "15." (Enter).
  - If the priority is set to the freq, you will move to 14015. To QSY
    to 15 meters, you can use "15M" (Enter).

  To set priority, use the Tools / Entering data / Priority menu.
  By default, the priority is set to the band. Tnx I4UFH.

- CW : You can now enable or disable the call correction when validating
  with the Options / CW / Correction / Disabled menu, or by using the
  CORRECT or NOCORRECT text commands. By default, the call correction
  is enabled. Tnx DL1MGB.

- CW : Feature request #47. Smart call correction introduced. It can be
  enabled with the Options / CW / Correction / Smart correction menu,
  or by using the SMARTCORRECT (or SMART) or NOSMARTCORREC (note the
  missing trailing T) (or NOSMART) text commands. This feature has to
  be improved, especially for complicated callsigns like G/F6FVY/P,
  or SP1ABC/M/2 etc... By default, this feature is disabled. Tnx OH4JFN.

- Network : INVENTORY (or INV) text command added to request all
  connected WT to send their version number. Additionnaly, the
  propagation delay is calculated and displayed.

- Bugfix : General : When Win-Test was started with no log opened, many
  (if not all) keystrokes were leading to a major crash. Tnx DL6RAI.

- Bugfix : CW : Internal keyer : Bug report #51. Half baud gap
  insertion (the ^ character) code revisited. The ^ char now pauses
  during one 1/2 dot duration. You can now chain several ^ characters
  if needed.

  Ex : "AA" leaves a standard 3 dot long pause between the two A's.
  "A^A" leaves a 3.5 dot long pause.
  "A^^A" leaves a 4 dot long pause, etc...

  Tnx OH4JFN

- Bugfix : IOTA Contest and several other contests : QSO logged with
  your own callsign gives no more credit points.

- Bugfix : Notes : Alt-N : If you entered a note on a blank QSO line,
  the note was attached to the previous QSO. Now, it is attached to the
  last QSO *you* worked. Tnx TM0HQ.

- Bugfix : IARU Contest : Bug #44. Points credit miscalculated when
  working your own country, but with different ITU zone. Tnx KD6WW.

- Bugfix : Opening an incompatible contest type log in a networked WT
  might lead to a major crash.

2.18.3 (July 10, 2005)

- Bugfix : IARU HF : QSO logged with your own callsign gives no more
  credit points.

- Bugfix: flood on the COM port when used to connected a packet radio
  TNC.

2.18.2

- Bugfix: HQ release (internal). Tks F8CRH.

- Solar activity window : You can now open or close all charts in a row
  by holding the Shift key down while clicking on one of the handles.

2.18.1 (July 3, 2005)

- Bugfix: the Antenna relay outputs (BDC) on each of the W5XD keyer
  DB25 terminals were inverted between Radio Left and Radio Right.
  Fixed. Tks VE3EY, F6IFY and F8CRH.

- Bugfix: wrong buffered speed handling with WinKey. Fixed.
  Tks OM7ZZ.

- Bugfix: pressing F5 ($LOGGEDCALL variable) was not working
  properly with WinKey. Fixed. Tks GM0VRP and GM4FDM.

- Bugfix: the advanced SO2R mode was not working as expected. NB: The
  $TR1 and $TR2 variables are not supported yet with the MK.
  Tks F8CRH.

- Bugfix: again a problem with IC-735. Tks G3SQX and DL2LAR.

- Bugfix : Alt-P (Private gabs) may be sent to the wrong station if the
  status window (Alt-J) was sorted by freq. Tnx F6FGZ.

- Bugfix : After a double click on a station name in the status window
  (Alt-J) and sending a private mail, WT sometimes crashed.

- Back Office : In floating windows mode only, and under some
  circumstances,the contextual menus openings sometimes failed. New
  experimental code introduced.

- Bugfix : ARRL V/UHF contests : Grabbing spots was leading to a major
  crash.

- RAC Contests (Canadian Day and Winter) : CY0 and CY9 stations weren't
  considered as Canadian stations.

- CW speed dialog (Alt-V) : PgUp and PgDown arrows increase and decrease
  CW speed by 2 wpm increments. Up and Down arrows increase and decrease
  CW speed by 1 wpm increments.

- Bugfix : Check partial window (F12) : Under special circumstances,
  the "In log only" option failed. Tnx G4BUO.

- Bugfix : IOTA contest : It was not possible to edit the serial number
  sent.

- IOTA contest : The packet data stream is now parsed and any valid
  IOTA ref. specified in the comment area is taken into account for
  multiplier checking. Tnx ON6QR.

- Bandmaps : IOTA contest : New IOTA are now displayed in green color.

- Bugfix : The CONTEST-NAME Cabrillo line in the RSGB IOTA contest was
  mispelled. Tnx F5VIH/SV3SJ.

- Bugfix : The CW text commands introduced in 2.3.0 (NOCUT, SEMICUT,
  FULLCUT and PROCUT) didn't work anymore. Tnx F5HRY.

- REF DDFM 50 MHz : Mult indicators field now displays new gridsquare (L)
  and/or new French dpt (D).

- Text commands : MAKELOG added. Equivalent to WRITELOG.

- Bugfix : REF DDFM 50 MHz : Claimed score in the REG1TEST .EDI output
  file was not correct. Tnx F4EGZ.

- Bugfix : REF DDFM 50 MHz : The French dpts window (Alt-Z) was 0-sized
  and empty.

- Bugfix : REF DDFM 50 MHz : The ADIF output file export failed.

- Bugfix : ARRL 10m : The ADIF output file was reporting empty
  gridsquares (irrelant in this contest), and bad sent reports if
  you were located in the US/VE side.

- Checkmult (F10) and checkcall (F9) windows :If the
  Tools / Exchange guessing menu is set to Automatic or timed out,
  the update settings of these two windows are now displayed as
  "automatic". Tnx OH4JFN.

- Log : Columns headers added. You can hide or display them with the
  Options / Log display / Hide headers menu, or the following text
  commands : NOHEADERS (or HEADERSOFF or HIDEHEADERS) and HEADERS
  (or HEADERSON or SHOWHEADERS). Tnx F6BGC.

2.17.0 (June 9, 2005)

- Bugfix: address was not correct for the Tentec Omni VI. Tks F6IFY.

- Bugfix: DTR handshaking on the serial lines was not working as
  expected. Tks W0RSR.

- Bugfix: when an entry was deleted in the secondary radio window
  with SHIFT+ALT+W, the band was changed by the band of the primary
  radio. The same operation using SHIFT+F11 was working OK. Fixed.
  Tks S51TA, and DJ5MW!

- Added rig Tentec Jupiter. Due to the poor protocol instruction set,
  there is some limitations:
    - split mode is not supported
	- the VFO A is always shown as active in WT, and WT will only
	  control the VFO A
	- there is no way to control the VFO B from the software
  BTW, you will need a 3-wires cable with CTS and RTS connected
  at the radio side.
  Tks W0RSR

- Dupe warning message shortened to be compliant with the log large
  bold font setting. Tnx F5IN.

- ARI Sezioni Contest added. [This contest is only opened to
  I stations]

  A database for this contest has been built and is downloadable
  from our usual directory :

  http://download.win-test.com/databases/ARI_SEZIONI.ZIP

  Tnx IZ7AUH and IZ2EJU.

- CW Prosigns : Prosigns are now allowed in CW messages. They
  are entered as a "&" character, followed by the 2 characters
  forming the prosign. For example : &BK or &VA, etc... All such
  prosigns are supported by the internal and the WinKey keyers.

  For now, the prosigns are not supported on the W5XD Multi-Keyer.

  Tnx IK7JWY. Special tnx to F6IFY and F8CRH for tests.

- Logs : New option added in the output logs configuration dialog to
  write the summary file (.SUM extension). Tnx DL1MGB.

- Text commands : CWABBREV added. Equivalent to CWFULLABBREV.
  Tnx DL1MGB.

- Text commands : RPT and NORPT added. Equivalent to REPEAT and
  NOREPEAT. Tnx DL1MGB.

2.16.0 (June 3, 2005)

- Added rig FT-757GX II

- Various bugfixes using the bandmaps for the secondary radio window.

- Run freq restore (Alt-F4) : A new method has been implemented to
  save the run freq. In the same time, this function has been
  extended to the secondary radio in advanced SO2R
  (with Shift-Alt-F4). Tnx DL6RAI.

- CQWW WPX : Band changes are now displayed for the M/2 category in
  the rate window (Alt-R). Tnx DL1MGB

- Edit keys : Ctrl-A and Ctrl-E mimics the Home and End keys.
  Tnx DL6RAI.

- Log browsing : Ctrl-PgUp and Ctrl-PgDown scroll log in 24 hours
  steps. Tnx DL6RAI.

- Dupe warning : The received exchange is added to the warning text.
  Tnx F5IN.

- IARU Field Day Rgn 1 added : Three flavours of this contest are now
  available : Generic, DARC and RSGB scorings.

  Unfortunatly, there are no well-defined Cabrillo formats for
  this contest and you must check _carefully_ the overlay category
  in the log you submit. Check with your national rules or sponsors.

- Helvetia contest : Cabrillo log format output is now compliant with
  the required definition. Tnx HB9CZF

- Zones window (Alt-Z) : The window title bar now includes the worked
  and the total zones counts. Tnx F5IN

2.15.0 (May 19, 2005)

- Zones window (Alt-Z) : When list permits, you can now display labels
  (mostly prefixes) attached to the provinces, regions etc... Works
  only for current band display. Tnx F5IN.

- Zones window (Alt-Z) : When list permits, you can now display zones
  in alphabetical order. It applies to both views (current band and all
  bands). Tnx 5B4WN/C4W.

- Ctrl + Space grabs spot on the current frequency, if any. Tnx DJ5MW.

- New message variable : $GRABSPOT, which grabs spot on the current
  frequency, if any. Can be used in F4 messages for example. Tnx DJ5MW.

- Web site : Quickstart guides in English and French are updated and
  available in pdf format. Tnx F1HAR.

- Databases : King Of Spain contest database added in the database
  directory (only valid for 2005+ rules).
  http://download.win-test.com/databases/KOS.ZIP
  To be downloaded and manually installed.

- Bugfix : In some circumstances, on XP systems, close, help and scroll
  boxes in the child windows were wrongly positioned. Tnx F1HAR.

- Bugfix : King of Spain contest : Cabrillo files imports failed.
  Tnx F5IN.

2.14.4 (May 5, 2005)

- REF THF Contest: WT is now compliant with the new rules 2005
  (F/TK stations worked from F/TK counts 4 pts/km).

- Bugfix: still a problem with the Split mode on Icom radios with
  double vfo. Fixed. Tks W5GN & EA3IN.

- Bugfix: communication with IC-735 was not working. To be tested!
  Tks DJ5MW.

- Secondary radio window redrawn. Tks CT1BOH.

- Commands (like frequency QSY, mode change, ...) can now be entered
  in the callsign field of the secondary radio as well.

- Bugfix: switching modes with shift/ctrl/F1/F2 wasn't working
  in the secondary radio window. Fixed. Tks DJ5MW.

- Bugfix: in EZMaster, the "control interface of Radio 2" was not
  working until the "control interface of Radio 1" was enabled.
  Fixed.

- For safety reason, bands changing when the transmitter is ON is
  locked by WT. However, if one uses an EZMaster, one can now (in SO2R
  mode) change the band of the radio which is not transmitting. This
  is only possible with an EZMaster because it carries out a check by
  itself regarding this, which makes this handling safe. Tks I4UFH.

2.14.0 (April 14, 2005)

- Bugfix: Main and sub VFOs were inverted in split mode with various
  Icom radio (IC-756Pro, ...). Tks W5GN & I4UFH.

- Added rigs: Icom IC-756proIII, Tentec Omni VI.

- Bugfix: IC756 address fixed. Tks F6IFY.

- YU DX Contest : WT is now compliant with the new rules 2005. Tnx F5IN
  and YT1NT/VA3TTN.

- WPX : Mults Window (Alt-M) : The "copy as text" menu item now works.

- Status window (Alt-J) : You can now display Radio 1 frequencies only,
  to save some screen space. Tnx M0CLW.

- To avoid unwanted behaviour, grabbing a spot from the spot list (Alt-A)
  or the radio bandmaps is now allowed only if the cursor is located on
  the last line of the log. Tnx M0CLW @ G6PZ.

- Radio windows : Spot list tab : Scrolling capability added. Tnx W8JY.

- Bugfix : RDXC : The /MM stations are no more counting for DXCC mults.

- Bugfix : RDXC : Typo in the CTY_OBL.DAT file. UA4C and UA4D callsigns
  were resolved as an unknown "EU" oblast instead of "SA". This file is
  updated in the Win-Test download site, in the /databases directory.

- Bugfix : Mixed category - Networked M/* : After editing a logged QSO,
  the networked stations might get a wrong Rcvd report if they were not
  set in the same mode as the edited QSO. Tnx M0CLW @ G6PZ.

- Bugfix : Mixed category : When grabbing a spot from the radios or the
  spots windows, the default reports were not adapted if required by a
  mode change.

- Bugfix : RDXC : The sent serial wasn't displayed in the log. It was
  very annoying if you wanted to edit it ! Tnx M0CLW @ G6PZ.

- Bugfix : WAEDC : The sent serial wasn't displayed in the log and you
  were not able to edit it.

- Bugfix : DXPed logs : The default CW F2/F3 messages included a $ZONE
  variable which is irrelevant for a DXPed log. Tnx M0CLW.

2.13.5 (Mars 18, 2005)

- Bugfix: Again a split mode problem fixed with the Orion. Tks W8JY & W5GN.

- Helvetia Contest added. Tnx F5IN, F6HJO.

- 9KCC Contest 15m added.

- UBA Spring 80m, 6m and 2m contests added.

- General : In most of the displayed modal dialogs to set parameters
  or options, you can now still use the Fx keys to play messages.
  However, it will not work with dialogs which act on hardware
  (interfaces, etc...). Tnx FY5KE.

- Bugfix: Still some problem with the WX0B interface. Mny tks to S51TA!

- Bugfix: Split mode with the Orion RIG fixed. Tks W8JY and W5GN.

- Split frequency dialog box (-): it is now possible to enter only the last
  digits of the split frequency. For example, entering 249 will get the
  radio programmed to xx249 in the current band. Tks W5GN.

- Bugfix: In some condition, when activating the Automatic CQ repeat mode,
  the keyer was transmitting to the wrong radio. Fixed. Tks GM0GAV.

- Radios windows : New option in bandmap and list displays : You can
  save some screen space in displaying the kHz only of the frequencies.

- Bugfix: the stereo bit available on the LPT1 always remained to 1.
  Tks GM0GAV.

- Bugfix: SHIFT+F<key> (used to play a message to the secondary
  radio) was not working properly with the WX0B SO2R interface.
  Tks S51TA.

- Statistics (Ctrl-F9) and radios windows : A left click on tabs now
  brings these windows to the front.

- Packet window (Alt-O) : You can now set a timeout on the packet data
  stream. If there is no activity after this time, a warning will be
  issued in the main window.

- Radio windows - Bandmaps : A grey marker (same color as the VFO display
  background) is now displayed for the inactive VFO frequency. And if
  it's right on a spot freq, its callsign background is set to the same
  color.

- Bugfix : Internal voiceKeyer : Every Fx message was blocking further
  use of the same Fx message ! Tnx S51TA

- Bugfix : Secondary radio display : The callsign field wasn't correctly
  rendered with small fonts.

- Bugfix : RSGB Commonwealth contest : In some conditions, multipliers
  window (Alt-M) bookmarks didn't work well.

2.12.0 (Mar 11, 2005)

- Bugfix: external voice keyer controlled through the LPT port was
  not working anymore since the advanced SO2R mode. Fixed.

- Bugfix: random program crash when exiting (especially with the
  internal VoiceKeyer activated).

- RSGB Commonwealth Contest (BERU) added.

- REF HF : When working a French overseas station, default exchange
  is now set to his prefix. Tnx F5LIW.

- Kenwood rigs : WT now follows the mode changes for RTTY. Tnx F5LIW.

- Bandmaps and statistics windows display improved to avoid tabs
  flickering with slower machines. Tnx FY5KE.

- Bugfix : A memory leak in graphical objects was leading WT to a violent
  crash under stressed environments (especially Win98). Tnx FY5KE, M0CLW.

- Bugfix : Internal voice keyer : Playing a Fx message which has not
  been recorded caused the voice keyer to hang. You had to stop (Esc)
  the non-existent file (!) to get back control. Tnx F5LIW.

- Bugfix : Bandmaps : In some conditions, callsigns were not displayed
  in the bandmap window. Tnx FY5KE.

- Bugfix : In some conditions, WT was violently crashing when exiting
  (especially with the internal VoiceKeyer activated).

- Bugfix : UBA Contest (Non-ON side only) : Some countries were wrongly
  considered as members of the EEC. Tnx F5IN.

2.11.0 (Feb 28, 2005)

- Bugfix: QSY done on the second radio in SO2R mode was not working
  until at least one QSO is logged.

- Bugfix: Various fixes with the SO2R advanced mode in SSB.

- New "List" tab added in the radios windows to display spots in lists.
  See the appropriate contextual menu for options. You can even sort
  this list by heading (Tnx W5GN).

- A new menu item allows to modify spot callsigns if it is busted. This
  item is available in the contextual menus attached to the spots window
  (Alt-A) and the radios windows.

- Contextual popup menus management modified when using floating child
  windows. Tnx VK6NU.

- Several typos and grammar fixes in the English version. Many thanks
  to M0CLW.

- Confirmation dialog added when deleting a spot.

- Bugfix : In some circumstances, the timestamp of a note was incorrect.

- Bugfix : Sun icons weren't displayed if SR or SS hour was 0000z.

- Bugfix : CQWW 160 : The avg column of the summary window (Alt-S) was
  a bit narrow.

2.10.0 (Feb 22, 2005)

- Something modified in the CW internal generator which might get it
  more accurate. To be tested! :)

- A new tab named Continents has been added to the statistics (Ctrl-F9)
  window. It's available for the HF bands only. Bars and pie charts
  display the percentage of QSOs per continent. Tnx CT1BOH.

- Comments in the spot window (Alt-A) can now be cut to save space
  on the screen. If a comment is longer than the allowed space, it's
  replaced by an ellipsis string. To read the full comment, point on the
  ellipsis and a tooltip will appear.

- In spots (Alt-A), packet (Alt-O) and gab (Alt-I) windows, if the
  scrollbar is not in the downmost position, a small icon is displayed
  in the window title bar. Clicking this icon scrolls down to the last
  line of the window.

- Bugfix : When using the intenal voice keyer, any Fx key was always
  sending the same F3 message. Tnx F5HIJ, F5LIW, EA3IN.

- Bugfix : The image generated by the "Copying as image" menu in the
  statistics window was sometimes broken.

2.9.0 (Feb 17, 2005)

- Bugfix: The cross redefinitions of keys did not work correctly.
  Fixed.

- Bugfix: WinKey version 9 supported. Tks N4ZR. Special thanks to K1EL
  for his kind support!

- SO2R advanced mode for SSB implemented (beta-test). It works in the
  same way as for CW.

- Bugfix: CTRL+RETURN (or CTRL+J) was initializing in an incorrect
  way the QSO.

- A time OFF timer is added to the Rate window (Alt-R). It is reset on
  every entered QSO (matching the set options). You can set the alarm
  time (the background will be bright red after this delay) in using the
  contextual menu.

- GACW WWSA DX Contest added : Tnx LU1DZ (and F5JFU).

- RSGB 80m Club Championship added. Tnx G4TSH.

- DXPedition : The space bar now moves the cursor on the S character of
  the RST received report. Tnx F6GNZ.

- Bugfix : CQWW-VHF and ARRL-V/UHF : Using the Tab key was leading to a
  violent crash in some circumstances.

- Bugfix : KCJ TopBand : The summary window wasn't counting correctly
  the QSO and the dupes.

- Bugfix : The Options/Log/Display spots wasn't considered in the code.

- Back office : The clock and timer above codes are rewritten to lower
  a bit the CPU load. [Experimental]

2.8.0 (Feb 10, 2005)

- Bugfix: mode changes with the Tentec Orion radio fixed. To be
  tested. Tks W5GN.

- Hourly comparison between data and objectives is now available in
  the Objectives tab of the statistics window.

- You can now set an off threshold not listed in the menu choices
  between 1 and 120 minutes. Tnx CT1BOH.

- If a 4-chars valid gridquare is entered in the contest settings dialog,
  WT now warns and offers to complete it with the LL centered sub-square.

- KCJ TopBand Contest added.

- Bugfix : PACC Contest : Being DX, logging a non-PA station was leading
  WT to a major crash in some circumstances. Tnx VK6NU.

- Bugfix : If guessed exchange was displayed in the bandmaps, and if no
  exchange was guessed, an ugly "()" was appended to the callsign.

- Bugfix : PACC Contest : The NH province was not displayed in the
  multipliers window. Tnx F5TJW.

- Bugfix : PACC Contest : Mode category wasn't mentionned in the
  Cabrillo header.

2.7.0 (Feb 7, 2005)

- Bugfix: bandwidth changes problem when frequency is changed with
  the TenTec Orion fixed. To be tested. Tks W5GN.

- Added a way to bind the keyboard entries into the secondary radio
  window with a second footswitch. This works with EZMaster firmware
  1.28 and later. The second footswitch is connected between pin 14
  and GND of the Parallel DB25 port of the EZMaster.

- F5 was not sending anymore the logged callsign in certain
  circumstances. Tks F5TJW and F6IFY.

- Bugfix: adding a QSO logged in the secondary radio using
  SHIFT+CTRL+ENTER or SHIFT+CTRL+J is now working as expected.

- RSGB 160m CW Contest added. Tnx M0CLW.

- PACC Contest added.

- Time ON and time OFF added in the rate window (Alt-R). By default,
  the off threshold is set to 10 minutes. You can set it within the
  attached contextual menu up to one hour by 10 mins increments. That
  parameter means that if this threshold period goes by, WT counts it
  as offtime. In a low activity or VHF contest, you should increase
  this value.

- Guessed exchange can be displayed in the bandmaps (new option in the
  attached contextual menu). Tnx F6BGC.

- Sun status can be displayed or hidden in the bandmaps (new option in
  the attached contextual menu).

- In CQWW 160, when working a non US/VE station, the guessed report was
  not filled. Tnx F5IN.

- In CQWW 160, in SSB mode, the summary window was not counting QSO and
  dupes.

- FT990 code rewritten. Experimental. Tnx F6GOX.

2.6.0-beta (23 Jan 2005)

- Added new shortcut aliases:
  old             new
  --------------- ---------------
  CTRL+BACKSPACE  SHIFT+BACKSPACE
  CTRL+DELETE     SHIFT+BACKSPACE
  SHIFT+F1...F7   ALTGR+F1...F7
  SHIFT+INSERT    ALTGR+INSERT
  SHIFT+PLUS      ALTGR+PLUS
  ALTGR+INSERT    ALTGR+F2 (in phone only)
  ALTGR+PLUS      ALTGR+F3 (in phone only)
  INSERT          F2 (in phone only)
  PLUS            F3 + <return> (in phone only)

- Added the new window "secondary radio", which allows when operating
  SO2R to log the QSO of the second radio without disturbing
  the run.

- The shift key can be used to bind every relevant keyboard entries
  into the "secondary radio". This feature can be enabled or disabled
  in the "Operating" menu (see below).
  The following entries are concerned:
    - letters and digits
	- SPACE, TAB, and editing keys (left and right arrows, delete,
	  backspace, ...)
	- F1...F7, INSERT, PLUS
	- ALT+F1, ALT+F2 (band change)
	- CTRL+F1, CTRL+F2 (mode change)

- New transmission on one radio starts immediatly (CW or DVK),
  stopping transmission on the other radio if necessary.

- Automatic CQ repeat mode supported for primary and secondary
  radio. The EZMaster internal voice keyer is also supported in
  repeat mode.

- Added CW variables $R1R1, $R1R2, $R2R2 which can be entered in the
  predefined CW messages to set the headphone at any moment of
  the transmission.

  $RxRy means: Left ear = Radio(x) and right ear = Radio(y).

- Fixed: serial num sent

- Fixed: INSERT with empty logged call sends the previous logged call on
  the same station

- Added CW variables: $INSERT and $PLUS

- New menu "Operating":

  - "Listen primary radio". Useful to focus the attention to the run
     frequency whereas one was listening the audio split mode.

  - The "Technique" menu lets the operator choose between "SO1R / MultiOp",
    "SO2R" and "advanced SO2R". The other features in this menu will be
	only available according to the selected operating technique.

	  - "SO1R / MultiOp" is for the operators who don't have a SO2R
	    interface

	  - "SO2R" is for the operators who have an external SO2R interface
	    which does not handle audio control by the software.

	  - "SO2R advanced" is for the operators who have connected a
	    next generation SO2R interface which handles full audio
		control by the software, like the EZMaster of
		Hamradiosolutions.

  - The "Modify scenarios" menu entry is reserved for the "SO2R avanced"
    technique, where the operator will define the SO2R behaviours in
	the different scenarios, like "plain pile up", "heavy pile up",
	"alternate CQ", ...

  - The "Shift binds to the secondary radio" menu entry can be
    selected if the operator wants to redirect automatically into
	the "Second radio" window each entered keys if the shift key
	is pressed at the same time.

  - The content of the popup menu "Commands | SO2R" moved into the
    Operating menu. The menu captions also changed a bit (the term
	"non active radio" becomes "secondary radio").

- Any manual change in the audio control setting by the operator will
  stop WT to take control of the audio. This "manual" mode can be
  canceled with the new CW variable "$RESET", or using the menu
  "Operating | Revert to automatic control"

- Any manual change in the audio control settings by the
  operator (pressing AltGr+A, AltGr+T, ...) will stop WT to
  take the automatic control of the audio. This "manual" mode can
  be canceled in the menu "Operating | Revert to automatic control"
  menu or by pressing AltGr+R. It can also be canceled with the
  new $RESET variable in a morse message.

- Shift+numpad number can now be bound to the secondary radio
  window.

- Shift+F12 shortcut (N+1 window) moved to F8.

- Advanced SO2R mode implemented for the internal keyer and
  the Multikeyer (partial support only with the MultiKeyer
  yet).

- Added CW variables: $ALTERNATECQ, $CQ, $TR1, $TR2,
  $MSG1...$MSG12

    - $ALTERNATECQ (or $ACQ): to be used at the end of a CW
	  message in the scenarios to swap primary and
	  secondary radios and send CQ on the secondary radio.
	  The "Alternate CQ" mode automatically stops if the
	  operator logged something on the keyboard. This can be
	  initialized either with AltGR+R or with the variable
	  $RESET.

	- $CQ: same as $ALTERNATECQ but does not swap radios.
	  Usually used at the end of the "TU" message in a
	  "alternate CQ" mode to send CQ on the seconday radio.

	- $TR1: switch to the primary radio during transmission
	  (hot switch). WT takes care of stopping transmission
	  on the secondary radio before switching to the primary
	  one.

	- $TR2: same as $TR1 but for secondary radio.

	- $MSG1...$MSG12: additionnal morse messages (see Alt+C)

	- Aborting a transmitting message with ESC reverts the
	  headphone configuration in its original configuration.

- AltGr + 1...8 can be use to select the active scenario.

- Band changes and mode changes not allowed anymore when the PTT is
  ON. Tks I4UFH.

- The protocol of control of the Icom radios not making it possible
  to know which is the active vfo, the bandmap always displays the
  operating frequency (whatever the VFO on the radio) in VFO A, and
  the VFO B is disabled except in split mode.

- Bugfix: WT was not anymore supporting 2 Icom radios connected at
  the same time. Fixed. Tks F6IFY.

- Bugfix: $SPACEBAR and $GUESSZONE was not working through a
  MultiKeyer. Fixed. Tks F6IFY.

- Polling mode of the rig control improved.

- Removed the popup dialog when recording a voice message through
  EZMaster. Tks I4UFH.

- Parity and Stopbits configuration fixed with EZMaster.

- Creation of new menu "tools", where the following entries have
  migrated in:
  - Exchange guessing
  - Redefine keyboard keys
  - Automatic CQ repeat mode

- The bandmaps are now available even if no radio are connected.

- New feature : Objectives files. (Tnx CT1BOH)

  In the statistics window (Ctrl-F9), there is a new tab called
  "Objectives", which displays the difference between the current
  data and objectives data recorded in an objectives file (.obf
  extension). The red bars indicate you're below the objective for
  a given hour (bad !), and green bars indicate you're above the
  objective (good !).

  The objectives files are textual, which means they can be opened, read
  and created with a basic text editor. The used syntax is very simple
  and flexible :

  Each data line is composed of :

  Hour DataKeyword=DataValue [DataKeyword=DataValue]

  Example :

  12 QSO=500 MULT=10

  which means : The objective for the hour 12 (= at 1259z) is to have
  500 QSO and 10 mults. You can combine any number of data you want
  on the same line or on different lines. The previous line could have
  been written as 2 lines :

  12 QSO=500
  12 MULT=10

  The allowed DataKeywords are :

  - QSO (or QSOS)
  - QSONODUPES (or QSOSNODUPES)
  - DUPE (or DUPES)
  - QTC (or QTCS) [WAE contest only]
  - MULT (or MULTS, MULTIS, MULTIPLIERS)
  - QSOPOINTS (or QSOPTS, QSOSPOINTS, QSOSPTS)
  - POINTS (or TOTAL, SCORE, PTS, PTSTOTAL)
  - AVGPTS (or PTSAVG, AVG, AVGPOINTS, POINTSAVG)
  - KM (or DIST, DISTANCE) [VHF+ contests only]
  - AVGKM (or KMAVG) [VHF+ contests only]

  You don't need to set objectives data for each hour. WT will compute
  the missing hours, if any. There must be at least the final hour data.
  Of course, setting more data hours increases accurancy.

  We assume to get data from hour 0 (objective for 0059z) to the hour
  47 (objective for 2359z the second day). If the contest doesn't last
  48 hours, you can restrict the start and end hours with the following
  syntax:

  START 6
  END 42

  In this example, the contest starts at 0600z (day 1) and the end is
  at 1800z (day 2, thus 24 + 18 = 42).

  You can also specify a graphics title with the syntax :

  TITLE CQWW contest 2004

  which will display "CQWW contest 2004" on the graphics.

  Even if you can manually create and edit the objectives files, we
  also provided an easy way to create objectives files from past WT
  contest files. In the Statistics window, a new item in the contextual
  "Export as objectives file" creates a file from current data. You just
  have to name it, and choose the data you want to be your objectives,
  and optional informations (start and end hours, graphics title). This
  item is also available in the Tools menu.

- The color of each child window title bar can be modified to ease its
  recognition in a cluttered layout. It can also be useful to use the
  same color to group them : General, Packet, Radio1, Radio2 etc...

- The multipliers window (Alt-M) now has bookmarks in its contextual
  menu (if headers are displayed for the contest). You can also use
  Shift + Mouse wheel to browse the bookmarks. Tnx CT1BOH.

- The DX announcements window (Alt-A) can now be filtered by bands. The
  displayed bands setting is recorded in the data log file.

- The default broadcast IP calculation in the Interfaces dialog is more
  accurate.

- In CW Keyboard mode (Alt-K), a Backspace key hit now sends an " E E "
  sign to indicate an error for the last sent character.

- Visibility of the toolbar is displayed and can be modified with the
  Tools / Toolbar menu item.

- Statistics window (Ctrl-F9) now can be copied as text. All data
  displayed in the window after this action will be in the clipboard in
  text and SYLK formats. It means you can paste these data in a text
  document, but also - more useful - directly in a spreadsheet (Excel,
  OpenOffice etc). Click in the top-left cell you want the data to be
  pasted and paste them.

- New item in the contextual menus of Bandmaps and DX spots window
  (Alt-A) to ease spot deletion.

2.5.2 (Dec 27 2004)

- Added menu "Windows | Close all windows" entry.

- Bugfix: A synchronization problem between processes caused
  erratic behaviours in the use of EZMaster integrated WinKey. Tks
  I4UFH of hamradiosolution who provided great support!

- Bugfix: wrong band data output with double-VFO rigs (like FT-1000MP).
  Fixed. Tks I4UFH.

- Abandonment of the CI-V mode with the Icom radios: Win-Test now
  polls the rig to get its operating frequency and mode. The owners
  of Icom radio must remember to disable the CI-V mode on their rig.

- One can now define on which port of the EZMaster are connected the
  radios or TNC. That way, it is possible to connect a RS-232 rig to
  either the COM or the RS-232 EZMaster connector.

- Bugfix: Radio 2 was not receiving rig information through EZMaster.
  Tks I4UFH.

- When the EZMaster WinKey is disabled, Win-Test does now configure
  EZMaster to accept CW on the DTR line and PTT on the RTS line, both
  via the USB port. Tks I4UFH.

- Bugfix: The speed pot changes is now ignored by WT when WinKey is
  disabled in the EZMaster properties window. Tks I4UFH.

- Extended DVK, pin 7 and 8, can now be used. As WT only sends a short
  pulse (100 ms long) to these pins, it is possible to share their
  use with BandData output if the hardware (SO2R interface) supports
  it. It is an option of the LPT configuration window. Tks ZS4TX.

- Added a StereoToggle signal on either pin 9 or 5. It is an option
  of the LPT configuration window. Tks ZS4TX.

- New variables in the CW messages : $SPACEBAR and $TAB which mimic
  a space bar or a tab key hit while playing. And $GUESSEXCH (or
  $GUESSEXCHANGE) also mimics a space bar hit (filling exchange field(s)
  if possible), but the cursor remains in the same edit field. This way,
  you can easily save a spacebar hit by using the following Ins key msg :

  $LOGGED $QSOB4 $GUESSEXCH $F2  (the cursor will not move)

  or

  $LOGGED $QSOB4 $SPACEBAR $F2  (the cursor will move to the next field)

  (assuming the F2 msg contains the exchange message to send).

  Tnx CT1BOH.

- Experimental : Exchange guessing (from the various databases or from
  the previous QSOs worked) can now be triggered in three different ways
  (use the Edit / Guess exchange mode menu item to choose of the three
  options) :

  - After hitting the space key : It was the default mode, and was
    used until this version.

  - After every key hit in the callsign field. Please note, even if
    we tried to optimize at most this process, it is a bit CPU-intensive
	and synchronous to key typing. Old computers users and/or high
	speed typists may experience a slowing down. All reports are
	welcome.

  - After a timeout : For now, this timeout is fixed and set to 1,5
    second. The exchange fields are filled after this timeout of
	keyboard inactivity in the callsign field.

- New contextual menu items in the CheckCall (F9), CheckCountry (F10),
  Multipliers (Alt-M) and Zones (Alt-Z) windows to choose which bands
  to display in these windows. These items are only available for the
  non-monoband contests. This can be useful, for example, if :

  - You are taking part as a monobander in a multiband contest.
    Then, you don't need to waste screen space with the other bands
	data.

  - You are taking part in a multiband contest, but you don't have
    any antenna or equipment on such and such bands : You can then
	hide them in these windows.

  Note that choosen bands are recorded in the data file, and that these
  four windows are all synchronized.

- The CheckCountry (F10) window has been redesigned for VHF+ contests
  Tnx F6BGC.

- Bugfix : Hitting Ins right after a * was sending the wrong callsign
  and, also, the dupe checking failed.

- Bugfix : Stew Perry contest : The CATEGORY: line included an
  irrelevant LIMITED keyword instead of ALL. Tnx F5IN.

- Bugfix : UBA Contest : You were not warned if a new country was
  entered.

- Bugfix : Choosing 'All bands' in the zones window (Alt-Z) might
  randomly lead to a crash. Tnx VE3EY

- Bugfix : In Baltic or ARRL 10 meter contests in mixed category,
  hitting space or tab keys when editing sent report was crashing WT.

2.5.1

- EZMaster is now fully supported in advanced mode. See the menu
  "Options | Configure EZMaster...".

- The "Rate" window (ALT+R) now shows the Paddle Speed of the
  WinKey interface. It is displayed after the WT speed in the
  window bottom : "CW 32/28 WPM" means that the automatic speed is
  set to 32 and the paddle speed is set to 28.
  Tks OM7ZZ, I4UFH,...

- A new setting in the "WinKey properties" window let decide if the
  computer speed and pot are independant. This option can be usefull
  to simulate independant keyer speeds.

- Bugfix: Starting WT, whereas EZMaster was in standard mode, caused a
  blocking PTT to ON. Tks I4UFH.

- Bugfix: EZMaster was sometimes initialized with the PTT set to ON.
  Tks I4UFH.

- Bugfix: The CT-space option in the "WinKey configuration" window
  is now synchronized with the option of menu "Options|CW ".
  Tks F6FVY.

- UBA DX Contest added.

- RAC Canada Winter and RAC Canada Day contests added.

- Using your own callsign in a QSO will now credit no point, and it will
  not be considered for multiplier checks. This QSO will even be tagged
  as invalid. Tnx F8CRH.

- The CheckPartial (F8) and NPlusOne windows can now display the guessed
  zones (or states or provinces... or gridsquares, depending on the
  contest) associated with shown callsigns. Use the right-click on these
  windows to enable this feature. Tnx F6BGC.

- After wiping a QSO (F11, Alt-F8 or Alt-W), the CheckPartial and
  NPlusOne windows are emptied.

- In SO2R mode, radio switching now also switches the content of the
  CheckPartial (F8), NPlusOne, and CheckMult (F10) windows. Some
  other data were not also correctly swapped.

- You can now redefine AltGr keys. Note : As you might know, the AltGr
  key is totally equivalent to Ctrl + Alt pressed together.

- To be compliant with the WinKey syntax, the "|" character is now also
  considered as an half-baud CW space. It works for both keyers (internal
  and WinKey - assuming its firmware version is 9 or later).

- The soapbox edit box is the log export dialog is now limited to 1023
  characters rather than 254. Tnx FY1FL.

- Bugfix : Double-click on a QSO in the CheckCountry window (F10) in
  IOTA contest failed.

- Bugfix : When importing a Cabrillo file, if the soapbox was on several
  lines, the resulting string in the log export dialog was missing
  space characters.

- Bugfix : The CW keyboard mode button in the toolbar was missing its
  text hint.

2.5.0

- Bugfix: WinKey: the speed changes of CW were not taken into account during
  when transmitting.

- Bugfix: In SO2R, the mixed mode (a different mode by radio) was not
  correctly managed.

- First step in implementation of the Hamradiosolution EZMaster SO2R
  interface in advanced mode. All SO2R features are supported: radios
  switching, internal DVK, internal WinKey interface. The antenna matrix
  outputs are also operational, although there is no user interface to
  define the configuration yet. While waiting for the "matrix configuration"
  window in WT, that can be done manually in the file "WT.INI" in the
  section [EZMaster]. Four numbers respectively represent the decimal
  equivalent values of the binary settings for RX/Radio1, TX/Radio1,
  RX/Radio2, TX/Radio2. The following example shows what it is necessary to
  indicate to activate the bit 0 on 160, the bit 1 on 80...

  [EZMaster]
  Matrix@160 = 1 1 1 1
  Matrix@80 = 2 2 2 2
  Matrix@40 = 4 4 4 4
  Matrix@20 = 8 8 8 8
  Matrix@15 = 16 16 16 16
  Matrix@10 = 32 32 32 32

  This [EZMaster] section will probably not exist yet in your file wt.ini,
  but it is enough to add it to the end so that it is taken into account
  with the next restarting.

  The support of the CAT ports and serial lines will be the subject of
  a forthcoming update.

2.4.0

- The K1EL WinKey is supported (experimental). The interface can be
  configurated in the menu "Option | Configure WinKey...".
  - Keying mode: Iambic A, Iambic B, Ultimatic and Bug (semi-automatic)
  - Second output: you can use the pin 5 of the WinKey interface to
    control the PTT, connect a highspeaker to monitor CW, or
	connect the keyer input of a second radio (SO2R).
  - Sidetone frequency: only relevant if the pin 5 is used for
    monitoring CW.
  - Short spaces, also known as "CT spaces": to reduce wordspace time
    by one dit.
  - Paddle Watchdog: will disable the paddle after 128 consecutive
    dits or dahs. This is to guard against the paddles being accidently
	keyed continuouslt.
  - Autospaces: if you pause for more than one dit time between a dit
    or dah, WinKey will interpret this as a letter-space.

  The half baud CW character is supported by WinKey version 9 and
  later.

  The WinKey interface can be feeded but the COM port: set DTR and
  RTS to "Always On" in the COM port option window.

- PTT output on COM port is working again. Tks MM0EAX.

2.3.2

- DVK/STOP information was generating a pulse on the bad pin (DVK #1).
  Tks I4UFH.

- Half baud CW character added : The ^ character in a CW message inserts
  a half dit delay time. It can be included in a text to add extra
  emphasis to similar sounding sequences. An example is F6IIE, sending
  it as F6I^I^E makes it easier to copy.

- Croatian Cw Contest : Cabrillo CONTEST: header renamed to CROATIAN-CW
  as needed. Tnx 9A2EU.

2.3.1

- RIG interface working again. Tks VK6NU.

- New options for the Cabrillo file output : You can exclude some bands
  from the log, and choose the CHECKLOG category. Tnx F5IN.

- Log cleaning now allows to remove the /QRP extensions from worked
  callsigns.

- After a log cleaning completion, you can load it.

- Bugfix : Some French labels were mispelled in the LPT1 properties
  dialog.

2.3.0

- "DTR always_on" in wt.ini not used anymore: this can be set in the
  "setting interface" windows directly.

- The "Interface configuration" was changed into different points:

  - "PTT/CW for Radio 1/2" option is removed from the serial port
  devices list. You should select "Other interface" instead.

  - The "configure" button associated with each device open a new
  COM port property window, which allow to set more precisely
  how to manage either DTR or RTS lines: one can select between:
  handhake, CW, PTT, always ON, always OFF, Active radio. For CW
  and PTT, one can also select which radio is concerned with.

  These settings are available with every devices connected to the
  serial port, even with a TNC or WT Network.

  - The data sent to the LPT1 printer port can now be more
  precisely defined, clicking on the "configure" button located
  near the LPT1 checkbox. One can change the LPT port address, and
  define which data are sent (DVK, DVK/STOP, Data bands, Active
  Radio, CW/PTT. NB: both DVK/STOP and Band data are sharing the
  pin 2! Some SO2R interfaces can support this, as the DVK/STOP
  signal is only a short pulse. Please check the manual of your
  SO2R interface to insure that it supports this feature.

  These modifications imposed many changes in the source code. I
  tried to carry out many checks but it is not safe from a side
  effect in your particular environement. I recommend to you to
  check well as your equipment is still working as before (radio,
  packet/internet cluster, CW/PTT interfaces, band decoder, ...).

- Croatian CW Contest added.

- Scrollbars in Gab (Alt-I), Packet (Alt-O)  and Spots (Alt-A) windows
  added. Tnx F5TNI.

- QSX frequency automagically added in split mode when sending a spot
  to the DX Cluster (Alt-F3).

- NOCUT, SEMICUT, FULLCUT and PROCUT text commands added to mimics menu
  items for CW cut numbers.

- Cut numbers adjustment :
  - SEMICUT includes T = 0 only.
  - FULLCUT includes T = 0, A = 1, N = 9 (usual case).
  - PROCUT includes T = 0, A = 1, U = 2, V = 3, E = 5, B = 7, D = 8 and
    N = 9 (for those who were born with a keyer in their hand).

- Alt-F8 CT compatibility added to wipe current QSO.

- Ctrl-Shift + Up/Down arrows grabs spots even if they are not needed
  QSO (can be a dupe or a 0 points).

- Bugfix : When specifiying a root directory for logs output, the export
  was failing. Tnx F8CRH.

- Bugfix : Modifying the default directory for logs output was
  cancelling the choosen output formats.

- Bugfix : In CQWW DX, /MM stations are no more credited for country
  multiplier.

- Bugfix : Some windows were not updated after hitting Alt-W, and the
  warning text was not cleared. Tnx F5IN.

- Bugfix : Big scores display in RateSheet window (Ctrl-F9) was
  showing negative hourly points in some circumstances.

- English reference manual included into the distribution package.

- wtDxTelnet included into the distribution package.

2.2.6

- Bugfix: CW "type ahead" mode was not transmitting the callsign in
  some circumstances. Tks F5IN, F8DNX.

2.2.5

- Bugfix: reloading the log in a M/S or M/M configuration caused
  troubles in the network. Tks TM2Y.

- One can now validate a QSO without stopping the transmission of the
  logged callsign (in "type ahead" mode). Tks F5MUX.

- Rig TenTec Orion support added, but not really tested... If you are
  an Orion owner, your comments are welcome!

- Bugfix: CTRL+ENTER was not inserting the callsign in the bandmap
  with either an FT1000 or an FT1000MP. Tks 6W1RY and F8CRH.

- Bugfix: ADIF output of an ARRL 10-meter is working again.

- The title of the database loading progress window now includes the
  database filename.

- The title of the log loading progress window now includes the file
  name.

- Private DX cluster talks to MyCallsign-## are now also considered.

- Bugfix : In some circumstances, sending a spot on the packet
  cluster was misinterpreted, and gargabes were displayed in the
  gab window.

- Bugfix : UpdateQSO protocol updated to handle QSO on 47 Gig band.

- Bugfix : Ukrainian DX Contest : Mode category was not specified
  in the Cabrillo output file. Tnx F5IN.

- Bugfix : Ukrainian DX Contest : SP stations were considered as
  zone stations. Tnx VK6NU and F5IN.

2.2.4

- Bugfix: the english translation for "All" in the "Chat" window
  (sending a Gab) was erroneous.

- Bugfix : In CQWW VHF, using tab key was crashing WT in some
  circumstances. Tnx F6ETI.

- Bugfix : Using the mouse wheel in "included windows" mode was
  leading to a major crash with some operating systems. Tnx F5MUX.

- Bugfix : HamCAP 1.2 broke the background/foreground window
  management code.

2.2.3

- Stew Perry Topband Distance Challenge added. Specific database is
  available at http://download.win-test.com/databases/

- Bugfix in "interfaces configuration window": having both the multikeyer
  defined on a COM port and a radio defined on another one is implying that
  *two* rigs must be configurated. The configuration window now checks this.
  Tks F6IFY.

- A new text command NOSPLIT (or SPLITOFF) sets split operation off for
  the current radio.

- In bandmaps windows, if the DX callsign can't be entirely displayed,
  it's included in the associated tooltip informations.

- LZ DX Contest added.

- New CLEARLOG text command added. Mimics Edit / Clear all QSO menu
  item.

- The sun icons can be now displayed or not in the Spots window
  (Alt-A) in HF contests. A new option in the same contextual menu
  also allows to display all optionnal fields or to hide them all in
  a row.

- The QSO information displayed in the F9 tooltip now includes the
  sent exchange if it is a serial number.

- You can now enter a frequency also with no decimal point (CT style)
  in the callsign field and "Enter" to jump to this freq. For ex.
  18235 Enter will jump to 1823.5 kHz. Tnx F6FGZ.

- The standard space time between CW words is now set to 7 dits length,
  instead of 6 (known as "CT space"). But there is now a new option in
  the Options / CW menu to set it back to 6 dits if you want. You can
  also use the new text commands CTSPACE and NOCTSPACE to set it to 6
  or 7 dits.

- Upon log opening, WT now warns if your country can't be resolved from
  your callsign, and aborts file loading. Tnx F5MUX/TO7X

- If you have a wheel mouse, you can now set a bigger or smaller font
  for the child windows in clicking in it, and use the Ctrl key while
  rolling the wheel (a la Mozilla/Firefox).

- In the multipliers window (Alt-M), Shift + mouse wheel scrolls the
  list to the first or the last line.

- The mouse wheel is now also active the usual way in the multipliers
  window (Alt-M) for scrolling, In the locators window (Alt-L), it
  enlarges or reduces the area of displayed land, and in the bandmaps
  windows, it modifies the scale.

- In VHF+ and Stew Perry contests, the current gridsquare is displayed
  in red color in the locators window. "Display contacts" option must
  be enabled. Tnx F6BGC.

- New experimental feature : Gridsquares are extracted from packet flow
  comments, if possible, and are used to calculate Az and distance spot.
  The syntax analyser is quite accurate, but it will not replace the
  human brain in some circumstances !

- Spots with known gridsquares (extracted from log, database or
  extracted from packet flow comments) can be displayed in the locators
  map window (Alt-L). The tooltip associated with them displays
  callsign, guessed locator, azimuth and distance.

- If a spot with known gridsquare is pointed in the spots window
  (Alt-A), its location is blinking in the locators map window
  (Alt-L).

- Bugfix : In CQWW DX, working a station in the same country as yours
  was giving points instead of 0. Tnx F5MUX.

- Bugfix : FT990 split operation is now working and displayed in the
  bandmaps. Tnx F6GOX.

- Bugfix : The ini key regarding the check country refresh mode was
  incorrect.

2.2.2

- Both PTT and CW can now be sent to a COM port different from the
  port assigned to the radio. You can either configure a COM port
  for the PTT/CW control for either radio 1 or radio 2 or both.

- Ukrainian DX Contest added.

- Ukrainian oblasts appended to the CTY_OBL.DAT file. Tnx F5IN, UT1IA.

- OK/OM DX Contest added.

- New tooltips in bandmaps. In HF contests, Az and Lp are guessed from
  the country resolver, and in VHF, Az and distance are guessed from
  the log (if the station has already been worked) or from the database.
  Tnx F8CRH.

- The Spots window (Alt-A) can now display spot heading. Same
  informations as above.

- You can now launch an external program by typing its name in the
  callsign field and the Ctrl-X key (stands for eXecute) to launch
  it. This is useful for example if you need to run a batch file
  while running Win-Test. This external program must be located in
  the Win-Test directory, or in a directory included the Windows
  system path.

  A practical application of this new feature is to use a batch
  file to change sound files when you change op in a multi-op
  environment.

  Another application could be to launch an on-demand backup on
  a volume different from the one specified in the backup command
  integrated in Win-Test.

- The long-awaited CheckCall window (by some users) is finally
  available. Its shortcut is F9. You can even set its refresh mode
  (on every keypress or on space key only). You can display data
  on a worked QSO by moving your mouse on the checkmark. A double
  click on a checkmark scrolls the log to display the specified QSO.
  Tnx F6BEE ;-)

- If the callsign field is empty, the serial sent in CW with the
  $SERIAL variable is now the QSO number of the previous QSO.

- Bugfix : Packet private talks containing extended ASCII code
  chars were truncated in the Gab window (Alt-I).

- Bugfix : In the WAG contest, DOKs different from usual format
  (One letter + Number) weren't considered as valid. Tnx F5IN.

- Bugfix : The Gab Window (Alt-I) couldn't be displayed anymore !

- Bugfix : In WAG contest, the default CW messages are now correct.

- Bugfix : When importing an Editest binary file, the last QSO was
  missing in the resulting Win-Test file. Tnx F6ETI.

2.2.1

- Bugfix in WAE contest: ALT+L and ENTER keys were not active in the
  QTC window. Tks F5IN.

- Rig FT-847 support added. Note that the CAT system of the '847 does
  not  support the Split mode nor switching between VFO A and VFO B.
  For this  reason, the VFO B is disabled in the radio window.
  Many thanks to VK6NU and EA3IN for their help!

- FT1000-MP support rewritten.

- Rig FT-900 support added.

- Rig FT-897 support added. The CAT system is not able to identify
  which VFO is currently activated. For this reason, the VFO B is
  disabled in the radio window, and the VFO A is always set as active.
  Split mode is supported.

- Rig FT-817 support added. Same remark as for the FT-897.

- Added support for some Icom RIG: IC-275, IC-475, IC-1275, IC-718,
  IC-728, IC-729, IC-736, IC-738, IC-746, IC-746Pro, IC-7800, IC-910.

- The first QSO Party is mainly implemented : The Texas QSO Party !

  Please note these specific data and limitations for all QSO parties :

  - When logging a Rover or a Mobile station, you MUST log the callsign
    as <Callsign>/<County> (ex K5MZN/FREE). Otherwise, dupe and
	mult checkings will be inaccurate for these stations. By the way,
	the county will be automagically extracted from this logged
	callsign.

  - If you enter in Rover or Mobile categories, to change the county
    where you transmit from, use the <, > or Tab keys to access the
	county field. Note that if you're entering a multi op Rover
	or Mobile category, you must change the county field on EVERY
    networked computer (and use the Rover or Mobile category in
	contest settings dialog).

  - For now, bonus points are not computed.

  - Dupes and mults are only checked for CW and SSB modes. Other
    modes are allowed (use the All Modes choice in contest settings
	dialog), for QSO and points but mults count will not be accurate.

- EU Sprint Contest added.

- Worked All Germany Contest added.

- The voice files are now named according to the function key name.
  MSG1.WAV is now associated with F1 key, MSG2.WAV to F2 key, etc...
  Tnx VK6NU.

- New experimental feature : The soundcard microphone input can be
  managed to be used in pass-thru mode with the voice keyer (VK)
  thanks to 4 new text commands :

  - MIC : Enables the mic input when the VK is not playing
  - NOMIC :  Mutes the mic input when the VK is not playing (*)
  - MICWHENPLAY : Enables the mic input when the VK is playing
  - NOMICWHENPLAY : Mutes the mic input when the VK is playing (*)

  (*) Default settings after installing.

  Notes :

  - These settings can be set only when you're in a Phone mode.

  - If you change mode to a non-phone (in a mixed contest for ex),
    the mic input will be muted. It will be also muted when
	exiting Win-Test.

  - Settings will not be applied immediatly if you modify them
    when the VK is playing.

  Tnx F8CRH

- A new text command "SETUP" opens the interfaces setup dialog.

- A new option in the CheckPartial contextual menu allows to check
  partial callsign only in the current log.

- New protocol version released (bugfixes + updates to allow QSO
  parties networking).

- HamCAP predictions are now also available within the contextual
  menu on a callsign in the bandmaps and in DX Cluster spots window
  (Alt-A).

- New sun icons are displayed in bandmaps, DX Cluster spots (Alt-A),
  and check country (F10) windows to indicate local sun position.

- Bugfix : Using child windows shortcuts with no contest file
  opened was leading to a major crash. Tnx N4ZR.

- Bugfix : An invalid locator in the contest settings dialog was
  preventing the log from being loaded. A validity check is now
  performed to avoid such a case. Tnx N4ZR.

- Bugfix : COM port speed was not correct when reopening this port
  if set speed was over 19200 bauds. Tnx VK6NU.

- You can jump to the start (resp. end) of the log by hitting the
  Ctrl-G (stands for "Goto") keys and the Home (resp. End) key when
  the goto dialog is displayed.

- Bugfix : If a packet spot comment was including an ampersand
  char (&), the comment was misprinted in the Spots announces
  window (Alt-A).

- Bugfix : Importing from a Cabrillo file failed if the target Win-Test
  file didn't have a wtb extension.

2.2.0

- Added offtime information in cabrillo for WAE and WPX contests in
  single-op category

- There is now a way to modify the callsign of a QTC even if it has
  been validated (notice that the new callsign must not be logged as
  a QTC before).

- ARRL August UHF Contest added

- ARRL January VHF Sweepstakes Contest added

- ARRL June VHF QSO Party Contest added

- ARRL September VHF QSO Party Contest added

- IARU 50 MHz contest added

- REF DDFM 50 MHz contest added. Notice that no field is designed for
  the  received departments. Rules stipulates that the French stations
  give <callsign>/<dpt> and thus we must log the French stations that
  way. The software will automatically extract the departement number
  from the callsign field.

- Bugfix : In some circumstances, valid registration key checking
  failed.

- Private packet talks via DX cluster are displayed and recorded in the
  gab window (Alt-I). You can directly answer with a double-click on
  the received talk. It doesn't work in conference mode.

- Private gabs across the network can be sent by choosing the station
  name in the Gab dialog (Alt-G). You can also sent a private gab with
  a double-click on the station name in the Status window (Alt-J) or in
  the gab window. You can easily answer (in private) with a double-click
  in the gab window, on the private line received.

- In either case (private gab or private packet talk), you can also
  quickly answer to the last received with an Alt-P (P stands for
  Private) shortcut

- New version of the ratesheet window (Ctrl-F9), which can now display
  many different data : Have a look to the "Data" item of its
  contextual menu.

- Rate window (Alt-R) now also displays QSO count since last round hour.
  Tnx F5IN.

- SAC (Scandinavian Activity Contest) added.

- TOEC WW Grid Contest added.

- Bugfix : Some very high frequencies (241 GHz+ !) were not correctly
  saved in the ini file.

- Bugfix : Modifying the first QSO of the log was adding a Qso in
  the ratesheet every time.

- Bugfix : Locators validity checks were not correct.

- New solar activity window : Data are extracted from Packet data flow,
  and saved in .wwv and .wcy file. You can switch between WWV and WCY
  with the contextual menu, or with "WWV" and "WCY" text commands. Each
  chart can be displayed or hidden with a click on the triangle atop
  the chart (handle). An hatched graph means that the index is missing
  for this hour, and the most recent known was used instead.

- HamCAP interface : HamCAP solar indexes can be set from data
  gathered for the solar activity window. Use the Options / HamCAP menu.
  The priority item sets which data will be send to HamCAP (WWV or WCY)
  when both indexes are known for the same last hour.

- Bugfixes : Cancelling a file opening and merging files were creating
  two tiny memory leaks ;-)

- RDA Contest added.

- KCJ Contest added.

- CTY_OBL.DAT updated. Tnx F5IN.

- CheckCountry window (F10) width, rate window (Alt-R) height and
  width and bandmaps windows height should be now adapted for all
  Windows fonts sizes. Tnx F5IN and F6IFY.

- DX spots given by a SH/DX cluster command are now checked against
  bandmap timeout and displayed accordingly.

- DX spots senders callsigns whose lengths were more than 6 characters
  were trunctated.

- Bugfix : In RateSheet window (Ctrl-F9), mode display option was
  not correctly saved.

- Bugfix : In floating windows mode, if you chose an item in a child
  window contextual menu, WT main window might loose focus.

2.1.6-rc3

- Bugfix: again a problem with the date fields in REG1TEST! Tks F8ACF.

- WAE: QSO are copied before QTC in cabrillo when they are both
  validated at the same time.

- Bugfix: In WAE, the worked QTC number was not initialized in the summary
  when one deleted all the QSO in the LOG. Fixed. Tks F5IN.

- ReverseMultChecking (Shift-F10) was displaying dupes and invalid
  QSOs callsigns. Fixed.

- ReverseMultChecking (Shift-F10) is now only available for all
  contests supporting this feature.

- HamCAP interface now supports two settings (Options / HamCAP):

  Options / HamCAP / In background, if you want or not the HamCAP
  window to stay in background after a call to it. If your screen
  is large enough (or if you're lucky enough to have two), HamCAP
  can certainly be displayed side by side of WT (you can use
  floating windows mode to save space). In this case, setting
  In Background will guarantee you'll not loose focus,
  when you call HamCAP.

  Options / HamCAP / Tab

  If you use the map tab, the displayed band will be the one
  of the WT QSO. Warning : HamCAP is not supposed to display all
  bands : In that case, HamCAP will display its default band.

- HamCAP interface is now disabled for VHF contests.

- DX spots directly received or via a SH/DX command are compatible
  with DXNet, AR, CLX and DXSpider type clusters.

- Display choice in Zone window is now saved and restored on file
  opening.

- New text command "BYE" added. Equivalent to File / Quit.

2.1.6-rc2

- BugFix: EU-HF contest: Year 00 to year 09 were not valid multipliers.
  Fixed. Tks F5IN.

- WAE bugfix: The "points" column of the summary was wrong. Fixed.
  Tks F5IN.

- WAE: Some CW messages used in the WAE contest are manually configurable.
  For that, it is necessary to open the file "WT.INI" located in the Win-Test
  directory. Then, you can to modify the messages in the section [QTC].

    [QTC]
    CwRxF1=QTC?
    CwRxF2=QRV
    CwRxF3=TIME?
    CwRxF4=CL?
    CwRxF5=NR?
    CwRxF6=QSL ALL
    CwRxCR=R
    CwRxPlus=TU
    CwTxF1=QRV?
    CwTxPlus=TU

  Both variables $CR and $MYCALL are supported. Thus, you can decide ie that
  the + key must, in addition to validate the QTC dialog window, validate the
  QSO and send your own callsign. The following replacement of CwRxPlus
  variable in WT.INI will perform this that way :

    CwRxPlus=$CR TU $MYCALL

  Tks F5IN.

2.1.6-rc1

- WAE bugfix: the QTC were disordered in the log after a cabrillo output. The
  number of QTC was also wrong. Tks F6IFY.

- WAE bugfix: frequency was often wrong in cabrillo for the QTCs.

- WAE bugfix: the number of QTC available is displayed only with a valid
  callsign. Tks F6IFY.

- WAE bugfix: log deleting also initialize QTC. Tks F5IN.

2.1.6 beta

- WAE Dx Contest added. Still in BETATEST, use it at your own risk! :)

- New network protocol version released (added both QTC and BandMap
  protocols, and updated ADDQSO/UPDATEQSO ones).

- HamCAP (http://www.dxatlas.com/hamcap/) basic interface added. HamCAP
  must be installed and working on a standalone basis. Then, you can
  get propagation predictions by entering a callsign, and Ctrl-P. For
  now, indices must be manually entered in HamCAP (or via Ionoprobe
  written by the same author). Future versions should extract them
  from cluster traffic...

- wt.ini management code modified for sanity. Some recorded options
  could be reset. Check them before complaining ! Thanks.

- YO DX contest added.

- European HF Championship added.

- Oceania DX contest added.

- A new text command "SPEED" (or "CWSPEED") mimics a call to the CW
  speed dialog.

- Saved notes now include date and time of related QSO.

- SR and SS in the clock window are now displayed and updated only
  for HF contests.

- Alt-F4 (or text command RUNFREQ) moves to last Run frequency after
  an instant QSO on another freq. The Run freq is determined by the
  last 3 QSOs in a row on the same freq (+/- 100 Hz) on the current
  radio.

- Bandmap op. added entries (Ctrl-Enter) are now shared across the
  network and saved on every networked station.

- Bugfix: IcomGenericRadio<1|2> address in the section [Interfaces] of
  WT.INI fixed:

    IcomGenericRadio1=<n>h    when n is the radio 1 HEXA address
    IcomGenericRadio2=<n>h    when n is the radio 2 HEXA address

    For example : IcomGenericRadio2=48h   will use address 48 hexadecimal
	for the Radio 2
  Tks F6IFY & F8CRH.

2.1.5

- Rig FT-100 support added. Tnx F0EAQ!

- Rig FT-1000D support added, but not tested in real life with a radio!

- Rig FT-920 support added. Tnx F6EPY!

- Fixed potential bad directory path for STATES.DAT and ARIPROV.DAT.

- IOTA DX contest support added. NB: The IOTA reference must be entered
  *without* hyphen in the LOG. Notice that WT will automatically complete
  the IOTA reference with the 0 which are missing: for example,
  the entry "EU5" in the IOTA field will be changed by EU005 when pressing
  <enter>. The file "IOTA.DAT" contains a list of the IOTA references, with
  the name of the islands.

- Added CW keying weight support in the Multi-Keyer.

- The W5XD/K5DJ Multi-Keyer is supported:
  http://www.writelog.com/SO2R/w5xd_multikeyer.htm

  Select W5XD Multi-Keyer in the Interface Configuration Window. By default,
  the Multi-Keyer shares the COM port with "radio 1", except if
  "radio 1" is explicitly defined in the Interface Configuration Windows
  (that way, the Multi-Keyer will share the "radio 2" COM port).

  There are 3 available options in menu "Commands | SO2R" to control the
  headphone:
    - Split mode (AltGr+S): to listen both radio.
	- Toggle mode (AltGr+T): to puts the headphone to the non active radio.
	- Latch mode (AltGr+L): to automatically puts the headphone to the non
	  active radio during transmit.
  The initial of each headphone mode indicates in the bottom of the Rate Window
  which mode are currently activated.

  Tune (CTRL+T) is working as well, except the pulse mode.

  Use either the '*' or Alt+: key to switch between "radio 1" and "radio 2".

  There is 3 additionnal settings you can done in WT.INI:
  [MultiKeyer]
  CwAutoLtrSpace=no			yes->Turns on auto letter space
  CwSidetonePaddles=no		yes->Turns on CW sidetone for paddle-sent CW
  CwSidetoneMachineSent=no	yes->Turns on CW sidetone for machine-sent CW

  Tks F6IFY!

- Main window title now includes StationName.

- A new text command "VERSION" shows WT version.

- A new text command "RELOAD" (or "REOPEN") reopens the current
  opened file.

- A new text command "WEIGHT" (or "CWWEIGHT") opens a CW keying weight
  setting dialog. Weight can be set between 2.0 and 4.0. Tnx F5IN.

- New network protocol version released.

- CheckCountry window (F10) was broken when the current QSO was a dupe.
  Fixed.

- Double click on the QSO number in the F10 window should now set
  the log on the specified QSO for every contest !

- F10 window now displays country local time (according to CTY.DAT
  time zone data). Tnx F5IN.

- Contests list reordered by HF / VHF / Dxpedition groups.

2.1.4

- Bugfix: 5-wire RS-232 line is working again. Tks F6BEE, F6FGZ, F6BGC.

- N+1 window : small bug fix.

- All packet traffic is recorded in .pkt file and last 8 Ko are reloaded
  in pkt window on file opening.

- Status window : During a timeout, the station name is still displayed.

2.1.3

- N+1 window now displays callsign count adapted to its size.

2.1.2

- Bandmaps are filled on file opening.

- Updating a QSO keeps QSO frequency if band does not change.
  Otherwise, WT uses the default Cabrillo frequency. Tnx F5IN.

- In some circumstances, worked stations were shown on wrong
  bandmap band or frequency. Fixed.

- Check partial window now displays callsign count adapted to its
  size.

2.1.1

- LOG synchronisation through the network (experimental).

- Deleting QSO not allowed when LOG synchronisation is enabled.

2.1.0

- English translation available: menu "Options | Language" will leave you the
  choice between French and english.

- Bugfix: date format in REG1TEST header. Tnx F6ETI.

- CW output on COM port added. Click on "configure" button associated with a
  COM port to enable CW output on that port. CW output can be shared on all
  radio COM port or each radio can be keyed separatly regarding to the
  active one in SO2R mode.

- Bugfix: crash on exiting when still transmitting CW.

- Bug fix on Cabrillo export log for several VHF contests. Tnx F6ETI.

- Key remapping dialog now shows Alt Return and Ctrl Return keys.

- Partial and NP1 windows are now limited to 20 callsigns.

- Reverse mult check window (Shift F10) is now limited to one line
  per band.

2.0.8

- Added a serial number column for both ARRL 10 (dx side only) and Baltic
  contests.

- Bugfix: deleting a QSO no longer disorder serial number in V/UHF contests.
  Tks F8ACF.

- ADIF files export fixed for various contests. Tnx F5IN.

- Long prefixes (LY2004 for example) are now no more truncated,
  if new prefix multiplier applies. Tnx F5IN.

- Equivalences zones files (STATES.DAT, OBLASTS.DAT, ARIPROV.DAT)
  can now have commented lines (starting with # character).

- King of Spain Contest support added.

- Baltic Contest support added.

- CQ-M country file (CTY_CQM.DAT) added within distribution,
  with last informations gathered from different sources.
  Special tnx to UA9CIR.

- ARI International DX contest support added.

- SP DX Contest : Dupe check in mixed mode was broken. Fixed.

- Bug fix: Date in REG1TEST format fixed (year must be 2 digit long only).

- New network protocol version released.

- The note file (.not) now includes the mode of the annoted QSO.

- The DX Cluster spots are now recorded in a .dxc file. Only relevant
  spots are recorded (ie the ones displayed in the Announce window). The
  main purpose of this new feature is not only to help users for
  after-contest statistics, but the file is also reloaded at startup,
  thus avoiding to send an usual SH/DX 500 to fill up the bandmaps.

- In CQWW WPX M/S or M/M grabbing a spot from another band wasn't
  modifying the serial numbering as it should do. Fixed.

- CQ-M International DX contest support added.

- When using the 'extended' DXCC list (e.g. for CQWW), 4U1VIC was still
  processed as an OE station. Fixed.

- KG4x (KG4 + 1 letter only) callsigns are now resolved to an US station.

- SP DX contest : Cabrillo file generation bug fix (mode forgotten).

- YU DX contest support added.

- RDXC country list used is now the same as for the CQWW DX. The RDXC
  rules didn't specify it ! Sorry for inconvenience. Tnx F6GOX/F5IN/RW1AC.

- Bugfix in DXCC_lookup internal function. Entering a callsign like "TK/7"
  (if you were hearing the end of W8TK/7 callsign for example) was leading
  to a violent crash !

- Bandmap windows : Spot time now displays the elapsed time since this
  spot was sent rather than spot time.

- Shift-Del deletes all chars under and after cursor position.

- Greyline display : Some glitches were still appearing during this equinox.
  Code entirely rewritten. Should be ok now (and faster...).

- Rate window : Calculations might be wrong in Mixed mode : Fixed.

- F10 window in DXped : Some modes weren't visible with some OS : Fixed.
  Tnx F5JSD/5V7C.

- Summary added for each bandmap : Displayed infos are : Spots count,
  needed QSOs count, new countries count, new zones count and
  new HQ count (IARU DX).

- Setting CW speed by calling Alt-V dialog with an entered callsign in the
  log was deleting this callsign. Fixed. Tnx F6GOX.

2.0.7

- Bug fix : defective grayline near the equinoxe

- The CheckCountry window can be refreshed automatically each time a new key
  is pressed. This feature can be enabled or disabled right-clicking on the
  Check Country window.

- Bug fix: after a "fixmine", WT importuned us with a dialog box reporting a
  log synchronisation error. Tks F8CRH.

- In DXped mode, summary window was lacking a total QSO count. Fixed.

- In DXped mode, summary window copy as text could crash WT. Fixed.

- The backup volume (including its path) can be set in Options menu
  item. Note : For safety reasons it's recommanded to backup on a
  different physical device from the one where the wtb file is.
  Tnx F5IN.

- New layout for F10 window in DXped mode. Tnx F5JSD/5V7C.

- In DXped mode, stations aren't no more warned as dupes when worked
  on the same band, in another mode. Tnx F5JSD/5V7C.

- To comply with other font effects for daltonians (and the rest of us)
  bandmap font have been modified (but colors remained). Italics for
  dupes and not allowed stations. Bold for mults (and station on current
  VFO freq), and normal font for needed stations.

- Ctrl-Up and Ctrl-Down now grab previous and next spot (instead of Alt).
  To be consistent with new Alt Up command which copies previous callsign.

- Alt Up was crashing WT when entered in an empty log. Fixed.

- Bug fix : Cabrillo import for THF European, THF European with GridSquare
  and REF THF was broken. Tnx F5TJW.

- In the Cabrillo log, claimed score for most VHF and higher bands
  contests was 0. Fixed.

- New layout for Zones window in All band / All mode display.

- A new option in Edit menu allows to scroll in your own log (ie the QSO
  you entered) in a multi station environnement. You can bypass this
  constraint by hitting the shift simultaneously. And if the option
  isn't set, hitting shift with arrows temporarly sets this feature on.

- The CTY_OBLAST and OBLASTS.DAT are modified to fit with new russian
  abbeviations for RDXC. Tnx F5IN (and UA9KM).

- The REG1TEST export city field was filled with the operators name. Fixed.
  Tnx F6ETI.

- A properties dialog can be open from the Radio windows. It allow to
  change spots duration in the bandmaps, and others options regarding
  the  bandmaps. Please note that these properties are set for both
  radios windows.

- Bug fix : In some circumstances, Alt-M window was displaying countries it
  wasn't supposed to !

- Bug fix : The Alt-M Display contextual submenu wasn't updated.

- In the clock window, 59 and 01 minutes displays time in light red, and
  00 minutes displays time in bright red. Useful for operator shift
  in multi op operations. Tnx F1HAR.

- ARRL DX, K/VE side : WT wasn't guessing power from a previous QSO. Fixed.

- Bug fix : In some circumstances, Partial Check window was displaying
  several times the same callsign.

- In Zones Window / All bands - All modes, clean sweep and never worked
  zones are displayed with different colors. Tnx F1HAR.

- Ctrl-Del removes current freq spot (if any) from bandmap. In fact, it
  mimics a F11 followed by a Ctrl-Return.

2.0.6
- Bug fix: F11ing a QSO on the second radio moved the active
  band to the first radio band.

- If a frequency is entered in the callsign field, switching to the other
  radio (ALT+/ or *) will automatically QSY the radio to this frequency and get
  the callsign of the previous QSO copied. This is intended to ease passing a
  multiplier to the second radio.
  Alternatively, a band name can be entered instead of the frequency.

- ALT+UP copy the previous QSO callsign
  ("commands | copy previous qso" in the main menu)

- Added a new memory keyer (ALT+C), useful to send some extra preprogrammed
  CW messages. A new entry in the commands menu has been added for this
  feature: "CW Messages".
  The ALT+C window can be used to send one of the 12 preprogrammed messaged,
  using the function keys (F1 to F12). The window automatically closes itself
  when sending a message. The changes in the messages are saved as well.

2.0.5
- Bugfix: mode display in the check country window.

2.0.4
- Freeware version, for the REF HF contest, DX side.

2.0.3
- Reference manual menu item added (+ remote / local option)

- Ref manual pages openings automated with child windows
  help icons, contextual menus items (if any), Alt-H log shortcut,
  and HELP text command.

- Edit / Goto QSO menu item added. Its text depends on callsign field.

- Start and End buttons added in Goto QSO dialog. You can also type
  "START" (or "FIRST") or "END" (or "LAST") in the edit field.

- Double click on a QSO in the CheckCountry window moves log on this QSO.

- RTTY text command added.

- F6 and F7 voice messages are now handled. Tks F8CRH.

- PTT delay can now be specified in Interfaces dialog. It's now working
  with CW and voice keyers. Its value must be set between 0 (full QSK)
  and 1000 ms (broadcast station amplifier relay ;-) ) included.

- CW speed can be directly set by typing WPM value in callsign field
  and Alt-V. If the callsign field is empty, or is not meaningful, a
  dialog box appears to set the speed.

- Commands / CW speed menu item added. Its text depends on callsign field.

- All Asian : Default zone wasn't filled even if callsign was worked on
  another band. Fixed.

- All Asian : QSOs between Asian stations of the same entity gave points
  instead of 0. Fixed.

- All Asian : Rules for QSO with /MM stations are now handled.

- DXPed : Mode display in CheckCountry window wasn't correct. Fixed.

- QSO column widened to allow 10k+ QSOs in Summary window for CQWW DX.

- Added All Asian contest Cabrillo import. Tnx F5IN.

- Freq field in HF Cabrillo files is now right justified, following
  Cabrillo specifications.

- Ctrl-Z shortcut added to Edit / Restore QSO item.

- CTY.DAT exceptions are now handled in every case.

- In REF contest, DX side, default CW messages now use serial
  numbers rather than zone !

- Small fixes in Cabrillo import / export for RDXC contest.

- In REF Contest - DX side, non-French contacts were added for mult
  credit, and the DXCC window was visible. Fixed.

- In ARRL DX Contest - DX side, non US/VE contacts were warned as
  "New country". Fixed.

- In RDXC : KR oblast was missing. Fixed (stupid typo in code...). Tnx F5IN.

- In RDXC, oblasts are now guessed from callsign. CTY_OBL.DAT file needed.

- ARRL 160M contest added.

- There are now different main window layouts, depending on mono-mode or
  mixed-mode choosen (if applicable). The same rule applies for summary
  window.

- SP DX contest added. To be improved (In particular, the three-band
  category is not yet supported).

- New mult(s) indicators changed : If there's only one mult type (country,
  zone, province, etc...), it's displayed as a whole. If there are two
  mults types (like in CQWW DX), the abbrev indicators are displayed as
  before.

- Japan International DX contest (JIDX) added.

- New "----" indicator when a QSO is not allowed, according to the
  contest rules.

- New font syles for daltonians added in Check Partial and N+1 windows.
  Tnx F5AEG and F5IN.

- REF HF : Breaktime total was wrong when over 24 H. Fixed.
  Tnx F6ETI/F8BPN.

- Zones window code fixed to avoid flickering effect during the first
  opening of the window.

- COM port properties dialog UI fixes : Cancel button was labelled
  Cancel instead of Annuler (Tnx F5TJW) and combo boxes were editable
  instead of drop lists.

- QSO numbering was wrong during Cabrillo import, if an imported QSO
  had an invalid format. Fixed.

- Added SR and SS in clock window. Text color changes when you're
  within 30 minutes of SR or SS.

- Mults check strengthened for spots displayed in the bandmaps
  and DX cluster annonces windows, and in the status line.

- Cabrillo import : Warns when a QSO line format is invalid and allows
  to skip line to continue import, or to abort it.

- All contests with "Zones" multipliers : The window can now display
  worked zones following the current QSO band (or mode), or all zones
  by band (or mode), according to the contextual menu option.

- ARRL 10 m : Hawaii and Alaska states are now counted as US States,
  rather than DXCC countries, following the contest rules.

- Mult window (Alt M) : Internal code improved. 50% of repainting time
  saved.

- PSK, PKT, HELL, and SAT modes and associated text commands added.

- DIGITAL = Mixed(RTTY, PSK, PKT, HELL) mode category added. Doesn't
  work for all contests.

- FT-990 basic support added (to be improved). Tnx F6GOX.

- Zone window : "Copy as text" added (you must be in All Bands or All
  Modes display). Further paste can be done in text or in a spreadsheet
  as the SYLK format in supported.

- Mult window (Alt M) : "Copy as text" in progress. To be improved.

- Contextual menus added to the clock and SSB vu meter windows.

- Shift + BS deletes all characters before the insertion point.

- The Space key now also stops repeat mode and F1 message playing.

- New CW variable $REPEAT : Reset the automatic repeat mode interval.
  Usually used at the end of the + CW message.

2.0.2
- Added ALL ASIAN DX CONTEST rules

2.0.1
- Pressing either the down key or the page down key could validate a qso
  accidentally. Fixed.

- Added DXpedition category (HF + 50 MHz). Still in beta test.

- Bug fix: the program might crash when the VFO of the connected radio is
  out of band.

- Merge log crash fixed.

- Added CTRL+G to move on the QSO number specified in the callsign field
  or in a dialog box if no QSO number was entered in the callsign field.

- Bug fix: importing an HF binary log generated by win-test without .DTA
  Tks F4DXW.

1.4.0
- The specific databases of the HF contests are no more included in the
  distribution package, and must be downloaded separatly. The database files
  are still available on the download site :
  http://download.wintest.online.fr/databases

- Resizable child windows have a minimum size to allow to move and
  resize them if needed.

- The extension file name of the REG1TEST log files changed to .EDI
  instead of .REG, which was confusing a lot.

- Changed the way WT communicates with the Kenwood radios (poll mode).

- In ARRL DX, any valid callsign is now accepted. Anyway, a unvalid contact
  (ie a W station worked by a W station) won't be credited.

- In the summary window, the total points for each bands is now the total of
  the QSO points. This applies to the HF contests only.

- Bugfix : N+1 was sometimes showing duplicates callsign. Fixed.

- Right click on a child window also brings it to top.

- Changing mode on the second radio in SO2R had no effect in WT. Fixed.

- The frequency of the connected radio is no more initialized by WT at
  startup. On the other hand, the opposite is now done.

- IARU HF and all others HF contests : Summary window : Scores checked
  and columns widened to allow "big" scores to fit. Tnx TM0HQ

- Loading a large log was crashing if a FT1000 was connected. Fixed.
  Tks TM0HQ.

- ARRL DX : Summary window bugfix : Grand total points were wrong. Also
  points and QSO columns widened one car to allow 10M+ pts scores,
  and QSO count 10k+ to be displayed.

- IARU HF summary window widened to allow 10M+ points scores to be
  displayed. Tnx TM0HQ.

- Alt-1 and Alt-2 were not working anymore. Fixed. Tnx F1HAR.

- Shortcut for reversed zone checking was mispelled in its menu item.
  Fixed. Tnx F1HAR.

- Qso updates through the network is working again.

- CQWW WPX : summary bugfix : multiplier information might be wrong.
  Tnx F5IN.

- bugfix : pressing up key on the first QSO in the LOG caused mess in both the
  band points and the total points.

- Keyer type (CW or SSB) wasn't switched after grabbing a spot in a different
  mode. Fixed.

- Added SPLITFREQ command. Mimics Commandes / Freq de split menu or
  "-" (on numeric pad) key action.

- In floating windows mode, the send gab dialog doesn't loose focus when
  a new gab is displayed in its window. It was rather annoying when chatting
  in a large network.

- Couldn't anymore create a CQWW WPX contest file, because of disabled Zone
  edit field, which was waiting to be filled ! Fixed. Tnx F5IN.

- Bug fix : the multiplier information might be wrong after a modification in
  a QSO.

- Network released.

1.3.0 released
- IARU HF supported.

- Fixed a security problem with the network protocol.

- Bulletproof check on IP broadcast address validity in Interfaces dialog.
  Well, I hope so. Tnx F6BEE.

- Titles of zones window and mults window, their associated menu items,
  and shortcuts enabling are now dependent on the contest type. This
  new code should ease maintenance and new contests addition.

- The active mode is updated when we move up or down in the log.

- Alt-K (shortcut to Keyboard mode) was allowed in SSB mode, which could
  lead to a violent crash if keys were pressed afterwards ! This shortcut
  is now disabled in SSB.

- N+1 fixed (it was not working when the contest file was in a different
  directory than wt.exe).

- When grabbing spot from bandmaps or announce windows, log is switched
  in the right mode. Useful for mixed contests (ARRL 10m for example).
  Packet spots modes are assigned according to the MODE.DAT file.

- New Summary window code : that will ease future improvements.

- Clics on the VFO in the Radio windows are sent to the Kenwood radios again.
  Tks F8CRH.

- Bug fix : When current QSO was wiped with F11 (or Alt W) in a VHF
  contest, the distance and azimut fields were not cleared. Tnx F6HJO.

- Added text command "DEFINEKEYS" : Similar to menu Options / Redéfinir
  les touches du clavier....

- Added Ctrl + left (or right) arrow to move cursor to the start (or the
  end) of the current log field. It's equivalent to Home and End keys. It
  emulates the usual Windows shortcut in edit fields.

- Added band changes by text commands. For example you can type "20" or
  "144" or even "241G" (= 241 GHz) !!!

- Added mode change by text commands "SSB" and "CW".

- Frequency is now moved when a callsign is passed from the band map
  to the log. Tks F6FVY.

- Bug fix in the multiplier field of CQSOs in REG1TEST, which was always set
  to 1.

1.2.1 released
- Time distributed across the network is now accurate on every connected
  machine. Tnx F8CRH.

- Added a way to change the output directory the log files will be saved in.

- Size of the soapbox edit box increased.

- Average distance fixed for THF contests. Tks F6HJO.

- Mode is sent with a QSO or QSO UPDATE through the network. Notice that the
  actual protocol is no more compatible with the one of the older version
  of Win-Test.

- Points for the french stations in REF THF doubled. Tks F6BCG & F6HJO.

- Zone information is not needed anymore for neither the CQWW WPX nor the
  CQWW VHF contests.

- Last mode is saved in wt.ini

- Bug fix : WT might crash if no gridsquare were specified in the
  contest setting window for some contests.

- CW menus reorganized.

- Various cosmetic changes on menu titles.

- Bug fix on 'Desactiver le son' menu (and now becomes 'Son désactivé').

- New features on serial numbers sent in CW :

  1/ Enabling or disabling leading zeros sending by menu or text commands
  LEADINGZEROS (or in short LZ) and NOLEADINGZEROS (or in short NOLZ).

  2/ Four abbreviated levels. Can be set by menu or by text command :

  - Non abbreviated : NOCWABBREV (or NOABBREV) : Self explanatory
  - Semi abbreviated : CWSEMIABBREV (or SEMIABBREV) :

    In this level, the leading zeros (if enabled - see above) are keyed
	as T. Zeros included in serial number aren't.

  - Abbreviated : CWFULLABBREV (or CWABBREV or FULLABBREV) :

    In this level, 0 and 9 are all keyed as T and N.

  - Pro : CWPROABBREV (or PROABBREV) :

    In this level, 0, 1, 4, 5 and 9 are all keyed as T, A, V, E, N

  Summary examples :

   Serial number     010           5194

   NOABBREV          010           5194
   SEMIABBREV        T10           5194
   FULLABBREV        T1T           51N4
   PROABBREV         TAT           EANV

   NOTE : These abbreviations do concern serial numbers ONLY ($SERIAL
   variable in CW messages). To abbreviate zones, report sent etc... you
   have to modify in the CW messages texts themselves.

- Several display bugs in summary window fixed (especially for ARRL 10 m
  and CQWW 160 contests).

- When working a new US state or a new VE province in ARRL 10 m and
  CQWW 160 contests, a 'S' is displayed in the log (rather than a 'Z').

- EXIT command added ( = QUIT).

- CLOSE command added (= Fichier / Fermer menu)

- TUNE command added ( = Ctrl-T)

- Power dialog in ARRL DX DX side contest has now focus on the edit field
  rather than on the OK button when opening.

- This edit field is now uppercased.

- File dialog title for 'Nouveau...' is now 'Nouveau', rather than 'Ouvrir'.

- Combo boxes in the interfaces dialog are now droplists. It avoids the user
  to type in them (what for ?).

- Bug fix on closing the interfaces dialog with OK, when no log was opened,
  which led to an access violation error.

- Cosmetic bug in cursor position in CQWW VHF fixed.

1.2.0 released
- Fixed some bugs in WPX mode :
	- WT warns if the callsign is a new prefix (not a new country)
	- F10 fixed
	- Summary window total points
  Tks to F5IN, F8CRH, F6BEE, ...

- The azimut information was wrong in the check country window when no grid
  square were specified in the contest setting window.

1.2.0-rc1 (release candidate)
- Updated to inno setup 4.0-pre1 (Inno Setup is the installer)

- The installer will no more request for a reboot at the end of the
  installation except if needed.

- Added the wtCom.DLL which is an API designed to hack the Win-Test network.
  The API documentation, as well as some source code examples will be
  available later

- Added wtDxTelnet to the vault. wtDxTelnet is a freeware software designed
  to connect to a telnet DxCluster server. wtDxTelnet uses the wtCom API to
  communicate with Win-Test.

- Added a VHF database into the distribution package.

1.1.1
- Rate window crashed in WPX mode. Fixed. Tks F5CQ, F5IN.

- ALT-F1/F2 is now operationnal with the FT-1000MP as well. Tks F5CQ.

- Frequency was not decoded with all kenwood radios. Fixed. Tks F5IN.

- Station informations (name, address, etc) are stored in wt.ini. That way,
  some fields of the contest settings window will be filled with that
  informations the next time the user will create a new contest.

- Same for the equipment and antenna/station height informations needed
  for REG1TEST outputs.

- Fixed ADIF exports (some infomations, ie Gridsquares, was missing for
  the most recent supported contests). Tks F8ACF.

1.1.0 BETA released

1.0.7
- KG4abc problem (which is USA, not Guantanamo) fixed.

- Fixed off-time date bug for the SOAB entry of the REF contest.
  Tks F6AOI & F5CQ.

- /<digit> was not recognized when the callsign has got a digit in first place.
  Fixed.

- Added some controls in SO2R mode (to avoid ie to have the Radio2 active even
  if there is no Radio 2 !)

- Fixed the frequency bug in the spotting dialog box.

- Added submenu in the commands menu to allow selecting the station type :
  Run / Run1 / Run2
  It is also possible to set if this station is a support/inband one.

  NB : CTRL+F3 and ALT+Y can be use to toggle RUN1/RUN2 or RUN/MULT

- Multi/2 is now *really* supported in the ARRL DX contest.

- Fixed a problem with the serial numbers.

- Added support for the FT-1000MP / Mk5. Tks F6BEE.

- COM port settings modified. ComxOptions directive is no more needed in
  WT.INI.

- Added REF THF contest.

- Added CQWW VHF contest.

- Added a couple of generic contest suitable for most of the IARU region 1
  THF contest :
	- EU THF, suitable for the "National THF", "Concours du printemps", ...
	- EU THF, with gridsquare as multiplier, suitable for both the "CDD" and
	  the "contest d'été"

- UDP socket uses the SO_REUSEADDR mode. It means that the UDP potr can be
  shared by other applications on the computer. BTW, if you want to develop
  your own application, take care to use the SO_REUSEADDR as well !

- REG1TEST supported.

1.0.6
- Removed one extra space from the INS CW message, which was sent before
  the report in CW (INS key).

- F1 to F7 CW messages, as well as +, and INS can be sent in keyboard mode
  as weel.

- Validating a QSO with a ? as first character in the callsign field might
  crash Win-Test. Fixed.

1.0.5
- Still a computer keys problem with Windows 95 fixed. Many thanks to F5GYA
  for his patience. Tks also to F6BEE.

- Added feature : SHIFT+10 does search in the log every contact with made
  with the zone/departement/state specified in the logged callsign field.
  The information is shown in the check partial window.
  Tks F8CRH for suggestion.

- REF contest : F10 does not show any more the french station from a
  departement different of the logged one. Tks F6HJO.

- LPT pin 14 is used to send Radio1/2 information to an external interface.
  High = Radio1, Low = Radio2. Tks F6BEE

- ALT-/ is an alias to * to swap the radios. Tks F6BEE.

- The content of the logged callsign is memorised when swapping radios.
  Tks F6BEE.

- Background color is different for Radio 2. Tks F6BEE.

1.0.4
- Fixed some path problems :
	WT.INI, *.DTB, maps, ... : now same dir as application
	*.WTB, *.LOG, *.NOT : in the WTB directory
  Tks F6HJO and others.

- Added an extra configuration key in WT.INI to allow setting the DTR
  to be always ON. That key must be entered manually in the [Interfaces]
  section.

  COMxDTR=always_on    where x is the port COM number

- Generic Icom was crashing Win-Test. Fixed. Tks F6IFY.

- The GAB window will be closed after 15 seconds when it has been
  opened to show a new gab in. Tks F8CRH.

- Installer (Inno Setup) updated.

- Added an option in the EDIT menu de clear out all QSO from the LOG.

1.0.3
- The registration key module has been cleaned again. Tks to all for your
  patience.

- KL7 station can be both DX or US side. Fixed. Tks F6FVY.

- The "new country" / "new zone, departement, ..." warning information is now
  deleted when the QSO has been validated. Tks TK5EP.

- Macro commands SOUND/NOSOUND aren't annoying anymore that the callsign field
  is not correct. Tks TK5EP and F8CRH.

- When no radio is connected, the frequency showed in the cabrillo output is
  the frequency by default, as specified in the specs. Tks F6HJO.

- A .wtb file extension is added to the contest file name in the contest
  importation feature.

- Importing a CQWW 160 CW cabrillo file now works as it should. Tks F6FVY.

- Done some improvements in the radio initialization module.

- The month was wrong when importing a log from Editest. Fixed. Tks F1EBN.

- New feature : WT now computes the off-time for the single operator in the
  REF HF contest.

- Added support for IC735. NB : still in beta test. Tks F6IFR.

- Added support for Generic Icom-like radio. The radio address must be set
  manually in WT.INI, in the [Interfaces] section :

	IcomGenericRadio1=<n>h	when n is the radio 1 HEXA address
	IcomGenericRadio2=<n>h	when n is the radio 2 HEXA address

	In example : IcomGenericRadio2=48h	will used address 48 hexadecimal for
										the Radio 2

- By default, any serial port is opened with the following settings : 8 bits,
  no parity, 1 stop bit, no RTS/CTS
  This can now be overrided in the WT.INI file manually, in the [Interfaces]
  section. The following example shows how to configure the COM1 with
  default settings.

		COM1Options=8,n,1,norstcts
		   |        | | |    |
		   |        | | |    +--  RTS/CTS control   rtscts / norstcts
		   |        | | +-------  Stop bits         1 / 1.5 / 2
		   |        | +---------  Parity			n (no) / o (odd) / e (even)
		   |        +-----------  Byte size			8 / 7
		   +--------------------  COM Port num		1 / 2 / .... / 7 / 8

- Registration limitation changed. Users can now run Win-Test also after the
  2 weeks registration time limit. On the other hand, a popup windows will
  appair sometimes untill the software is registred.

1.0.2
- WT was unstable with the serial network activated. Fixed. Tks TK5EP

1.0.1
- Fixed a serial number problem - Tks TK5EP & F6CTT

- Fixed states in the ARRL US/VE database


1.0.0
- Added in the main menu the child/popup window Option which was previously only
  before loading a contest. Tks F6FVY.

- Again some cosmetic fixings. Tks F6FVY.

1.0.0-pre released

0.9.19
- Added CQWW 160 rule

0.9.18
- Demo version ready

- Added OVERLAY information in cabrillo (CLUB for the REF contest)

- Added RIG information according to the REF needs : the user will be prompted
  to enter his RIG information when he generates the cabrillo output for
  the REF contest.

0.9.17
- Fixed some cometic bugs

0.9.16
- Use ALT+F3 to send a spot to the Dx-Cluster

- Added R1, R2, R3 as new multipliers for maritime mobile stations in ARRL 10.
  Tks F6FVY.

- Problem sending data to a TNC-2 fixed.

- Caracters are OEM encoded before they are sent to the TNC. That way, extented
  characters are well interpreted, providing the TNC is set with 8BITCONV to ON.

0.9.15
- Added support for the ARRL 10-meter contest

- Build ARRL-ALL.DTA for the ARRL 10-meter contest

0.9.14
- Updated the cabrillo format for the REF contests according to the
  specifications

0.9.13
- Dx Spot are parsed and added into a database.

- Added a Dx cluster DX announcements window.

- Added the band map support (the bandmap is displayed in the radio window).

- Definitively fixed the GMT vs localtime problems.

- Added support for many Icom radios.

0.9.12
- Some canadian provinces (like AB, BC, ...) were not checked as multiplier. Tks
  to all.

- NE vs ME problem with US state fixed. Tks F6GOX/F6FVY/...

- Added aliases for state/provinces (ie NWT = NT, PC = QC, ...).

- Added menu "Command | kill qso" to remove a QSO from the LOG. Notice that this
  command is irreversible for now. For that reason, WT crates a backup copy of
  the log before removing the QSO from memory.

  REMARK : a killed QSO will not be shared through the network yet.

- When you logged a bad QSO but don't want to kill it for now, you can simply
  put your callsign in the logged callsign field. After the contest you will
  have to clean your log for such entries, using the "File | Clean up the log".

  Cleaning up feature also includes a way to remove all dupes from the LOG.

- Fixed cabrillo output for ARRL DX. Tks F5SDD.

- KH6/KL7 can operate from either W/VE or DX side.

- Default morse messages were not set opening a log which has been imported
  from cabrillo. Fixed. Tks F6GOX/F6FVY.

- Radio 2 supported. There is several ways to set the active one :
	-> Menu "Commands | Active Radio"
	-> Double clicking on the VFO LCD display in the "Radio" tool window
	-> Using the STAR key (*) to swap the radios

- Radio feature is enabled even if there is no controled radio connected.

- Entering a frequency in the callsign field will set the
  active VFO with.

- Fixed some problems with the TNC buffers. Tks F8BQQ.

- In the cluster command dialog, CTRL+E sends an ESC code to the TNC.
  Tks F8BQQ.

- Added a way to enable/disable the sound blaster in the interface
  configuration dialog. If disabled, WT sends a signal to command a digital
  voice keyer (like MFJ432/434) to the LPT port.

  Signal sent is as following :
	MSG1 (F1) : pin 3
	MSG2 (F1) : pin 4
	MSG3 (F1) : pin 5
	MSG4 (F1) : pin 6

0.9.11
- Again some problems with UTC. Fixed.

- Band Data for Radio1 is available on LPT1. The data is compatible with the
  Yaesu standard :

	pin2 pin7 pin8 pin9
	A    B    C    D
	H    L    L    L     160m
	...
	H    L    L    H      10m

- N+1 window displays "[UNIQUE]" when the logged callsign is unknown.

- Time/date shortcut key moved to ALT+F (was CTRL+F).

- Added "Split Frequency" in menu "Commands" (shortcut key "-") to
  set the split frequency for the active radio.

- Terminal Packet Controler (TNC) supported on COM port.
  -> To monitor the received packet frames :
		menu "Windows | Dx Cluster monitoring" or ALT+O
  -> To send commands to the TNC :
		menu "Commands | Dx Cluster" or ALT +T
  Remark : you must configure the TNC in the interface settings dialog
  with the computer the TNC is connected to but you have nothing to do
  with the other ones in the network.

- Added some network protocols to check if everything is OK in the
  network configuration.

0.9.10
- Menu "Options | set up interfaces" replace all serial and parallel port
  configuration

- Added support for KENWOOD transceivers. Only one radio is allowed at this
  step of the developpement.

- ARRL DX contest supported.

- Cancelling in the contest configuration window crashed WT if a different
  contest was already open. Fixed. Tks F8BQQ.

- Removed some bugged code from the map window. There is now less features
  but the code would be more stable.

- Added a Radio1 window which displays the RIG frequency of both VFO A and B.
  It is also possible to switch between VFOs clicking on the "LCD" display.
  That feature needs the font "Digital Readout Upright" to be installed.
  The same window for the Radio2 will be available later.


0.9.9
- Improved log and tool windows refreshing when moving in the log (up or down
  using the arrow keys).

- Fixed some problem with local time and UTC.

- CTRL+F or "Edit | Date and time" menu can be used to edit date and time of a
  QSO.

- Fixed the break time entry in cabrillo for the REF contest in SOAB category.

- The semi-colomn character (:) is now optionnal in the time field.

- QSO number is displayed in REF HF rather than the serial one.

- Added a merging logs feature (menu File | Merge Logs). That part of code
  is maybe (!) not free of bug. So please check your log carefully after
  a merge.

- Super check partial displays the dupe callsign in RED.

- Mult/mult fixed in Rate windows (it was wrong for the first hours in
  the contest).

- Tried to fix the font display problem in some tool windows. Tks F5IN.

- REF HF : WT now warms when you're going to log a new departement. Tks F8CRH.

- Added N+1 feature (SHIFT F12 or Window | N + 1). N+1 tool window shows
  the callsigns which are close to the logged one. N+1 does only search
  the database for now.

- CTRL+T or menu "Commands | Tune" switch the transceiver to TX and send
  a CW tune (either continous or a pulsed one).

0.9.8
- WT freezed when the sun neither rises or sets for a specified callsign.

- Done some improvements in worked-DXCC windows display.

- Notes (ALT+N) are forwarded to the network. That way, all station in the
  network will have the same copy of the notes file.

- Enlarged the "points" column in the summary window. Tks F6FVY.

- Moving to the QSO immediatly before the logged one was not updating the
  tool windows. Fixed. Tks F6FVY.

- Improved the variable parser in CW messages.

- Focus problem in "floating mode" fixed. Tks F6FVY.

0.9.7
- Fixed some cosmetic bugs. Tks F6FVY.

- Added Keyboard mode in CW.

- The Rate window now displays the current mode (CW vs SSB), and if the REPEAT
  mode is enabled. It also displays the CW speed.

- Added an option to disable sound in CW

- Some commands can be entered in the logged callsign field :
	QUIT
	SOUND / NOSOUND
	WRITELOG
	SAVELOG
	WRITEDB
	REPEAT / NOREPEAT

- It it now possible, before loading/starting a contest, to set if you want to
  allow the tool windows to be moved anywhere out of the main window or not.
  That setting can be done in the "windows" menu when no contest is loaded.
  Tks F6FVY.

0.9.6

- CW morse messages were not saved. Fixed. Tks to F8CRH, F6ETI, F5IN, ...

- CTRL + W wipes the current field.

- ALT + W is equivalent to F11. Tks F5IN.

- Exporting a CW contest to editest wasn't OK. Fixed. Tks F5HIJ.

- Added some icons in the toolbar.

- Fixed Claimed-Score entry in cabrillo file. Tks F6FNL.

- REF contest : Now displays a D in the log for a new departement.

- Added BREAK-TIME entry in cabrillo for the single-op category in the REF
  contest.

- CABRILLO can be imported.

0.9.5

- Fixed a problem displaying the supported contest. Tks F8BQQ

- DATE field in ADIF export was wrong. Fixed. Tks F8BQQ.

- ESC key went down the wrong way with some notebook keyboard drivers. Fixed.
  Tks F6ETI

- Known problem : SHIFT+(keypad)PLUS does not work with certain windows
  version. As far as I know this can not be fixed. Anyway it works using the
  other '+' key.

- Fixed DUPE problem in CW. Tks F5IN.

- Pressing any key will immediatly stop sending call message in Repeat Mode.
  Tks F6DZD.

- Added a warning message when the DXCC prefix is unknown.

- The whole CW messages can be edited at once using "Set CW messages" from
  the "Options" menu. Tks F8BQQ.

- Width of Rate window reduced. Tks F6GOX.

- Loading file time optimized.

- REF HF database up to date (refhf.wtb).

0.9.4

- Fixed some problems in morse messages. Tks F8CRH.

- Fixed a default cursor position in RST_sent field. Tks F6ETI.

- Added REF-SECTION in cabrillo.

- Fixed a conflict in report for TK stations. Tks F4CIB.

- QSYing a logged dupe QSO was messing up the zone multipliers database. Fixed.
  Tks F5FJL.

- Added ADIF support

- It is now possible to open automatically a contest when importing it.

- The number of rows displayed in the DXCC window is adapted to the window
  width. Tks F6ETI.

- Added REPEAT MODE feature (can be enabled/disabled in "Options" menu).
  Tks F6DZD.

0.9.3
- Fixed some bugs

- Added support of REF HF contest

- Added CABRILLO output format for all contests (see in menu File)

- Added network support (both via serial port and via ethernet) -
  (see in menu "Options")

- BETA 0.9.3 available

0.9.2
- Done some improvements in database loading - loading a 30.000 callsigns
  database spends now about 5 seconds on a K6-350 (was > 30 s before
  improvements).

- F4CIB noted that the voike keyer might crash pressing a couple a F-key
  (ie F1 & F2) at once. Fixed. Tks Franck.

- Locator field overflow fixed. Tks F6ETI & TM1Y.

- Fixed database update. Tks F6ETI.

- Database is now updated as QSO are logged.

- Fixed the "last hour rate" display problem (it was sometimes missing).

- REGION 1 IARU UHF contest supported.

- Both log and super check partial window are now paint using the microsoft
  Andale Mono font. That font must be installed before running WT 0.9.2.

- Graphic interface might display some garbage after a while. Fixed.

- WT checks the position of the tool windows at start-up taking care they will
  be visible. That way, if a tool window is not visible for any reason, its
  position will be ajusted as to get it visible again.

- Added best DX information in Rate Window.

- First tries with the CW support : it is not ready to use yet but you can give
  it a try anyway (ie playing CQ using F1).

- Added CW variables :

	variable		send
	$MYCALL			my callsign
	$LOGGEDCALL		the logged callsign
	$SERIAL			the serial number
	$CR				simulate a RETURN
	$CORRECT		send a call correction, if any
	$F1...$F6		send the message associated with F1 ... F6 function key

	+	up speed
	-   low speed

	In example, press SHIFT + F1 and enter : CQ $MYCALL $MYCALL ++TEST--
	then press F1 to play that message. You will heard your callsign instead of
	"$MYCALL"

- If mixed mode is selected in the configuration panel, CTRL+F1 will switch
  between SSB and CW.
